{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["원가계산서","총공사비집계표","내역서"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"원가계산서","index":0,"n_rows":37,"n_cols":18,"rows_kept":37,"cut":false,"hidden":false,"merged":[[0,0,0,17],[8,4,8,8],[8,13,8,14],[2,0,2,3],[2,4,2,12],[2,14,2,15],[3,13,3,14],[4,13,4,14],[5,4,5,8],[5,13,5,14],[6,13,6,14],[7,4,7,8],[7,13,7,14],[17,13,17,14],[9,13,9,14],[10,4,10,8],[10,13,10,14],[11,4,11,8],[11,13,11,14],[12,4,12,8],[12,13,12,14],[13,13,13,14],[14,13,14,14],[15,13,15,14],[16,4,16,8],[16,13,16,14],[17,4,17,8],[17,9,17,12],[25,4,25,8],[25,13,25,14],[18,13,18,14],[19,4,19,8],[19,13,19,14],[20,13,20,14],[21,4,21,8],[21,13,21,14],[22,4,22,8],[22,13,22,14],[23,4,23,8],[23,13,23,14],[24,4,24,8],[24,13,24,14],[36,13,36,14],[36,0,36,12],[33,1,33,12],[33,13,33,14],[34,9,34,12],[34,13,34,14],[32,13,32,14],[26,13,26,14],[27,13,27,14],[29,13,29,14],[35,9,35,12],[35,13,35,14],[30,13,30,14],[31,13,31,14],[28,13,28,14]]}
["공  사  원  가  계  산  서"]
[]
["공 사 명",null,null,null,"동탄(2)택지개발사업 부지조성공사(5-2공구)",{"$nulls":8},"관리번호"]
[null,"1. 순 공 사 원 가 ",{"$nulls":7},"[가+나+다]",{"$nulls":5},"직공비[합계액]\n대비","과세(100%)","비과세(0%)"]
[null,null,"가. 재료비"]
[null,null,null,"가-1.","직접재료비"]
[null,null,"나. 노무비"]
[null,null,null,"나-1.","직접노무비"]
[null,null,null,"나-2.","간접노무비 ",{"$nulls":4},"[나1] 의",8.6999999999999993,"%"]
[null,null,"다. 경   비"]
[null,null,null,"다-1. ","산 출 경 비"]
[null,null,null,"다-2.","산재보험료 ",{"$nulls":4},"[나] 의",3.8,"%"]
[null,null,null,"다-3. ","고용보험료 ",{"$nulls":4},"[나] 의",1.17,"%"]
[null,null,null,"다-4.","건강보험료",{"$nulls":4},"[나1]의",1.7,"%",null,358317917,null,null,358317917]
[null,null,null,"다-5.","노인장기요양보험",{"$nulls":4},"[다4]의",6.5500000000000007,"%",null,23469823,null,null,23469823]
[null,null,null,"다-6.","연금보험료",{"$nulls":4},"[나1]의",2.4900000000000002,"%",null,524830361,null,null,524830361]
[null,null,null,"다-7. ","퇴직공제부금",{"$nulls":4},"[나1] 의",2.2999999999999998,"%"]
[null,null,null,"다-8. ","산업안전보건관리비 ",{"$nulls":4},"※관급포함시: ⓑ와 ⓒ 비교후 적은금액 적용"]
[null,null,null,"ⓐ.","일반경우",{"$nulls":4},"[가+나1]  의",1.27,"%  +",0]
[null,null,null,"ⓑ.","ⓐ의 1.2배"]
[null,null,null,"ⓒ.","[가+나1+관급자재대] 의",{"$nulls":5},1.27,"%  +",0]
[null,null,null,"다-9.","환경보전비",{"$nulls":4},"[가+나1+다1] 의",0,"%"]
[null,null,null,"다-10. ","공사이행보증수수료",{"$nulls":4},"[가+나1+다1] 의",1.4E-2,"%","[13.5백만원+(직접공사비\n-500억원)×0.0140%]×공기년수"]
[null,null,null,"다-11.","건설하도급대금지급\n보증서발급수수료",{"$nulls":4},"[가+나1+다1] 의",7.0999999999999994E-2,"%"]
[null,null,null,"다-12.","기타경비 ",{"$nulls":4},"[가+나] 의",6.5,"%"]
[null,null,null,"다-13.","건설기계대여대금 \n지급보증서 발급금액",{"$nulls":4},"[가+나1+다1] 의",0.41,"%"]
[null,"2. 일 반 관 리 비  ",{"$nulls":7},"[1] 의",4.9000000000000004,"%"]
[null,"3. 이             윤",{"$nulls":7},"[1나+1다+2] 의",10,"%"]
[null,"4. 시공상세도작성비"]
[null,"5. 총     원     가 ",{"$nulls":7},"[1+2+3+4]"]
[null,"6. 소             계",{"$nulls":7},"[5]"]
[null,"7. 부 가 가 치 세 ",{"$nulls":7},"[6] 의",10,"%"]
[null,"8. 총             계",{"$nulls":7},"[6+7]"]
[null,"도급액"]
[null,"9.관 급 자 재 대",{"$nulls":11},7252630000,null,null,7252630000]
[null,"10. 부가가치세(관급자재)",{"$nulls":11},725263000,null,null,725263000]
["총       공       사       비"]

{"sheet":"총공사비집계표","index":1,"n_rows":4143,"n_cols":9,"rows_kept":4143,"cut":false,"hidden":false,"merged":[[0,0,0,8],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8]]}
["총 공 사 비  집 계 표"]
["공사명 : 동탄(2) 택지개발사업 부지조성공사(5-2공구)"]
["공    종","규  격","수 량","단위","합  계","재 료 비","노 무 비","경 비","비  고"]
[]
[" Ⅰ. 공 통 공 종","",1,"식",{"$nulls":4},""]
["  1. 공 통 공 사","",1,"식",{"$nulls":4},""]
[" Ⅱ. 토 목 공 사","",1,"식",{"$nulls":4},""]
["  1. 토 공 사","",1,"식",{"$nulls":4},""]
["  2. 도로 및 포장공사",null,1,"식",{"$nulls":4},""]
["  3. 우 수 공 사","",1,"식",{"$nulls":4},""]
["  4. 오 수 공 사","",1,"식",{"$nulls":4},""]
["  5. 상 수 공 사","",1,"식",{"$nulls":4},""]
[" Ⅲ. 특수구조물",null,1,"식"]
["  1. 송방천6교","합성형 라멘교",1,"식"]
[" Ⅳ. 가로수 조경공사",null,1,"식"]
["  1. 가로수 식재공사",null,1,"식"]
["  2. 가로수 유지관리공사",null,1,"식"]
["     순  공  사  비","",1,"식",{"$nulls":4},""]
["   A. 간접노무비","직접노무비 * 8.7%",1,"식",{"$nulls":4},""]
["   B. 산재보험료","노무비 * 3.8%",1,"식",{"$nulls":4},""]
["   C. 고용보험료","노무비 * 1.17%    ",1,"식"]
["   D. 건강보험료","직접노무비 * 1.7%",1,"식",{"$f":"원가계산서!Q14","v":358317917}]
["   E. 노인장기요양보험료","건강보험료 * 6.55%",1,"식",{"$f":"원가계산서!Q15","v":23469823}]
["   F. 연금보험료","직접노무비 * 2.49%",1,"식",{"$f":"원가계산서!Q16","v":524830361}]
["   G. 퇴직공제부금비","직접노무비 * 2.3%",1,"식"]
["   H. 산업안전보건관리비","(재료비+직.노+관급자재) * 1.27%",1,"식"]
["   I. 공사이행보증수수료","[13.5백만원+(직접공사비-500억원)*0.00140%) * (44/12)년",1,"식"]
["   J. 건설하도급대금\n      지급보증서 발급수수료","[(재료비+직.노+산출경비) * 0.071%",1,"식"]
["   K. 기타경비","(재료비+노무비) * 6.5%",1,"식"]
["   L. 건설기계대여대금지급보증서 발급금액","(재료비+직접노무비+산출경비) * 0.41%",1,"식"]
["순 공 사 원 가",null,1,"식"]
["   M. 일반관리비","(재료비+노무비+경비) * 4.9%",1,"식"]
["   N. 이윤","(노무비+경비+일반관리비) * 10.0%",1,"식"]
["   O. 시공상세도 작성비",null,1,"식"]
["공급가액"]
["   P. 부가가치세","(공급가액) * 10%",1,"식"]
[" 도급공사비"]
[" Ⅴ. 관급자재",null,1,"식",{"$f":"원가계산서!Q35","v":7252630000}]
["  관급자재 부가가치세","(관급자재) * 10%",1,"식",{"$f":"E38*0.1","v":725263000}]
["총공사비",null,1,"식"]
{"$rows_empty":4102}
[" 31. 관급자재비 단수조정"]

{"sheet":"내역서","index":2,"n_rows":2159,"n_cols":13,"rows_kept":2159,"cut":false,"hidden":false,"merged":[[0,0,0,12],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,6,2,7],[2,8,2,9],[2,10,2,11],[2,4,2,5],[2,12,3,12]]}
["예  산  내  역  서"]
[]
["공    종","규  격","수 량","단위","합    계",null,"재 료 비",null,"노 무 비",null,"경    비",null,"비  고"]
[{"$nulls":4},"단  가","금  액","단  가","금  액","단  가","금  액","단  가","금  액"]
["*. 순 공 사 비","",0,""]
[" Ⅰ. 공 통 공 종","",0,""]
["  1. 공 통 공 사","",0,""]
["   가. 가설공사","",0,""]
["    1) 임시시설","",0,""]
["     가) 공사용 가설도로","",0,""]
["      공사용가설도로(골재포장)_유지관리","T=20cm",7305,"㎥"]
["    2) 특정임시시설","",0,""]
["     가) 배수시설-가배수로","",0,""]
["      터파기/육상토사","0-2m 기계",7738,"㎥"]
["      되메우기(기계100%)","비다짐",7738,"㎥"]
["      PVC천막지깔기","",8134,"㎡"]
["      비닐깔기","",3576,"㎡"]
["      P．P마대쌓기 및 헐기","",2802,"개"]
["     나) 배수시설-공동주택내미성토부지가배수로","",0,""]
["      터파기/육상토사","0-2m 기계",5132,"㎥"]
["      되메우기(기계100%)","비다짐",5132,"㎥"]
["    3) 임시 공용주차장","",0,""]
["     가) 보조기층포설및다짐","T=20cm",1730,"㎥"]
["   나. 공통가설","",0,""]
["    1) 발주자용가설건물","",0,""]
["     가) 감독사무실(발주자)","36개월",250,"㎡"]
["    2) 도급자용가설건물","",0,""]
["     가) 감독사무실(도급자)","36개월",430,"㎡"]
["     나) 창고","36개월",120,"㎡"]
["     다) 시험실","36개월",100,"㎡"]
["    3) 편의부대시설","",0,""]
["     가) 숙소(당직실)","숙소용,36개월",22,"㎡"]
["     나) 업무용차량","",0,""]
["      업무용차량,품질시험차량비","트럭",36,"개월"]
["     다) 가설화장실","",0,""]
["      이동식가설건축물","36개월,18M2",1,"식"]
["      바닥자기질타일붙이기","화장실200X200,바탕10+압착5",17.4636,"㎡"]
["      화장실칸막이","시공도",17.117999999999999,"㎡"]
["      가설화장실 기계설비","공용(오수정화조 포함)",1,"식"]
["      콘테이너화장실 전기공사","18M2(30개월)",1,"식"]
["      비 계 공","",0.57999999999999996,"인"]
["      특별인부","",0.34,"인"]
["      크레인(타이어)","10 ton",1,"시간"]
["     라) 안내시설","",0,""]
["      사업소입간판","아연도강판 T = 1.2mm",1,"개"]
["      단지조성공사사업소 유도간판","아연도강판 T = 1.2mm",1,"개"]
["      현장사업소 부착간판","아연도강판 T = 1.2mm",1,"개"]
["      표지판","아연도강판 T = 1.2mm",1,"개"]
["      편의·부대시설,안내판·현황판","아연도강판 T = 1.2mm",1,"개"]
["      상황판","목간판 5.4m*1.8m",1,"개"]
["     마) 현장사무소 포장 부대공사","",0,""]
["      보조기층포설및다짐","T=30cm",480,"㎥"]
["      아스콘포장/프라임코팅","RSC-3",1600,"㎡"]
["      아스콘포장/표층/포설및다짐","T = 5cm",1600,"㎡"]
["     바) 가설사무실비품_사무용가구","",0,""]
["      책상","",7,"개"]
["      협탁","",7,"개"]
["      TV탁자","",1,"개"]
["      조립식창고선반","",7,"개"]
["      주방가구","",1,"대"]
["     사) 가설사무실비품_사무용캐비넷","",0,""]
["      캐비넷","",1,"개"]
["      화일캐비넷","",10,"개"]
["      옷장(사물함)","",7,"개"]
["      신발장","",1,"대"]
["     아) 가설사무실비품_회의용탁자및의자","",0,""]
["      탁자","",2,"조"]
["      의자","",7,"개"]
["      접이의자","",4,"개"]
["     자) 가설사무실비품_응접셋트","",0,""]
["      응접탁자","",2,"조"]
["      응접소파","",2,"조"]
["      전화탁자","",2,"조"]
["     차) 가설사무실비품_전기냉장고","",0,""]
["      전기냉장고","",1,"대"]
["     카) 가설사무실비품_냉난방기","",0,""]
["      냉방기(에어콘-스텐드형)","",2,"대"]
["      냉방기(에어콘-벽걸이형)","",2,"대"]
["      난방기(튜브히터)","",1,"대"]
["      난방기(석유난로)","",1,"대"]
["     타) 가설사무실비품_컴퓨터및프로젝터","",0,""]
["      컴퓨터","",1,"대"]
["      프린터(레이저)","",1,"대"]
["      칼라프린터","",1,"대"]
["      스캐너","",1,"대"]
["      빔프로젝터","",1,"대"]
["      전동식스크린","",1,"대"]
["      이동식스크린","",1,"대"]
["     파) 가설사무실비품_TV및가전제품","",0,""]
["      TV","",1,"대"]
["      전자렌지","",1,"대"]
["      전기포트","",1,"대"]
["      진공청소기","",1,"대"]
["      디지털사진기","",2,"개"]
["      비데","",1,"개"]
["     하) 가설사무실비품_복합기(FAX)및전화기","",0,""]
["      복합기","",1,"대"]
["      전화기","",7,"대"]
["     거) 가설사무실비품_비품기타","",0,""]
["      소화기","",2,"개"]
["      벽시계","",2,"개"]
["      화이트보드","",2,"개"]
["      거울","",2,"개"]
["     너) 가설사무소기초","",0,""]
["      무근콘크리트타설","빈배합(leanmix)",92,"㎥"]
["    4) 공사용설비","",0,""]
["     가) 공사용건축마감","",0,""]
["      가설건물,건축마감공사","",22,"㎡"]
["     나) 공사용난방위생설비공사","",0,""]
["      가설건물,난방·위생설비공사","",702,"㎡"]
["     다) 공사용전기설비","",0,""]
["      가설건물,내부전기·통신공사","",702,"㎡"]
["     라) 공사용정화조공사","",0,""]
["      가설건물,정화조설치공사","1인용",50,"인조"]
["     마) 상황실 인테리어","",1,"식"]
["    5) 쇄석 및 잡석생산","",0,""]
["     가) 골재선별및생산 (발파암)","보통암,보조기층,Ø80mm이하",2612,"㎥"]
["   다. 공통장비","",0,""]
["    1) 플랜트","",0,""]
["     가) 크랏샤 설치 및 해체","정치식, 100ton이상",1,"sum"]
["     나) 크랏샤장기초","",0,""]
["      무근콘크리트타설","빈배합(leanmix)",40,"㎥"]
["   라. 현장관리비","",0,""]
["    1) 환경보전비","",0,""]
["     가) 수질오염방지","",0,""]
["      흙깍기공/토사","대규모",21380,"m3"]
["      되메우기(기계100%)","비다짐",21380,"m3"]
["      PVC천막지깔기","",3550,"M2"]
["      톤마대쌓기 및 헐기","",2683,"M2"]
["      원심력철근콘크리트관 접합 및 부설","칼라식, D1000MM,P.E수밀벨트접합",59,"M"]
["     나) 수질오염방지- 임시침사지준설","",0,""]
["      임시 침사지 준설","기계(B/H , DT)",21685,"㎥"]
["     다) 수질오염방지- 공동주택내미성토부지침사지","",0,""]
["      흙깍기공/토사","대규모",190,"m3"]
["      되메우기(기계100%)","비다짐",190,"m3"]
["      PVC천막지깔기","",336,"M2"]
["      톤마대쌓기 및 헐기","",187,"M2"]
["      원심력철근콘크리트관 접합및부설","칼라식,D600MM,P.E수밀벨트접합",178,"M"]
["     라) 대기오염방지-자동식세륜기(수조기)","",0,""]
["      자동식세륜기(수조기) 설치, 해체","",2,"개소"]
["      터파기/육상토사","0~2m,기계",376,"m3"]
["      되메우기(기계100%)","비다짐",376,"M3"]
["      철근콘크리트타설","다짐포함",52,"M3"]
["      무근콘크리트타설","",49,"M3"]
["      무근콘크리트타설","빈배합",8,"M3"]
["      거푸집공/보통마감","0~7M",182,"M2"]
["      거푸집공/거친마감","0~7M",26,"M2"]
["      잡석부설","기계",110,"M3"]
["      철근가공조립","보통",1.6930000000000001,"TON"]
["     마) 대기오염방지-세륜세차유지관리비","",0,""]
["      세륜세차시설 유지관리비","",2,"개소"]
["     바) 대기오염방지-공사현장살수","",0,""]
["      공사현장살수","물탱크16000ℓ",1,"sum"]
["     사) 소음진동방지","",0,""]
["      가설판넬설치및해체","H=3.0m x W=2.0 , DEP(36개월)",146,"경간"]
["      가설판넬설치및해체","H=3.0m+1.5m(분진)xW=1.5,DEP(36개월)",200,"경간"]
["     아) 폐기물처리비","",0,""]
["      터파기/육상토사","0~1M,30%",2,"M3"]
["      되메우기/토사","인력30%",1.75,"M3"]
["      잔토처리","토사",0.25,"M3"]
["      문주파이프(주주)","Φ60.5ⅹ2.3T(융융)",11.6,"m"]
["      문틀파이프(주주)","Φ48ⅹ2.3T(융융)",7,"m"]
["      후레임","45ⅹ35ⅹ1.5T",19.2,"m"]
["      주주캡","Φ76.3",4,"nr"]
["      연결판","후레임용",2,"nr"]
["      고정판","50*80*2.0T(융융)",8,"nr"]
["      망고정크립","25*20*1.2T",108,"nr"]
["      P．V．C망(능형망)","#12*40*40",19.934000000000001,"㎡"]
["      횡  선","#8",42.16,"m"]
["      직선볼트너트","ø8*70",8,"nr"]
["      L볼트너트","ø6*50(융융)",8,"nr"]
["      연결판볼트너트","ø6*12",8,"nr"]
["      망고정볼트너트","ø6*40",108,"nr"]
["      각재(미송)","3.0cmx3.0cmx3.6m",7.0000000000000001E-3,"㎥"]
["      불연단연강판","0.6*960mm",9.6,"㎡"]
["      무근콘크리트타설","빈배합",0.83,"M3"]
["      거푸집공/거친마감","0~7M",3.77,"M2"]
["    2) 품질관리비","",0,""]
["     가) 품질관리비,품질시험비","",1,"sum"]
["    3) 준공표지판설치","",0,""]
["     가) 준공표지판설치","화강석",1,"개소"]
["     나) 터파기/육상토사","0-1m 인력30%",1.53,"M3"]
["     다) 되메우기/토사(인력30%)","",0.81,"㎥"]
["     라) 잔토처리","토사",0.72,"M3"]
["     마) 거푸집공/거친마감","0-7m",1.92,"㎡"]
["   마. 기타","",0,""]
["    1) 필지경계점 말박기","",0,""]
["     가) 필지경계점말박기(내부)","",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","",0.88,"㎥"]
["      경계말뚝(지적경계점표지)","3.0X3.0X35",146,"개"]
["      항타보호캡","",146,"개"]
["      토사 터파기","인력,굴착깊이0-1M,보통토사",3.5,"㎥"]
["      되메우기 및 다짐","인력",2.63,"㎥"]
["      잔토처리","인력,소운반고르기",0.88,"㎥"]
["     나) 필지경계점말박기(외부)","",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","",0.68,"㎥"]
["      철못(지적경계점표주)","7cm,2호",339,"개"]
["      유성페인트칠(적색)","조합페인트2회,0.0015㎡/개소",0.50900000000000001,"㎡"]
["      토사 터파기","인력,굴착깊이0-1M,보통토사",4.07,"㎥"]
["      되메우기 및 다짐","인력",3.39,"㎥"]
["      잔토처리","인력,소운반고르기",0.68,"㎥"]
["   바. 주요자재 구입","",0,""]
["    1) 시멘트","",0,""]
["     가) 시멘트","40kg/포",19,"포"]
["    2) 모래","",0,""]
["     가) 모래","",1,"㎥"]
["    3) 골재","",0,""]
["     가) 자갈","Ø40mm",2,"㎥"]
["     나) 잡석골재","Ø150mm이하",114,"㎥"]
["    4) 흄관","",0,""]
["     가) 흄관(칼라 미포함)","D600mm,2종",184,"M"]
["     나) 흄관(칼라 미포함)","D1000mm,2종",61,"M"]
["    5) 아스팔트유제","",0,""]
["     가) 공통공사","",0,""]
["      아스팔트유제(KSM2203)","RS(C)-1,2,3,4",12,"D/M"]
["   사. 주요자재 운반","",0,""]
["    1) 철근운반","",0,""]
["     가) 철근운반","L=10.00km(하치장-현장)",1.744,"Ton"]
["    2) 시멘트운반","",0,""]
["     가) 시멘트운반","40kg/포,L=10km(하치장-현장)",19,"포"]
["    3) 보조기층재운반","",0,""]
["     가) 보조기층재 운반","80m/m이하, L=498m",2612,"㎥"]
[" ","",0,""]
[" ","",0,""]
[" Ⅱ. 토목공사","",0,""]
["  1. 토공사","",0,""]
["   가. 벌목 및 벌개제근공","",0,""]
["    1) 벌개제근","",0,""]
["     가) 벌개제근공","",679814,"m2"]
["    2) 뿌리부소운반","",0,""]
["     가) 임목폐기물운반","현장->적치장(L=0.630KM)",6636,"Ton"]
["   나. 지장물철거","",0,""]
["    1) 콘크리트깨기","",0,""]
["     가) 철근구조물","",0,""]
["      철근콘크리트깨기","T=30cm이상",876,"m3"]
["      철근콘크리트깨기","T=30cm미만",272,"m3"]
["     나) 무근구조물","",0,""]
["      무근콘크리트깨기","T=30cm 이상(기계 100%)",25,"m3"]
["      무근콘크리트깨기","T=30cm 미만(기계 100%)",335,"㎥"]
["    2) 포장깨기","",0,""]
["     가) 콘크리트포장깨기","T=30cm 미만",93,"㎥"]
["     나) 아스팔트포장깨기","T=30cm 미만",326,"m3"]
["    3) 구조물헐기","",0,""]
["     가) 호안블록헐기","",220,"m2"]
["     나) 자연석헐기","메쌓기",1077,"㎡"]
["    4) 상수관(고철)","중량A",1.873,"Ton"]
["   다. 비탈면보호공","",0,""]
["    1) 잔디","",0,""]
["     가) 성토부(토사)","",0,""]
["      비탈면보호공","줄떼",13641,"㎡"]
["    2) 녹화공법","",0,""]
["     가) 친환경생태복원공법","토사,무망,T=2cm",19914,"㎡"]
["     나) 친환경생태복원공법","리핑암,천연섬유망,T=5cm",3184,"㎡"]
["     다) 친환경생태복원공법","발파암,PVC코팅철망,T=7cm",3347,"㎡"]
["   라. 흙깎기","",0,""]
["    1) 토사","",0,""]
["     가) 흙깍기공/토사","대규모",254301,"㎥"]
["     나) 흙깎기공/토사","기계(B/H 2.0㎥)",1371853,"㎥"]
["    2) 리핑암","",0,""]
["     가) 흙깍기공/리핑암","",2179413,"㎥"]
["    3) 발파암","",0,""]
["     가) 일반발파","",0,""]
["      일반발파","(3구역)",50942,"㎥"]
["     나) 대규모발파","",0,""]
["      대규모발파","(1구역)",497077,"㎥"]
["      대규모발파","(2구역)",2123912,"㎥"]
["      대규모발파","(3구역)",1038481,"㎥"]
["    4) 발파암 소할","",0,""]
["     가) 발파암소할","",2974842,"㎥"]
["    5) 시험발파비","",1,"회"]
["    6) 발파상시계측","(2개소)",2,"개월"]
["   마. 비옥토절취","",0,""]
["    1) 비옥토절취","기계, B/D 32Ton",13461,"㎥"]
["   바. 흙쌓기","",0,""]
["    1) 다짐도95%","",0,""]
["     가) 흙쌓기/토사","노상, 다짐도95%이상",100408,"m3"]
["    2) 다짐도90%","",0,""]
["     가) 흙쌓기/토사","노체, 다짐도 90%이상",837984,"m3"]
["    3) 비다짐","",0,""]
["     가) 흙쌓기/토사","비다짐, B/D32ton",37303,"m3"]
["     나) 흙쌓기/리핑암","비다짐, B/D32ton",514308,"㎥"]
["     다) 흙쌓기/발파암","비다짐, B/D32ton",702786,"㎥"]
["   사. 흙운반","",0,""]
["    1) 유용무대","",0,""]
["     가) 토사(도로)","B/D 32ton",5073,"㎥"]
["     나) 토사(블럭)","B/D 32ton",65959,"㎥"]
["     다) 리핑암(도로)","B/D 32ton",578,"㎥"]
["     라) 리핑암(블럭)","B/D 32ton",10685,"㎥"]
["    2) 직접운반","",0,""]
["     가) 도자운반","",0,""]
["      토사(도로)","L=23m, B/D 32ton",16583,"㎥"]
["      토사(블럭)","L=23m, B/D 32ton",166687,"㎥"]
["      리핑암(도로)","L=26m, B/D 32ton",18056,"㎥"]
["      리핑암(블럭)","L=26m, B/D 32ton",79271,"㎥"]
["     나) 순성토운반","",0,""]
["      순성토운반(토사)","805m,백호우2.0,덤프15톤",745306,"m3"]
["      흙운반(적재ㆍ적하)/토사(직상차)","덤프15톤",745306,"m3"]
["      순성토운반(리핑암)","884m,로더3.5,덤프15톤",1714360,"m3"]
["      흙운반(적재,적하)/리핑암","로더+덤프15톤",1714360,"m3"]
["      순성토운반(발파암)","841m,리더3.5,덤프24톤",2342621,"m3"]
["      흙운반(적재ㆍ적하)/발파암","로더3.5㎥+D/T24ton",2342621,"㎥"]
["    3) 기타운반","",0,""]
["     가) 비옥토운반","",0,""]
["      비옥토운반(토사)","319m,백호우2.0,덤프15톤",13461,"m3"]
["      흙운반(적재ㆍ적하)/토사(직상차)","덤프15톤",13461,"m3"]
["     나) 크라샤장운반","",0,""]
["      크라샤장운반(절취 크라샤장)","보통암,85m,로더3.5,덤프24톤",23195,"m3"]
["      크라샤장운반(적재ㆍ적하)/보통암","로더3.5㎥+D/T24ton",23195,"㎥"]
["     다) 치환성토(토사)"," ",0," "]
["      순성토운반(토사)","805m,백호우2.0,덤프15톤",319966,"m3"]
["      흙운반(적재ㆍ적하)/토사(직상차)","덤프15톤",319966,"m3"]
["     라) 모암매각(보통암)","",0,""]
["      보통암"," ",461538,"㎥"]
["    4) 외부반출토운반","",0,""]
["     가) 외부반출토","5-1공구 반출",0,""]
["      외부반출토운반(토사)","2211m,백호우2.0,덤프15톤",206581,"m3"]
["      흙운반(적재ㆍ적하)/토사(직상차)","덤프15톤",206581,"m3"]
["      외부반출토운반(리핑암)","2311m,로더3.5,덤프15톤",266131,"m3"]
["      흙운반(적재ㆍ적하)/리핑암/집토후상차","로더+덤프15톤",266131,"m3"]
["      외부반출토운반(발파암)","2293m,로더3.5,덤프24톤",632220,"m3"]
["      반출토운반(적재,적하)/발파암","로더3.5㎥+D/T24ton",632220,"㎥"]
["      흙쌓기/토사","비다짐, B/D32ton",61974,"m3"]
["      흙쌓기/리핑암","비다짐, B/D32ton",79839,"㎥"]
["      흙쌓기/발파암(사토장)","비다짐, B/D32ton",189666,"㎥"]
["     나) 외부반출토","진위2지구 반출",0,""]
["      반출토운반(적재)/토사","기계(B/H 2.0㎥)",100000,"㎥"]
["      반출토운반(적재)/리핑암","로더3.5㎥",90909,"㎥"]
["      반출토운반(적재)/발파암","로더3.5㎥",250836,"㎥"]
["   아. 부대공","",0,""]
["    1) 비옥토보관","",0,""]
["     가) PE천막지설치","",5830,"㎡"]
["     나) 터파기/육상토사","0-2m 기계",198,"M3"]
["     다) 되메우기,토사","기타구조물,B/D 19Ton",198,"㎥"]
["    2) 규준틀","",0,""]
["     가) 토공규준틀","수평규준틀",166,"nr(개소)"]
["    3) 절토면고르기","",0,""]
["     가) 비탈면고르기","토사",19914,"m2"]
["     나) 비탈면고르기","리핑암",3184,"㎡"]
["     다) 비탈면고르기","발파암",3347,"㎡"]
["    4) 성토면고르기","",0,""]
["     가) 성토면고르기","인력",13641,"㎡"]
["  ","",0,""]
["  2. 도로 및 포장공사","",0,""]
["   가. 토공","",0,""]
["    1) 터파기","",0,""]
["     가) 토사","",0,""]
["      토사 터파기","인력,굴착깊이0-1M,보통토사",667,"㎥"]
["      터파기/육상토사","0-2m 기계",5032,"㎥"]
["     나) 발파암(연암)","",0,""]
["      터파기/육상발파암(연암)","0-2m 기계",331,"m3"]
["    2) 되메우기","",0,""]
["     가) 되메우기/토사(인력30%)","다짐",614,"m3"]
["     나) 되메우기/기계(100%)","",115,"㎥"]
["     다) 되메우기/기계","비다짐",4974,"㎥"]
["     라) 잔토처리","",0,""]
["      잔토처리","토사",435,"㎥"]
["      잔토처리","발파암(연암)",331,"㎥"]
["   나. 동상방지층,보조기층,기층","",0,""]
["    1) 동상방지층","",0,""]
["     가) 동상방지층재 운반","L=367m",9532,"㎥"]
["     나) 동상방지층,포설및다짐","100m/m이하,42cm",8102,"㎥"]
["    2) 보조기층","",0,""]
["     가) 보조기층재 운반","80m/m이하,L=498m",10603,"㎥"]
["     나) 보조기층,포설및다짐","80m/m이하,15cm",9331,"㎥"]
["   다. 아스콘포장","",0,""]
["    1) 프라임코팅","",0,""]
["     가) 프라임코팅","RSC-3:150ℓ/a",64572,"㎡"]
["    2) 택코팅","",0,""]
["     가) 택코팅","RSC-4:45ℓ/a",91791,"㎡"]
["    3) 가열아스팔트안정처리기층","",0,""]
["     가) 기층,포설및다짐","#467, 8cm",64637,"㎡"]
["    4) 아스콘 중간층","",0,""]
["     가) 중간층,포설및다짐","T = 6cm",27090,"M2"]
["    5) 아스콘 표층","",0,""]
["     가) 표층,포설및다짐","T = 5cm",58829,"M2"]
["     나) 표층, 포설및다짐(암적색)","T = 5cm",3680,"M2"]
["     다) 저소음포장,표층,포설및다짐","T=5cm",2193,"㎡"]
["    6) 사고석포장","",0,""]
["     가) 사고석포장","T=11+3CM",63,"㎡"]
["   라. 경하중포장","",0,""]
["    1) 보도블럭포장","",0,""]
["     가) 경하중포장,소형고압블록(대규모)","T=6+3+10CM",4530,"㎡"]
["     나) 투수블록포장","T=6+3+10CM",14996,"㎡"]
["     다) 투수콘크리트 포장","T=5CM",8344,"㎡"]
["     라) 도막형바닥재","T=2CM",8344,"㎡"]
["    2) 장애자용블럭","",0,""]
["     가) 장애인용블럭포장-유도블럭","T=6cm,황색",71,"㎡"]
["     나) 장애인용블럭포장-점자블럭","T=6cm,황색",120,"㎡"]
["    3) 자전거도로포장(코팅+투수콘크리트포장)","",0,""]
["     가) 투수콘크리트 포장","T=5CM",5400,"㎡"]
["     나) 도막형바닥재","T=2CM",5400,"㎡"]
["    4) 보조기층재 운반","",0,""]
["     가) 보조기층재 운반","40m/m이하,L=498m",3740,"㎥"]
["   마. 경계블럭설치","",0,""]
["    1) 보차도경계석","",0,""]
["     가) 보차도경계석및측구(중1류이상)","",0,""]
["      보차도경계석및측구(중1류이상)","화강석,200×250×1000(직선)",3672,"M"]
["      무근콘크리트타설","빈배합(leanmix)",459,"㎥"]
["      모르터(1:3)(토목,조경)","",1.8360000000000001,"㎥"]
["     나) 보차도경계석및측구(중1류이상)","",0,""]
["      보차도경계석및측구(중1류이상)","화강석,200×250×1000(곡선)",418,"M"]
["      무근콘크리트타설","빈배합(leanmix)",52,"㎥"]
["      모르터(1:3)(토목,조경)","",0.20899999999999999,"㎥"]
["     다) 보차도경계석및측구(중2류이하)","",0,""]
["      보차도경계석및측구(중2류이하)","화강석,180×200×1000(직선)",952,"M"]
["      무근콘크리트타설","빈배합(leanmix)",117,"㎥"]
["      모르터(1:3)(토목,조경)","",0.33700000000000002,"㎥"]
["     라) 보차도경계석및측구(중2류이하)","",0,""]
["      보차도경계석및측구(중2류이하)","화강석,180×200×1000(곡선)",421,"M"]
["      무근콘크리트타설","빈배합(leanmix)",52,"㎥"]
["      모르터(1:3)(토목,조경)","",0.151,"㎥"]
["     마) 보차도경계석및측구(소로)","",0,""]
["      보차도경계석및측구(소로)","콘크리트,150×170×200×1000",8677,"M"]
["      무근콘크리트타설","빈배합(leanmix)",1050,"㎥"]
["      모르터(1:3)(토목,조경)","",2.7770000000000001,"㎥"]
["    2) 단차경계석","",0,""]
["     가) 보차도경계석및측구-경사","",0,""]
["      보차도경계석및측구-경사","화강석,200×250~100×1000",320,"M"]
["      무근콘크리트타설","빈배합(leanmix)",27,"㎥"]
["      모르터(1:3)(토목,조경)","",0.112,"㎥"]
["     나) 보차도경계석및측구-낮춤","",0,""]
["      보차도경계석및측구-낮춤","화강석,200×100×1000",360,"M"]
["      무근콘크리트타설","빈배합(leanmix)",43,"㎥"]
["      모르터(1:3)(토목,조경)","",7.1999999999999995E-2,"㎥"]
["     다) 보차도경계석및측구-경사","",0,""]
["      보차도경계석및측구-경사","화강석,180×200~100×1000",216,"M"]
["      무근콘크리트타설","빈배합(leanmix)",18,"㎥"]
["      모르터(1:3)(토목,조경)","",5.8000000000000003E-2,"㎥"]
["     라) 보차도경계석및측구-낮춤","",0,""]
["      보차도경계석및측구-낮춤","화강석,180×100×1000",243,"M"]
["      무근콘크리트타설","빈배합(leanmix)",28,"㎥"]
["      모르터(1:3)(토목,조경)","",4.3999999999999997E-2,"㎥"]
["    3) 도로경계블럭 및 분리 경계석","",0,""]
["     가) 도로경계블럭","",0,""]
["      도로경계블럭 설치","콘크리트,120×120×1000",14025,"M"]
["      무근콘크리트타설","빈배합(leanmix)",273,"㎥"]
["      거푸집공/거친마감","0-7m",2805,"M2"]
["      모르터(1:3)(토목,조경)","",2,"㎥"]
["    4) 중앙분리경계석","",0,""]
["     가) 중앙분리경계석(회전차로)","",0,""]
["      중앙분리 경계석 설치","화강석,200×250×1000",49,"M"]
["      무근콘크리트타설","빈배합(leanmix)",2,"㎥"]
["      모르터(1:3)(토목,조경)","",2.5000000000000001E-2,"㎥"]
["   바. 교통시설공","",0,""]
["    1) 험프횡단보도(7개소)","",0,""]
["     가) 칼라아스콘포장","적색, T=5cm",586,"M2"]
["     나) 아스콘포장/표층 포설및다짐","T = 10cm",488,"㎡"]
["     다) 아스콘포장/택코팅","RSC-4",1172,"㎡"]
["     라) 융착성도료형수동식/횡단보/백색","",218,"㎡"]
["     마) 차선도색(기타 재료비)","백색-재료비",218,"㎡"]
["    2) 고원식교차로(3개소)","",0,""]
["     가) 칼라아스콘포장","T = 7cm",874,"㎡"]
["     나) 아스콘포장/택코팅","RSC-4",1044,"㎡"]
["     다) 융착성도료형수동식/횡단보/백색","",167,"㎡"]
["     라) 차선도색(기타 재료비)","백색-재료비",167,"㎡"]
["    3) 과속방지턱(8개소)","",0,""]
["     가) 아스콘포장/표층 포설및다짐","T = 8-10cm",154,"㎡"]
["     나) 아스콘포장/택코팅","RSC-4",272,"㎡"]
["     다) 융착성도료형 수동식/실선,황색","",136,"㎡"]
["     라) 융착성도료형 수동식/실선,백색","",136,"㎡"]
["     마) 차선도색(기타 재료비)","황색-재료비",136,"㎡"]
["     바) 차선도색(기타 재료비)","백색-재료비",136,"㎡"]
["    4) 도로표지병","",0,""]
["     가) 도로표지병(설치)","",741,"EA"]
["    5) 차선도색","",0,""]
["     가) 차선도색(융착식도료형)","수동식(황색,실선)",869,"㎡"]
["     나) 차선도색(융착식도료형)","수동식(백색,실선)",1006,"㎡"]
["     다) 차선도색(융착식도료형)","수동식(백색,파선)",193,"㎡"]
["     라) 차선도색(융착식도료형)","수동식(백색,문자,기호)",377,"㎡"]
["     마) 차선도색(융착식도료형)","수동식(백색,횡단보도,주차장)",1754,"㎡"]
["     바) 차선도색(기타 재료비)","황색-재료비",869,"㎡"]
["     사) 차선도색(기타 재료비)","백색-재료비",3330,"㎡"]
["    6) 표지판","",0,""]
["     가) 어린이보호구역표지판 설치","",0,""]
["      어린이보호구역표지판 설치비","사각3000x2000",3,"EA"]
["      철근콘크리트타설","다짐포함",22,"㎥"]
["      거푸집공/거친마감","0-7m",48,"㎡"]
["      철근가공조립","간단",2.157,"Ton"]
["     나) 견인지역표지판 설치","",0,""]
["      견인지역표지판 설치비","사각600x600mm",8,"EA"]
["      레미콘타설","소형구조물,리어카소운반",1,"㎥"]
["      거푸집공/거친마감","0-7m",10,"㎡"]
["     다) 주정차금지표지판 설치","",0,""]
["      주정차금지표지판 설치비","원형ø600",8,"EA"]
["      레미콘타설","소형구조물,리어카소운반",1,"㎥"]
["      거푸집공/거친마감","0-7m",10,"㎡"]
["     라) 어린이보호표지판 설치","",0,""]
["      어린이보호표지판 설치비","삼각2.0Tx900mm",15,"EA"]
["      레미콘타설","소형구조물,리어카소운반",2,"㎥"]
["      거푸집공/거친마감","0-7m",19,"㎡"]
["     마) 갈매기표지판 설치","",0,""]
["      갈매기표지판 설치비","사각450x600mm",13,"EA"]
["      레미콘타설","소형구조물,리어카소운반",1,"㎥"]
["      거푸집공/거친마감","0-7m",6,"㎡"]
["     바) 좌회전금지표지판 설치","",0,""]
["      좌회전금지표지판 설치비","원형ø600",6,"EA"]
["      레미콘타설","소형구조물,리어카소운반",1,"㎥"]
["      거푸집공/거친마감","0-7m",8,"㎡"]
["     사) 일방통행표지판 설치","",0,""]
["      일방통행표지판 설치비","사각600x600mm",8,"EA"]
["      레미콘타설","소형구조물,리어카소운반",1,"㎥"]
["      거푸집공/거친마감","0-7m",10,"㎡"]
["    7) 보호휀스(어린이보호구역)","",0,""]
["     가) 레미콘타설","소형구조물,리어카소운반",11,"㎥"]
["     나) 거푸집공/거친마감","0-7m",150,"㎡"]
["    8) 회전교차로","",0,""]
["     가) 유공관설치","D200mm, P.E유공관",40,"M"]
["     나) 부직포설치-맹암거용","350g/㎡",288,"㎡"]
["     다) 골재 운반","L=498m",10,"㎥"]
["     라) 막자갈부설","t=20cm",8,"㎥"]
["   사. 부대공","",0,""]
["    1) 가로수분","",0,""]
["     가) 가로수분,정사각형","인조화강석 1170×1170",12,"EA"]
["    2) 도로반사경","",0,""]
["     가) 도로반사경 설치비","600×800",4,"개소"]
["     나) 레미콘타설","소형구조물,리어카소운반",1,"㎥"]
["     다) 거푸집공/거친마감","0-7m",10,"㎡"]
["    3) 볼라이드","",0,""]
["     가) 레미콘타설","소형구조물,리어카소운반",1,"㎥"]
["     나) 거푸집공/거친마감","0-7m",10,"㎡"]
["    4) 식수대 활용구간","",0,""]
["     가) 유공관설치","D200mm, P.E유공관",5586,"M"]
["     나) 부직포설치-맹암거용","350g/㎡",3493,"㎡"]
["     다) 보조기층재 운반","L=498m",65,"㎥"]
["     라) 막자갈부설","t=20cm",62,"㎥"]
["    5) 자전거보관소","L5,660×W2,179×H2,500,(12개소)",0,""]
["     가) 무근콘크리트타설","소형구조물",22,"m3"]
["     나) 거푸집/거친마감","0-7m",178,"m2"]
["    6) 쇄석및잡석생산","",0,""]
["     가) 골재선별및생산(발파암)","보통암,동상방지층,Ø100mm이하",9913,"㎥"]
["     가) 골재선별및생산(발파암)","보통암,보조기층,Ø80mm이하",11027,"㎥"]
["     나) 골재선별및생산(발파암)","보통암,골재,Ø40mm이하",3889,"㎥"]
["   아. 주요자재 구입","",0,""]
["    1) 철근","",0,""]
["     가) 고철","중량A",0.126,"Ton"]
["    2) 시멘트","",0,""]
["     가) 시멘트","40kg/포",99,"포"]
["    3) 모래","",0,""]
["     가) 석분","구입",987,"㎥"]
["     나) 모래","",9,"㎥"]
["    4) 아스팔트유제","",0,""]
["     가) 아스팔트유제(KSM2203)","프라임코팅,RS(C)-3",495,"D/M"]
["     나) 아스팔트유제(KSM2203)","택코팅,RS(C)-4",217,"D/M"]
["    5) 볼라드","",0,""]
["     가) 볼라드","110×900",28,"개"]
["    6) 도로 표지병","",0,""]
["     가) 도로표지병","130*110*30",741,"개"]
["    7) 수목보호틀","",0,""]
["     가) 수목보호틀","1170 x 1170",12,"nr"]
["    8) 도로반사경","",0,""]
["     가) 도로반사경","600×800",4,"조"]
["     나) 도로반사경 지주","ø76",4,"조"]
["   자. 주요자재 운반","",0,""]
["    1) 철근운반","",0,""]
["     가) 철근운반","L=10.00km(하치장-현장)",2.2829999999999999,"Ton"]
["    2) 시멘트운반","",0,""]
["     가) 시멘트운반","40kg/포,L=10km(하치장-현장)",99,"포"]
["  ","",0,""]
["  3. 우수공사","",0,""]
["   가. 토공","",0,""]
["    1) 터파기","",0,""]
["     가) 토사","",0,""]
["      터파기/육상토사","0-2m 기계",76182,"M3"]
["      터파기/육상토사","0-6m 기계",2493,"M3"]
["     나) 리핑암","",0,""]
["      터파기/육상리핑암","0-2m,기계",481,"m3"]
["     다) 발파암","",0,""]
["      터파기/육상발파암(연암)","0-2m 기계",326,"㎥"]
["      터파기/육상발파암(보통암)","0-2m 기계",358,"㎥"]
["    2) 되메우기","",0,""]
["     가) 되메우기/토사(기계100%)","",64905,"㎥"]
["     나) 되메우기/토사(인력30%)","다짐",5462,"m3"]
["     다) 잔토처리","",0,""]
["      잔토처리","토사",11340,"㎥"]
["      잔토처리","리핑암",646,"㎥"]
["      잔토처리","발파암(연암)",766,"㎥"]
["      잔토처리","발파암(보통암)",1481,"㎥"]
["   나. 관로","",0,""]
["    1) 파형강관","",0,""]
["     가) D250mm","",0,""]
["      PL파형강관접합 및 부설","D250mm",4771,"M"]
["     나) D450mm","",0,""]
["      HPL파형강관접합 및 부설","D450mm",4569,"M"]
["     다) D500mm","",0,""]
["      HPL파형강관접합 및 부설","D=500mm",244,"M"]
["     라) D600mm","",0,""]
["      HPL파형강관접합 및 부설","D=600mm",364,"M"]
["     마) D700mm","",0,""]
["      PE2중피복 파형강관접합 및 부설","D=700mm",819,"M"]
["     바) D800mm","",0,""]
["      PE2중피복 파형강관접합 및 부설","D=800mm",637,"M"]
["     사) D900mm","",0,""]
["      PE2중피복 파형강관접합 및 부설","D=900mm",326,"M"]
["     아) D1000mm","",0,""]
["      PE2중피복 파형강관접합 및 부설","D=1000mm",56,"M"]
["     자) D1100mm","",0,""]
["      PE2중피복 파형강관접합 및 부설","D=1100mm",242,"M"]
["     차) D1200mm","",0,""]
["      PE2중피복 파형강관접합 및 부설","D=1200mm",923,"M"]
["     카) D1350mm","",0,""]
["      PE2중피복 파형강관접합 및 부설","D=1350mm",78,"M"]
["     타) D1500mm","",0,""]
["      파형강관(평활형)접합 및 부설","D=1500mm",277,"M"]
["    2) 관날개벽","",0,""]
["     가) 철근콘크리트타설","다짐포함",10,"㎥"]
["     나) 거푸집공/보통마감","0-7m",37,"㎡"]
["     다) 철근가공조립","보통",0.16700000000000001,"Ton"]
["    3) 관기초","",0,""]
["     가) 무근콘크리트타설","빈배합(leanmix)",348,"㎥"]
["     나) 거푸집공/거친마감","0-7m",122,"㎡"]
["     다) 모래부설및다짐","석분",5469,"㎥"]
["    4) 관거 내부조사 및 경고용테이프","",0,""]
["     가) 우수관경고용테이프","회색,10cm",12800,"M"]
["     나) 우수관식별용테이프","회색,10cm",12800,"M"]
["     다) 하수관거 내부조사","신설",6959,"M"]
["     라) 하수도기계준설","흡입준설기(25Ton)",432,"㎥"]
["   다. 암거","",0,""]
["    1) PC암거설치","",0,""]
["     가) PC 암거설치 및 운반","1.5×1.8",219,"M"]
["     나) PC 암거설치 및 운반","1.5×2.3-낙차부",24,"M"]
["     다) PC 암거 기초","",0,""]
["      무근콘크리트타설","빈배합(leanmix)",52,"㎥"]
["      거푸집공/거친마감","0-7m",69,"㎡"]
["      모래 부설 및 다짐","",10,"㎥"]
["     라) 기초잡석","",0,""]
["      기초잡석부설,다짐,운반","80mm이하",147,"㎥"]
["    2) 현장타설암거","",0,""]
["     가) RC 암거설치(직선부)","1@2.0×2.0(H=3.00m미만),L=228.70m",0,""]
["      무근콘크리트타설","빈배합(leanmix)",64,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",640,"㎥"]
["      거푸집공/유로폼","0-7M",2013,"㎡"]
["      거푸집공/보통마감","0-7m",538,"㎡"]
["      거푸집공/거친마감","0-7m",50,"㎡"]
["      강관동바리","암거용(3개월)",815,"공/㎥"]
["      강관비계","3개월이하",1189,"㎡"]
["      체어블럭","슬라브 및 기초",961,"㎡"]
["      스페이셔","벽체용",2013,"㎡"]
["      지수판(시공이음용)","200×5",457,"M"]
["      조인트/스티로폴","T=20mm",54,"㎡"]
["      지수판(신축이음용)","200×5",176,"M"]
["      실런트충진","",160,"ｍ"]
["      시공이음면정리","",137,"m2"]
["      철근가공조립","복잡",52.829000000000001,"Ton"]
["     나) RC 암거설치(직선부)","1@2.5×2.0(H=3.00m미만),L=62.23m",0,""]
["      무근콘크리트타설","빈배합(leanmix)",21,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",193,"㎥"]
["      거푸집공/유로폼","0-7M",547,"㎡"]
["      거푸집공/보통마감","0-7m",179,"㎡"]
["      거푸집공/거친마감","0-7m",14,"㎡"]
["      강관동바리","암거용(3개월)",278,"공/㎥"]
["      강관비계","3개월이하",324,"㎡"]
["      체어블럭","슬라브 및 기초",324,"㎡"]
["      스페이셔","벽체용",548,"㎡"]
["      지수판(시공이음용)","200×5",124,"M"]
["      조인트/스티로폴","T=20mm",20,"㎡"]
["      지수판(신축이음용)","200×5",66,"M"]
["      실런트충진","",60,"ｍ"]
["      시공이음면정리","",37,"m2"]
["      철근가공조립","복잡",18.792999999999999,"Ton"]
["     다) RC 암거설치(직선부)","1@2.5×2.0(H=5.00m미만),L=109.10m",0,""]
["      무근콘크리트타설","빈배합(leanmix)",36,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",338,"㎥"]
["      거푸집공/유로폼","0-7M",960,"㎡"]
["      거푸집공/보통마감","0-7m",313,"㎡"]
["      거푸집공/거친마감","0-7m",24,"㎡"]
["      강관동바리","암거용(3개월)",541,"공/㎥"]
["      강관비계","3개월이하",567,"㎡"]
["      체어블럭","슬라브 및 기초",567,"㎡"]
["      스페이셔","벽체용",960,"㎡"]
["      지수판(시공이음용)","200×5",218,"M"]
["      조인트/스티로폴","T=20mm",34,"㎡"]
["      지수판(신축이음용)","200×5",112,"M"]
["      실런트충진","",103,"ｍ"]
["      시공이음면정리","",65,"m2"]
["      철근가공조립","복잡",39.712000000000003,"Ton"]
["     라) RC 암거설치(낙차부)","1@2.0×2.0(H=3.00m미만),L=27.00m",0,""]
["      무근콘크리트타설","빈배합(leanmix)",15,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",151,"㎥"]
["      거푸집공/유로폼","0-7M",475,"㎡"]
["      거푸집공/보통마감","0-7m",121,"㎡"]
["      거푸집공/거친마감","0-7m",11,"㎡"]
["      강관동바리","암거용(3개월)",192,"공/㎥"]
["      강관비계","3개월이하",281,"㎡"]
["      체어블럭","슬라브 및 기초",227,"㎡"]
["      스페이셔","벽체용",475,"㎡"]
["      지수판(신축이음용)","200×5",111,"M"]
["      시공이음면정리","",33,"m2"]
["      철근가공조립","복잡",13.473000000000001,"Ton"]
["     마) RC 암거설치(낙차부)","1@2.5×2.0(H=3.00m미만),L=14.00m",0,""]
["      무근콘크리트타설","빈배합(leanmix)",9,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",87,"㎥"]
["      거푸집공/유로폼","0-7M",246,"㎡"]
["      거푸집공/보통마감","0-7m",77,"㎡"]
["      거푸집공/거친마감","0-7m",6,"㎡"]
["      강관동바리","암거용(3개월)",125,"공/㎥"]
["      강관비계","3개월이하",146,"㎡"]
["      체어블럭","슬라브 및 기초",146,"㎡"]
["      스페이셔","벽체용",246,"㎡"]
["      지수판(신축이음용)","200×5",58,"M"]
["      시공이음면정리","",17,"m2"]
["      철근가공조립","복잡",9.0579999999999998,"Ton"]
["     바) RC 암거설치(낙차부)","1@2.5×2.0(H=6.00m미만),L=25.00m",0,""]
["      무근콘크리트타설","빈배합(leanmix)",17,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",155,"㎥"]
["      거푸집공/유로폼","0-7M",440,"㎡"]
["      거푸집공/보통마감","0-7m",137,"㎡"]
["      거푸집공/거친마감","0-7m",10,"㎡"]
["      강관동바리","암거용(3개월)",248,"공/㎥"]
["      강관비계","3개월이하",260,"㎡"]
["      체어블럭","슬라브 및 기초",260,"㎡"]
["      스페이셔","벽체용",440,"㎡"]
["      지수판(신축이음용)","200×5",103,"M"]
["      시공이음면정리","",31,"m2"]
["      철근가공조립","복잡",19.225000000000001,"Ton"]
["     사) RC 암거설치(단면변화부#1)","1@2.0×2.0+1@1.5×1.8",0,""]
["      무근콘크리트타설","빈배합(leanmix)",1,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",11,"㎥"]
["      거푸집공/유로폼","0-7M",35,"㎡"]
["      거푸집공/보통마감","0-7m",12,"㎡"]
["      거푸집공/거친마감","0-7m",1,"㎡"]
["      강관동바리","암거용(3개월)",15,"공/㎥"]
["      강관비계","3개월이하",21,"㎡"]
["      체어블럭","슬라브 및 기초",16,"㎡"]
["      스페이셔","벽체용",35,"㎡"]
["      지수판(신축이음용)","200×5",8,"M"]
["      시공이음면정리","",2,"m2"]
["      철근가공조립","복잡",0.93899999999999995,"Ton"]
["     아) RC 암거설치(단면변화부#2)","1@2.5×2.0+1@2.0×2.0",0,""]
["      무근콘크리트타설","빈배합(leanmix)",1,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",12,"㎥"]
["      거푸집공/유로폼","0-7M",35,"㎡"]
["      거푸집공/보통마감","0-7m",10,"㎡"]
["      거푸집공/거친마감","0-7m",1,"㎡"]
["      강관동바리","암거용(3개월)",19,"공/㎥"]
["      강관비계","3개월이하",21,"㎡"]
["      체어블럭","슬라브 및 기초",20,"㎡"]
["      스페이셔","벽체용",35,"㎡"]
["      지수판(신축이음용)","200×5",8,"M"]
["      시공이음면정리","",2,"m2"]
["      철근가공조립","복잡",1.256,"Ton"]
["     자) RC 암거설치(곡각부)","1@2.5×2.0, 1EA",0,""]
["      무근콘크리트타설","빈배합(leanmix)",2,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",15,"㎥"]
["      거푸집공/유로폼","0-7M",26,"㎡"]
["      거푸집공/보통마감","0-7m",32,"㎡"]
["      거푸집공/거친마감","0-7m",1,"㎡"]
["      강관동바리","암거용(3개월)",25,"공/㎥"]
["      강관비계","3개월이하",21,"㎡"]
["      체어블럭","슬라브 및 기초",26,"㎡"]
["      스페이셔","벽체용",42,"㎡"]
["      철근가공조립","복잡",0.56499999999999995,"Ton"]
["     차) RC 암거설치(방류부)","1@2.5×2.0, 1EA",0,""]
["      무근콘크리트타설","빈배합(leanmix)",1,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",8,"㎥"]
["      거푸집공/유로폼","0-7M",13,"㎡"]
["      거푸집공/보통마감","0-7m",16,"㎡"]
["      거푸집공/거친마감","0-7m",1,"㎡"]
["      강관동바리","암거용(3개월)",10,"공/㎥"]
["      강관비계","3개월이하",11,"㎡"]
["      체어블럭","슬라브 및 기초",26,"㎡"]
["      스페이셔","벽체용",21,"㎡"]
["      철근가공조립","복잡",0.81599999999999995,"Ton"]
["     카) RC 암거날개벽","",0,""]
["      무근콘크리트타설","빈배합(leanmix)",1,"㎥"]
["      철근콘크리트타설/펌프카","슬럼프 8-12cm(50㎥미만)",14,"㎥"]
["      거푸집공/보통마감","0-7m",40,"㎡"]
["      거푸집공/거친마감","0-7m",1,"㎡"]
["      강관비계","3개월이하",22,"㎡"]
["      체어블럭","슬라브 및 기초",12,"㎡"]
["      스페이셔","벽체용",29,"㎡"]
["      철근가공조립","복잡",0.96799999999999997,"Ton"]
["     타) RC 암거 관 유입부 접합","",0,""]
["      무근콘크리트타설","빈배합(leanmix)",3,"㎥"]
["      거푸집공/거친마감","0-7m",31,"㎡"]
["      철근가공조립","복잡",2.3450000000000002,"Ton"]
["     파) 기초잡석","",0,""]
["      기초잡석부설,다짐,운반","80mm이하",509,"㎥"]
["   라. 맨홀","",0,""]
["    1) 우수원형1호맨홀","",0,""]
["     가) 우수원형1호맨홀-차도측","D900mm, H=1.68m(70개소)",0,""]
["      모르터","1 : 2",0.4,"㎥"]
["      인력비빔타설(소형구조물)","",6,"㎥"]
["      철근콘크리트타설","다짐포함",15,"㎥"]
["      무근콘크리트타설","소형구조물",109,"㎥"]
["      거푸집공/보통마감","0-7m",25,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",70,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ900",118,"M"]
["      강재거푸집(D=3m)","0-7m",35,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",280,"개소"]
["      강관동바리","암거용(3개월)",42,"공/㎥"]
["      체어블럭","슬라브 및 기초",73,"㎡"]
["      차도측 뚜껑 및 받침대 설치","D648MM",70,"조"]
["      철근가공조립","보통",2.0299999999999998,"Ton"]
["     나) 우수보강원형1호맨홀-차도측","D900mm, H=2.35m(8개소)",0,""]
["      모르터","1 : 2",0.04,"㎥"]
["      인력비빔타설(소형구조물)","",0.7,"㎥"]
["      철근콘크리트타설","다짐포함",2,"㎥"]
["      무근콘크리트타설","소형구조물",28,"㎥"]
["      거푸집공/보통마감","0-7m",3,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",8,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ900",20,"M"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",56,"개소"]
["      강관동바리","암거용(3개월)",7,"공/㎥"]
["      체어블럭","슬라브 및 기초",12,"㎡"]
["      차도측 뚜껑 및 받침대 설치","D648MM",8,"조"]
["      철근가공조립","보통",0.26400000000000001,"Ton"]
["     다) 우수원형1호맨홀-보도측","D900mm, H=1.76m(7개소)",0,""]
["      모르터","1 : 2",0.03,"㎥"]
["      인력비빔타설(소형구조물)","",0.3,"㎥"]
["      철근콘크리트타설","다짐포함",1,"㎥"]
["      무근콘크리트타설","소형구조물",11,"㎥"]
["      거푸집공/보통마감","0-7m",3,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",7,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ900",12,"M"]
["      강재거푸집(D=3m)","0-7m",3,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",28,"개소"]
["      강관동바리","암거용(3개월)",4,"공/㎥"]
["      체어블럭","슬라브 및 기초",7,"㎡"]
["      보도맨홀 뚜껑 및 받침대 설치","보도측",7,"조"]
["      철근가공조립","보통",0.20300000000000001,"Ton"]
["     라) 우수보강원형1호맨홀-보도측","D900mm, H=2.42m(4개소)",0,""]
["      모르터","1 : 2",0.02,"㎥"]
["      인력비빔타설(소형구조물)","",0.1,"㎥"]
["      철근콘크리트타설","다짐포함",1,"㎥"]
["      무근콘크리트타설","소형구조물",14,"㎥"]
["      거푸집공/보통마감","0-7m",1,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",4,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ900",10,"M"]
["      강재거푸집(D=3m)","0-7m",2,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",28,"개소"]
["      강관동바리","암거용(3개월)",3,"공/㎥"]
["      체어블럭","슬라브 및 기초",6,"㎡"]
["      보도맨홀 뚜껑 및 받침대 설치","보도측",4,"조"]
["      철근가공조립","보통",0.13200000000000001,"Ton"]
["    2) 우수원형2호맨홀","",0,""]
["     가) 우수원형2호맨홀-차도측","1200mm, H=1.95m(8개소)",0,""]
["      모르터","1 : 2",0.05,"㎥"]
["      인력비빔타설(소형구조물)","",1,"㎥"]
["      철근콘크리트타설","다짐포함",3,"㎥"]
["      무근콘크리트타설","소형구조물",24,"㎥"]
["      거푸집공/보통마감","0-7m",7,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø1200mm",8,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ1200",16,"M"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",40,"개소"]
["      강관동바리","암거용(3개월)",13,"공/㎥"]
["      체어블럭","슬라브 및 기초",16,"㎡"]
["      차도측 뚜껑 및 받침대 설치","D648MM",8,"조"]
["      철근가공조립","보통",0.60799999999999998,"Ton"]
["     나) 우수원형2호맨홀-보도측","1200mm, H=1.94m(6개소)",0,""]
["      모르터","1 : 2",0.02,"㎥"]
["      인력비빔타설(소형구조물)","",0.2,"㎥"]
["      철근콘크리트타설","다짐포함",2,"㎥"]
["      무근콘크리트타설","소형구조물",18,"㎥"]
["      거푸집공/보통마감","0-7m",5,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø1200mm",6,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ1200",12,"M"]
["      강재거푸집(D=3m)","0-7m",3,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",30,"개소"]
["      강관동바리","암거용(3개월)",10,"공/㎥"]
["      체어블럭","슬라브 및 기초",12,"㎡"]
["      보도맨홀 뚜껑 및 받침대 설치","보도측",6,"조"]
["      철근가공조립","보통",0.45600000000000002,"Ton"]
["     다) 우수보강원형2호맨홀-차도측","1200mm, H=2.06m(7개소)",0,""]
["      모르터","1 : 2",0.04,"㎥"]
["      인력비빔타설(소형구조물)","",0.9,"㎥"]
["      철근콘크리트타설","다짐포함",4,"㎥"]
["      무근콘크리트타설","소형구조물",49,"㎥"]
["      거푸집공/보통마감","0-7m",6,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø1200mm",7,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ1200",23,"M"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",63,"개소"]
["      강관동바리","암거용(3개월)",20,"공/㎥"]
["      체어블럭","슬라브 및 기초",18,"㎡"]
["      차도측 뚜껑 및 받침대 설치","D648MM",7,"조"]
["      철근가공조립","보통",0.61599999999999999,"Ton"]
["     라) 우수보강원형2호맨홀-보도측","1200mm, H=1.94m(2개소)",0,""]
["      모르터","1 : 2",0.01,"㎥"]
["      인력비빔타설(소형구조물)","",7.0000000000000007E-2,"㎥"]
["      철근콘크리트타설","다짐포함",1,"㎥"]
["      무근콘크리트타설","소형구조물",11,"㎥"]
["      거푸집공/보통마감","0-7m",2,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø1200mm",2,"nr"]
["      합성수지(P．E)원형맨홀거푸집","벽체 φ1200",5,"M"]
["      강재거푸집(D=3m)","0-7m",1,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",14,"개소"]
["      강관동바리","암거용(3개월)",4,"공/㎥"]
["      체어블럭","슬라브 및 기초",5,"㎡"]
["      보도맨홀 뚜껑 및 받침대 설치","보도측",2,"조"]
["      철근가공조립","보통",0.17599999999999999,"Ton"]
["    3) 우수각형특2호맨홀","",0,""]
["     가) 우수각형특2호맨홀-차도측","1200×1200mm,H=2.37m(15개소)",0,""]
["      모르터","1 : 2",0.09,"㎥"]
["      인력비빔타설(소형구조물)","",1.8,"㎥"]
["      철근콘크리트타설","다짐포함",77,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",7,"㎥"]
["      거푸집공/매끈한마감","0-7m",6,"㎡"]
["      거푸집공/보통마감","0-7m",17,"㎡"]
["      거푸집공/유로폼","0-7M",482,"㎡"]
["      강재거푸집(D=3m)","0-7m",8,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",90,"개소"]
["      강관동바리","암거용(3개월)",41,"공/㎥"]
["      스페이셔","벽체용",171,"㎡"]
["      체어블럭","슬라브 및 기초",99,"㎡"]
["      철근가공조립","보통",14.31,"Ton"]
["      차도측 뚜껑 및 받침대 설치","D648MM",15,"조"]
["     나) 우수각형특2호맨홀-보도측","1200×1200mm,H=2.76m(11개소)",0,""]
["      모르터","1 : 2",0.04,"㎥"]
["      인력비빔타설(소형구조물)","",0.4,"㎥"]
["      철근콘크리트타설","다짐포함",63,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",5,"㎥"]
["      거푸집공/매끈한마감","0-7m",4,"㎡"]
["      거푸집공/보통마감","0-7m",13,"㎡"]
["      거푸집공/유로폼","0-7M",403,"㎡"]
["      강재거푸집(D=3m)","0-7m",5,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",88,"개소"]
["      강관동바리","암거용(3개월)",35,"공/㎥"]
["      스페이셔","벽체용",146,"㎡"]
["      체어블럭","슬라브 및 기초",73,"㎡"]
["      철근가공조립","보통",11.209,"Ton"]
["      보도측 뚜껑 및 받침대 설치","보도측",11,"조"]
["    4) 우수각형특3호맨홀","",0,""]
["     가) 우수각형특3호맨홀-차도측","1400×1200mm, H=3.01m(12개소)",0,""]
["      모르터","1 : 2",7.0000000000000007E-2,"㎥"]
["      인력비빔타설(소형구조물)","",1.5,"㎥"]
["      철근콘크리트타설","다짐포함",79,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",6,"㎥"]
["      거푸집공/매끈한마감","0-7m",5,"㎡"]
["      거푸집공/보통마감","0-7m",17,"㎡"]
["      거푸집공/유로폼","0-7M",506,"㎡"]
["      강재거푸집(D=3m)","0-7m",6,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",108,"개소"]
["      강관동바리","암거용(3개월)",50,"공/㎥"]
["      스페이셔","벽체용",376,"㎡"]
["      체어블럭","슬라브 및 기초",88,"㎡"]
["      철근가공조립","보통",8.2919999999999998,"Ton"]
["      차도측 뚜껑 및 받침대 설치","D648MM",12,"조"]
["     나) 우수각형특3호맨홀-보도측","1400×1200mm, H=2.89m(2개소)",0,""]
["      모르터","1 : 2",0.01,"㎥"]
["      인력비빔타설(소형구조물)","",0.11,"㎥"]
["      철근콘크리트타설","다짐포함",28,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",2,"㎥"]
["      거푸집공/매끈한마감","0-7m",1,"㎡"]
["      거푸집공/보통마감","0-7m",4,"㎡"]
["      거푸집공/유로폼","0-7M",195,"㎡"]
["      강재거푸집(D=3m)","0-7m",1,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",30,"개소"]
["      등받이 사다리","스테인레스 스틸",6,"M"]
["      강관동바리","암거용(3개월)",20,"공/㎥"]
["      스페이셔","벽체용",151,"㎡"]
["      체어블럭","슬라브 및 기초",22,"㎡"]
["      철근가공조립","보통",3.2280000000000002,"Ton"]
["      보도측 뚜껑 및 받침대 설치","보도측",3,"조"]
["    5) 우수각형특4호맨홀","",0,""]
["     가) 우수각형특4호맨홀-차도측","1500×1500mm, H=2.89m(6개소)",0,""]
["      모르터","1 : 2",0.04,"㎥"]
["      인력비빔타설(소형구조물)","",0.7,"㎥"]
["      철근콘크리트타설","다짐포함",45,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",4,"㎥"]
["      거푸집공/매끈한마감","0-7m",3,"㎡"]
["      거푸집공/보통마감","0-7m",12,"㎡"]
["      거푸집공/유로폼","0-7M",277,"㎡"]
["      강재거푸집(D=3m)","0-7m",3,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",48,"개소"]
["      강관동바리","암거용(3개월)",34,"공/㎥"]
["      스페이셔","벽체용",104,"㎡"]
["      체어블럭","슬라브 및 기초",54,"㎡"]
["      철근가공조립","보통",10.446,"Ton"]
["      차도측 뚜껑 및 받침대 설치","D648MM",6,"조"]
["     나) 우수각형특4호맨홀-보도측","1500×1500mm, H=3.03m(2개소)",0,""]
["      모르터","1 : 2",0.01,"㎥"]
["      인력비빔타설(소형구조물)","",7.0000000000000007E-2,"㎥"]
["      철근콘크리트타설","다짐포함",36,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",1,"㎥"]
["      거푸집공/매끈한마감","0-7m",1,"㎡"]
["      거푸집공/보통마감","0-7m",4,"㎡"]
["      거푸집공/유로폼","0-7M",257,"㎡"]
["      강재거푸집(D=3m)","0-7m",1,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",27,"개소"]
["      등받이 사다리","스테인레스 스틸",11,"M"]
["      강관동바리","암거용(3개월)",34,"공/㎥"]
["      스페이셔","벽체용",105,"㎡"]
["      체어블럭","슬라브 및 기초",18,"㎡"]
["      철근가공조립","보통",9.67,"Ton"]
["      보도측 뚜껑 및 받침대 설치","보도측",2,"조"]
["    6) 우수각형특5호맨홀","",0,""]
["     가) 우수각형특5호맨홀-차도측","1500×1800mm, H=2.85m(5개소)",0,""]
["      모르터","1 : 2",0.03,"㎥"]
["      인력비빔타설(소형구조물)","",0.6,"㎥"]
["      철근콘크리트타설","다짐포함",52,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",4,"㎥"]
["      거푸집공/매끈한마감","0-7m",3,"㎡"]
["      거푸집공/보통마감","0-7m",12,"㎡"]
["      거푸집공/유로폼","0-7M",259,"㎡"]
["      강재거푸집(D=3m)","0-7m",3,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",40,"개소"]
["      강관동바리","암거용(3개월)",34,"공/㎥"]
["      스페이셔","벽체용",188,"㎡"]
["      체어블럭","슬라브 및 기초",56,"㎡"]
["      철근가공조립","보통",6.57,"Ton"]
["      차도측 뚜껑 및 받침대 설치","D648MM",6,"조"]
["     나) 우수각형특5호맨홀-보도측","1500×1800mm, H=4.57m(10개소)",0,""]
["      모르터","1 : 2",0.04,"㎥"]
["      인력비빔타설(소형구조물)","",0.4,"㎥"]
["      철근콘크리트타설","다짐포함",151,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",8,"㎥"]
["      거푸집공/매끈한마감","0-7m",6,"㎡"]
["      거푸집공/보통마감","0-7m",24,"㎡"]
["      거푸집공/유로폼","0-7M",838,"㎡"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",150,"개소"]
["      강관동바리","암거용(3개월)",118,"공/㎥"]
["      스페이셔","벽체용",647,"㎡"]
["      체어블럭","슬라브 및 기초",112,"㎡"]
["      철근가공조립","보통",19.95,"Ton"]
["      보도측 뚜껑 및 받침대 설치","보도측",10,"조"]
["    7) 우수암거맨홀","",0,""]
["     가) 우수암거맨홀-차도측","900×900mm, H=1.26m(6개소)",0,""]
["      모르터","1 : 2",0.04,"㎥"]
["      인력비빔타설(소형구조물)","",0.7,"㎥"]
["      철근콘크리트타설","다짐포함",15,"㎥"]
["      거푸집공/매끈한마감","0-7m",3,"㎡"]
["      거푸집공/보통마감","0-7m",3,"㎡"]
["      거푸집공/유로폼","0-7M",106,"㎡"]
["      강재거푸집(D=3m)","0-7m",3,"M2"]
["      맨홀발디딤쇠","PE코팅, D22mm",72,"개소"]
["      스페이셔","벽체용",38,"㎡"]
["      체어블럭","슬라브 및 기초",10,"㎡"]
["      철근가공조립","보통",1.3620000000000001,"Ton"]
["      차도측 뚜껑 및 받침대 설치","D648MM",6,"조"]
["    8) 맨홀 및 관 접속부","",0,""]
["     가) 모르터","1 : 2",5.2430000000000003,"㎥"]
["   마. 우수받이","",0,""]
["    1) 현장타설 - 0．4m X 0．3m","400×300mm(667EA)",0,""]
["     가) 무근콘크리트타설","다짐포함",261,"㎥"]
["     나) 모르터","1 : 2",3.9350000000000001,"㎥"]
["     다) 거푸집공/보통마감","0-7m",3098,"㎡"]
["    2) 현장타설 - 0．8m X 0．3m","800×300mm(11EA)",0,""]
["     가) 무근콘크리트타설","다짐포함",7,"㎥"]
["     나) 모르터","1 : 2",7.0000000000000007E-2,"㎥"]
["     다) 거푸집공/보통마감","0-7m",76,"㎡"]
["   바. 집수정","",0,""]
["    1) 집수정","300×300mm(67개소)",0,""]
["     가) 무근콘크리트타설","다짐포함",37,"㎥"]
["     나) 거푸집공/보통마감","0-7m",449,"㎡"]
["     다) 모르터","1 : 2",0.48299999999999998,"㎥"]
["    2) 집수정","600×600mm(1개소)",0,""]
["     가) 무근콘크리트타설","다짐포함",1,"㎥"]
["     나) 거푸집공/보통마감","0-7m",10,"㎡"]
["     다) 모르터","1 : 2",0.01,"㎥"]
["    3) 집수정","900×900mm(95개소)",0,""]
["     가) 무근콘크리트타설","다짐포함",161,"㎥"]
["     나) 거푸집공/보통마감","0-7m",1310,"㎡"]
["     다) 모르터","1 : 2",0.68500000000000005,"㎥"]
["    4) 집수정","1,500×1,500mm(9개소)",0,""]
["     가) 철근콘크리트타설","다짐포함",49,"㎥"]
["     나) 무근콘크리트타설","빈배합(leanmix)",4,"㎥"]
["     다) 거푸집공/보통마감","0-7m",438,"㎡"]
["     라) 거푸집공/거친마감","0-7m",8,"㎡"]
["     마) 철근가공조립","간단",3.133,"Ton"]
["     바) 모르터","1 : 2",6.4000000000000001E-2,"㎥"]
["   사. 측구","",0,""]
["    1) U형측구","",0,""]
["     가) U형측구","300×300(L=622.99m)",0,""]
["      무근콘크리트타설","다짐포함",118,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",50,"㎥"]
["      거푸집/유로폼","0-7M",1059,"m2"]
["      거푸집공/거친마감","0-7m",125,"㎡"]
["      조인트/스티로폴","T=20mm",8,"㎡"]
["     나) U형측구","400×400(L=2798.49m)",0,""]
["      무근콘크리트타설","다짐포함",658,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",252,"㎥"]
["      거푸집/유로폼","0-7M",5877,"m2"]
["      거푸집공/거친마감","0-7m",560,"㎡"]
["      조인트/스티로폴","T=20mm",45,"㎡"]
["     다) U형측구","500×500(L=1188.35m)",0,""]
["      무근콘크리트타설","다짐포함",380,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",119,"㎥"]
["      거푸집/유로폼","0-7M",3090,"m2"]
["      거푸집공/거친마감","0-7m",238,"㎡"]
["      조인트/스티로폴","T=20mm",25,"㎡"]
["     라) U형측구","600×600(L=959.71m)",0,""]
["      무근콘크리트타설","다짐포함",355,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",106,"㎥"]
["      거푸집/유로폼","0-7M",2879,"m2"]
["      거푸집공/거친마감","0-7m",192,"㎡"]
["      조인트/스티로폴","T=20mm",24,"㎡"]
["     마) U형측구","700×700(L=706.15m)",0,""]
["      철근콘크리트타설","다짐포함",297,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",85,"㎥"]
["      거푸집/유로폼","0-7M",2401,"m2"]
["      거푸집공/거친마감","0-7m",141,"㎡"]
["      조인트/스티로폴","T=20mm",20,"㎡"]
["      철근가공조립","간단",19.419,"Ton"]
["     바) U형측구","800×800(L=55.63m)",0,""]
["      철근콘크리트타설","다짐포함",26,"㎥"]
["      무근콘크리트타설","빈배합(leanmix)",7,"㎥"]
["      거푸집/유로폼","0-7M",211,"m2"]
["      거푸집공/거친마감","0-7m",11,"㎡"]
["      조인트/스티로폴","T=20mm",2,"㎡"]
["      철근가공조립","간단",1.7909999999999999,"Ton"]
["    2) 산마루측구","",0,""]
["     가) 무근콘크리트타설","다짐포함",484,"㎥"]
["     나) 거푸집/유로폼","0-7M",2966,"m2"]
["     다) 철근가공조립","간단",1.62,"Ton"]
["     라) 조인트/스티로폴","T=20mm",32,"㎡"]
["    3) 소단측구","",0,""]
["     가) U형 플륨 설치","50~150KG미만/개",163,"M"]
["    4) 도수로","",0,""]
["     가) 무근콘크리트타설","다짐포함",15,"㎥"]
["     나) 철근콘크리트타설","다짐포함",17,"㎥"]
["     다) 거푸집/유로폼","0-7M",223,"m2"]
["     라) 철근가공조립","간단",0.83299999999999996,"Ton"]
["    5) 외부유입수 처리시설","",0,""]
["     가) 철근콘크리트타설","다짐포함",12,"㎥"]
["     나) 거푸집/유로폼","0-7M",62,"m2"]
["     다) 철근가공조립","간단",0.36799999999999999,"Ton"]
["    6) 침투측구","",0,""]
["     가) 침투측구","400×400(L=66.31m)",0,""]
["      무근콘크리트타설","다짐포함",15,"㎥"]
["      거푸집/유로폼","0-7M",128,"m2"]
["      부직포 설치","200g/mm²",146,"㎡"]
["      배수파이프","P.V.C. ø50mm",36,"M"]
["      모래 부설 및 다짐","",7,"㎥"]
["      기초잡석부설,다짐,운반","80mm이하",23,"㎥"]
["      골재선별및생산(발파암)","보통암,골재,Ø80mm이하",24,"㎥"]
["      조인트/스티로폴","T=20mm",1,"m2"]
["     나) 침투측구","500×500(L=36.96m)",0,""]
["      무근콘크리트타설","다짐포함",11,"㎥"]
["      거푸집/유로폼","0-7M",90,"m2"]
["      부직포 설치","200g/mm²",89,"㎡"]
["      배수파이프","P.V.C. ø50mm",27,"M"]
["      모래(석분) 부설 및 다짐","",4,"㎥"]
["      기초잡석부설,다짐,운반","80mm이하",15,"㎥"]
["      골재선별및생산(발파암)","보통암,골재,Ø80mm이하",15,"㎥"]
["      조인트/스티로폴","T=20mm",1,"m2"]
["     다) 침투측구","600×600(L=70.51m)",0,""]
["      무근콘크리트타설","다짐포함",25,"㎥"]
["      거푸집/유로폼","0-7M",200,"m2"]
["      부직포 설치","200g/mm²",176,"㎡"]
["      배수파이프","P.V.C. ø50mm",51,"M"]
["      모래(석분) 부설 및 다짐","",8,"㎥"]
["      기초잡석부설,다짐,운반","80mm이하",30,"㎥"]
["      골재선별및생산(발파암)","보통암,골재,Ø80mm이하",32,"㎥"]
["      조인트/스티로폴","T=20mm",1,"m2"]
["     라) 침투측구","800×800(L=41.68m)",0,""]
["      철근콘크리트타설","다짐포함",19,"㎥"]
["      거푸집/유로폼","0-7M",152,"m2"]
["      부직포 설치","200g/mm²",113,"㎡"]
["      배수파이프","P.V.C. ø50mm",30,"M"]
["      모래 부설 및 다짐","",6,"㎥"]
["      기초잡석부설,다짐,운반","80mm이하",22,"㎥"]
["      골재선별및생산(발파암)","보통암,골재,Ø80mm이하",22,"㎥"]
["      조인트/스티로폴","T=20mm",1,"m2"]
["      철근가공조립","간단",1.2709999999999999,"Ton"]
["   아. 초기우수처리시설","",0,""]
["    1) 송방천-O방류부","",0,""]
["     가) 초기우수처리장치-SBO유역","처리면적: ha",1,"sum"]
["     나) 초기우수처리장치-SBF유역","처리면적: ha",1,"sum"]
["     다) 철근콘크리트타설","다짐포함",1,"㎥"]
["     라) 무근콘크리트타설","빈배합(leanmix)",15,"㎥"]
["     마) 거푸집공/보통마감","0-7m",2,"㎡"]
["     바) 거푸집공/거친마감","0-7m",7,"㎡"]
["     사) 철근가공조립","간단",1.6E-2,"Ton"]
["     아) 세트앙카설치","M16(5/8\")",25,"nr"]
["     자) 기초잡석부설,다짐,운반","80mm이하",46.3,"㎥"]
["   자. 골재선별및생산","",0,""]
["    1) 골재선별및생산(발파암)","보통암,골재, Ø100mm이하",858,"㎥"]
["    2) 골재선별및생산(발파암)","보통암,골재,Ø40mm이하",106,"㎥"]
["   차. 주요자재 구입","",0,""]
["    1) 철근","",0,""]
["     가) 고철","중량A",8.3640000000000008,"Ton"]
["    2) 시멘트","",0,""]
["     가) 시멘트","40kg/포",339,"포"]
["    3) 모래 및 석분","",0,""]
["     가) 석분","",5724,"㎥"]
["     나) 모래","",19,"㎥"]
["    4) 골재","",0,""]
["     가) 자갈","Ø25mm",10,"㎥"]
["    5) U형 플륨관","",0,""]
["     가) 철근콘크리트플륨관","300×300",163,"M"]
["   카. 주요자재 운반","",0,""]
["    1) 철근운반","",0,""]
["     가) 철근운반","L=10.00km(하치장-현장)",287.14600000000002,"Ton"]
["    2) 시멘트운반","",0,""]
["     가) 시멘트운반","40kg/포,L=10km(하치장-현장)",339,"포"]
["  ","",0,""]
["  4. 오수공사","",0,""]
["   가. 토공","",0,""]
["    1) 터파기","",0,""]
["     가) 토사","",0,""]
["      터파기/육상토사","0-4m 기계",13998,"M3"]
["     나) 풍화암","",0,""]
["      터파기/육상리핑암","0-4m,기계",3772,"m3"]
["     다) 연암","",0,""]
["      터파기/육상발파암","0-4m,기계",508,"m3"]
["     라) 보통암","",0,""]
["      터파기/육상발파암","0-4m 기계",1105,"m3"]
["    2) 되메우기","",0,""]
["     가) 되메우기/토사(기계100%)","기계(관상단)",16330,"㎥"]
["     나) 되메우기/토사(인력30%)","다짐",1141,"m3"]
["    3) 잔토처리","",0,""]
["     가) 잔토처리","리핑암",3772,"㎥"]
["     나) 잔토처리","발파암(연암)",508,"㎥"]
["     다) 잔토처리","발파암(보통암)",1105,"㎥"]
["   나. 관로접합 및 부설","",0,""]
["    1) 고강도 PE삼중벽관","",0,""]
["     가) 고강도PE삼중벽관 접합 및 부설","D150mm, PE조임소켓",120,"M"]
["     나) 고강도PE삼중벽관 접합 및 부설","D300mm, PE조임소켓",2039,"M"]
["    2) 고강성 PVC이중벽관","",0,""]
["     가) 고강성PVC이중벽관 접합 및 부설","D150mm",1815,"M"]
["     나) 고강성PVC이중벽관 접합 및 부설","D200mm",2770,"M"]
["     다) 고강성PVC이중벽관 접합 및 부설","D300mm",985,"M"]
["    2) 관기초","",0,""]
["     가) 모래(석분)기초","",0,""]
["      모래(석분)기초부설","",1774,"㎥"]
["    3) 관절단","",0,""]
["     가) 고강성 PE삼중벽관","",0,""]
["      고강성PE삼중벽관 절단","D150MM",7,"nr"]
["      고강성PE삼중벽관 절단","D300MM",57,"nr"]
["     나) 고강성 PVC이중벽관","",0,""]
["      고강성 PVC이중벽관 절단","D150MM",326,"nr"]
["      고강성 PVC이중벽관 절단","D200MM",296,"nr"]
["      고강성 PVC이중벽관 절단","D300MM",84,"nr"]
["    4) 이경티 접합 및 부설","",0,""]
["     가) 고강성 PE삼중벽관","",0,""]
["      PE삼중벽관 이경티 접합 및 부설","D150mm, PE조임소켓",6,"nr"]
["      PE삼중벽관 이경티 접합 및 부설","D300mm, PE조임소켓",12,"nr"]
["     나) 고강성 PVC이중벽관","",0,""]
["      PVC이중벽관 이경티 접합 및 부설","D200mmxD150mm",234,"nr"]
["      PVC이중벽관 이경티 접합 및 부설","D300mmxD150mm",64,"nr"]
["   다. 오수맨홀","",0,""]
["    1) 오수맨홀(차도측)","",0,""]
["     가) 원형1호맨홀(오수,차도)","",0,""]
["      철근콘크리트타설","다짐포함",17,"㎥"]
["      무근콘크리트타설","소형구조물",144,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",5.68,"㎥"]
["      모르터(1:2),(토목,조경)","1:2",1.68,"㎥"]
["      거푸집공/보통마감","0-7m",28,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",80,"nr"]
["      원형맨홀 벽체(강재거푸집)","원형맨홀1호(φ900mm)오염방지",142,"M"]
["      강재거푸집(D=3m)","0-7m",58,"M2"]
["      맨홀발디딤쇠","PE코팅ø22mm",320,"개소"]
["      강관동바리","암거용(3개월)",50,"공/㎥"]
["      스페이셔","슬라브 및 기초",83,"m2"]
["      철근가공조립","보통",2.3199999999999998,"Ton"]
["      하수맨홀 뚜껑및 받침대 설치","주철제(차도) D648MM",80,"조"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D150-200",134,"nr"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D250-400",33,"nr"]
["      지수링 설치","수퍼씰, 2005, 관스리브용",129,"M"]
["     나) 원형1호맨홀(오수,차도,보강)","",0,""]
["      철근콘크리트타설","다짐포함",1,"㎥"]
["      무근콘크리트타설","소형구조물",21,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",0.35499999999999998,"㎥"]
["      모르터(1:2),(토목,조경)","1:2",0.11,"㎥"]
["      거푸집공/보통마감","0-7m",2,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",5,"nr"]
["      원형맨홀 벽체(강재거푸집)","원형맨홀1호(φ900mm)오염방지",14,"M"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      맨홀발디딤쇠","PE코팅ø22mm",40,"개소"]
["      강관동바리","암거용(3개월)",5,"공/㎥"]
["      스페이셔","슬라브 및 기초",7,"m2"]
["      철근가공조립","보통",0.30499999999999999,"Ton"]
["      하수맨홀 뚜껑및 받침대 설치","주철제(차도) D648MM",5,"조"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D150-200",2,"nr"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D250-400",11,"nr"]
["      지수링 설치","수퍼씰, 2005, 관스리브용",13,"M"]
["    2) 오수맨홀(보도측)","",0,""]
["     가) 원형1호맨홀(오수,보도)","",0,""]
["      철근콘크리트타설","다짐포함",5,"㎥"]
["      무근콘크리트타설","소형구조물",52,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",0.55200000000000005,"㎥"]
["      모르터(1:2),(토목,조경)","1:2",0.52800000000000002,"㎥"]
["      거푸집공/보통마감","0-7m",8,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",24,"nr"]
["      원형맨홀 벽체(강재거푸집)","원형맨홀1호(φ900mm)오염방지",55,"M"]
["      강재거푸집(D=3m)","0-7m",10,"㎡"]
["      맨홀발디딤쇠","PE코팅ø22mm",144,"개소"]
["      강관동바리","암거용(3개월)",20,"공/㎥"]
["      스페이셔","슬라브 및 기초",25,"m2"]
["      철근가공조립","보통",0.69599999999999995,"Ton"]
["      하수맨홀 뚜껑및 받침대 설치","디자인(보도용), D648",24,"조"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D150-200",11,"nr"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D250-400",46,"nr"]
["      지수링 설치","수퍼씰, 2005, 관스리브용",56,"M"]
["     나) 원형1호맨홀(오수,보도,보강)","",0,""]
["      철근콘크리트타설","다짐포함",7,"㎥"]
["      무근콘크리트타설","소형구조물",97,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",0.50600000000000001,"㎥"]
["      모르터(1:2),(토목,조경)","1:2",0.48399999999999999,"㎥"]
["      거푸집공/보통마감","0-7m",8,"㎡"]
["      합성수지(PE)원형맨홀거푸집","기초및슬라브ø900mm",22,"nr"]
["      원형맨홀 벽체(강재거푸집)","원형맨홀1호(φ900mm)오염방지",68,"M"]
["      강재거푸집(D=3m)","0-7m",9,"M2"]
["      맨홀발디딤쇠","PE코팅ø22mm",176,"개소"]
["      강관동바리","암거용(3개월)",24,"공/㎥"]
["      스페이셔","슬라브 및 기초",33,"m2"]
["      철근가공조립","보통",0.72599999999999998,"Ton"]
["      하수맨홀 뚜껑및 받침대 설치","디자인(보도용), D648",22,"조"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D150-200",3,"nr"]
["      원형맨홀 반구형연결거푸집(강재+PE)","원형1호,연결관경D250-400",48,"nr"]
["      지수링 설치","수퍼씰, 2005, 관스리브용",53,"M"]
["   라. 부대공","",0,""]
["    1) 내부검사 및 수밀시험","",0,""]
["     가) 하수관거 내부검사","신설관",5794,"M"]
["     나) 하수관 수밀시험","Φ200mm",60,"개소"]
["     다) 하수관 수밀시험","Φ300mm",71,"개소"]
["    2) 오수관표시 및 분기표식","",0,""]
["     가) 오수관테이프설치","흑갈색, 200MM",11594,"M"]
["     나) 분기표식(표시못)","상,오수관용(D45×140)",333,"개소"]
["     다) 분기표식 ELP관","Ø80mm, H-1.5m",25,"nr"]
["    3) 인입관로 유도장치 통합맨홀","",0,""]
["     가) 인입관로 유도장치 통합맨홀","L1894xW551xH880",308,"nr"]
["    4) 관마개 설치","",0,""]
["     가) PVC관마개 설치","D150mm",326,"개"]
["     나) PE관마개 설치","D150mm",7,"개"]
["   마. 주요자재 구입","",0,""]
["    1) 고재","",0,""]
["     가) 고철","중량A",0.128,"Ton"]
["    2) 시 멘 트","40kg/포",111,"포"]
["    3) 모래 및 석분","",0,""]
["     가) 석분(기초용)","",1845,"㎥"]
["     나) 모래(콘크리트, 모르타르용)","강모래",6,"㎥"]
["    4) 골재","",0,""]
["     가) 자갈(잡석)","Ø25mm∼Ø40mm",4,"㎥"]
["    5) 인입관로 유도장치(통합맨홀)","L1894xW551xH880",308,"개"]
["    6) 관마개","",0,""]
["     가) PVC관 마개","D150mm",326,"개"]
["     나) PE관 마개","D150mm",7,"개"]
["    7) PVC이중벽관 고무링","",0,""]
["     가) PVC이중벽관 고무링","150MM",307,"EA"]
["     나) PVC이중벽관 고무링","200MM",482,"EA"]
["     다) PVC이중벽관 고무링","300MM",132,"EA"]
["   바. 주요자재 운반","",0,""]
["    1) 철근운반","L=10.00km(하치장-현장)",4.1689999999999996,"Ton"]
["    2) 시멘트운반","40kg/포,L=10km(하치장-현장)",111,"포"]
["  ","",0,""]
["  5. 상수공사","",0,""]
["   가. 토공","",0,""]
["    1) 터파기","",0,""]
["     가) 토사","",0,""]
["      터파기/육상토사","0-2m 기계",6126,"㎥"]
["     나) 풍화암","",0,""]
["      터파기/육상리핑암","0-2m,기계",1482,"m3"]
["     다) 연암","",0,""]
["      터파기/육상발파암","0-2m 기계",60,"m3"]
["     라) 보통암","",0,""]
["      터파기/육상발파암","0-2m 기계",58,"㎥"]
["    2) 되메우기","",0,""]
["     가) 다짐도95%","",0,""]
["      되메우기/토사(인력30%)","다짐",797,"m3"]
["      되메우기/토사(기계100%)","기계",5963,"㎥"]
["    3) 잔토처리","",0,""]
["     가) 잔토처리","리핑암",1482,"㎥"]
["     나) 잔토처리","발파암(연암)",60,"㎥"]
["     다) 잔토처리","발파암(보통암)",58,"㎥"]
["    4) 관기초","",0,""]
["     가) 모래부설 및 다짐","",723,"㎥"]
["   나. 관로접합 및 부설","",0,""]
["    1) 닥타일 주철관","",0,""]
["     가) 닥타일 주철관 부설","",0,""]
["      주철관(시멘트라이닝닥터일)","ø80mm,토사기초KP메카니컬접합",142,"m"]
["      주철관(시멘트라이닝닥터일)","ø100mm,토사기초KP메카니컬접합",4825,"m"]
["      주철관(시멘트라이닝닥터일)","ø150mm,토사기초KP메카니컬접합",118,"M"]
["      주철관(시멘트라이닝닥터일)","ø200mm,토사기초KP메카니컬접합",944,"m"]
["      주철관(시멘트라이닝닥터일)","ø250mm,토사기초KP메카니컬접합",85,"M"]
["      주철관(시멘트라이닝닥터일)","ø300mm,토사기초KP메카니컬접합",190,"m"]
["      주철관(시멘트라이닝닥터일)","ø350mm,토사기초KP메카니컬접합",487,"M"]
["      주철관(시멘트라이닝닥터일)","ø400mm,토사기초KP메카니컬접합",653,"m"]
["     나) 닥타일 주철관 KP메카니칼 접합","",0,""]
["      주철이형관 접합 및 부설","Φ80mm",50,"개소"]
["      주철이형관 접합 및 부설","Φ100mm",1185,"개소"]
["      주철이형관 접합 및 부설","Φ150mm",32,"개소"]
["      주철이형관 접합 및 부설","Φ200mm",216,"개소"]
["      주철이형관 접합 및 부설","Φ250mm",58,"개소"]
["      주철이형관 접합 및 부설","Φ300mm",44,"개소"]
["      주철이형관 접합 및 부설","Φ350mm",104,"개소"]
["      주철이형관 접합 및 부설","Φ400mm",148,"개소"]
["     다) 닥타일주철관 절단","",0,""]
["      주철관절단","ø80mm",12,"개소"]
["      주철관절단","ø100mm",115,"개소"]
["      주철관절단","ø150mm",7,"개소"]
["      주철관절단","ø200mm",20,"개소"]
["      주철관절단","ø250mm",13,"개소"]
["      주철관절단","ø300mm",3,"개소"]
["      주철관절단","ø350mm",8,"개소"]
["      주철관절단","ø400mm",12,"개소"]
["    2) 스테인레스 강관","",0,""]
["     가) 스테인레스 부설","",0,""]
["      스테인리스 강관부설","프레스접합,D=25mm",1231,"M"]
["      스테인리스 강관부설","프레스접합,D=50mm",153,"M"]
["     나) 주름마디 슬립인 조인트 접합","",0,""]
["      슬립인 조인트 접합","주름마디 스테인레스,D=25mm",930,"nr"]
["      슬립인 조인트 접합","주름마디 스테인레스,D=50mm",36,"nr"]
["   다. 밸브 부설","",0,""]
["    1) 게이트밸브","",0,""]
["     가) 게이트밸브(청동)","D25mm 10kg/cm2",310,"nr(개소)"]
["     나) 게이트밸브(청동)","D50mm 10kg/cm2",12,"nr(개소)"]
["    2) 소프트실 제수밸브","",0,""]
["     가) 주철제 게이트 제수밸브 부설및접합","관경 80mm",11,"기"]
["     나) 주철제 게이트 제수밸브 부설및접합","관경 100mm",121,"기"]
["     다) 주철제 게이트 제수밸브 부설및접합","관경 150mm",4,"기"]
["     라) 주철제 게이트 제수밸브 부설및접합","관경 200mm",13,"기"]
["     마) 주철제 게이트 제수밸브 부설및접합","관경 250mm",6,"기"]
["     바) 주철제 게이트 제수밸브 부설및접합","관경 350mm",1,"기"]
["    3) 버터플라이밸브","",0,""]
["     가) 주철제 버터플라이 제수밸브 부설및접합","관경 400mm",4,"기"]
["    4) 공기밸브","",0,""]
["     가) 급속공기변 부설(보수일체형)","관경 100mm",5,"기"]
["    5) 소화전","",0,""]
["     가) 승하강 소화전","D100mm",11,"개소"]
["    6) 관세척벨브","",0,""]
["     가) 표준형 세척밸브","",0,""]
["      표준형세척밸브","D100mm",39,"nr"]
["      표준형세척밸브","D150mm",1,"nr"]
["      표준형세척밸브","D200mm",2,"nr"]
["      표준형세척밸브","D350mm",2,"nr"]
["      표준형세척밸브","D400mm",6,"nr"]
["     나) 티분기형 관세척밸브","",0,""]
["      티분기형세척밸브","D100mmⅹD100mm",10,"nr"]
["      티분기형세척밸브","D150mmⅹD150mm",1,"nr"]
["      티분기형세척밸브","D200mmⅹD100mm",2,"nr"]
["   라. 변  실","",0,""]
["    1) 제수변보호통(중형변실)","",0,""]
["     가) 중형변실 설치","Φ80mm",11,"개소"]
["     나) 중형변실 설치","Φ100mm",14,"개소"]
["     다) 중형변실 설치","Φ200mm",6,"개소"]
["     라) 중형변실 설치","Φ250mm",5,"개소"]
["     마) 제수변 받침 콘크리트","",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",0.1,"㎥"]
["      거푸집공/거친마감","0-7m",3,"㎡"]
["     바) 벽돌쌓기","",0,""]
["      시멘트벽돌(1．0B 쌓기)","1층 소운반 / 3.6m 미만",22,"㎡"]
["    2) 구형변실 설치(점검구 포함)","",0,""]
["     가) 제수변실","2.5 x 2.0",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",8,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",8,"㎥"]
["      철근콘크리트타설","다짐포함",301,"㎥"]
["      무근콘크리트타설","소형구조물",36,"㎥"]
["      거푸집공/유로폼","0-7M",1273,"㎡"]
["      거푸집공/거친마감","0-7m",91,"㎡"]
["      강재거푸집(D=3m)","0-7m",77,"M2"]
["      철근가공조립","보통",46.44,"Ton"]
["      상수맨홀 뚜껑 및 받침대 설치","차도용",28,"조"]
["      상수맨홀 뚜껑 및 받침대 설치","보도용",2,"조"]
["      맨홀발디딤쇠","PE코팅ø22mm",180,"개소"]
["      잡석부설","50mm이하",1,"m3"]
["      강관동바리","암거용(3개월)",225,"공/㎥"]
["      스페이셔","벽체용",1138,"m2"]
["      스페이셔","슬라브 및 기초",451,"m2"]
["      모르터(1:2),(토목,조경)","1:2",4.0000000000000001E-3,"㎥"]
["      아스팔트코팅","2회",1219,"m2"]
["     나) 제수변실","3.0 x 2.0",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",1,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",1,"㎥"]
["      철근콘크리트타설","다짐포함",28,"㎥"]
["      무근콘크리트타설","소형구조물",3,"㎥"]
["      거푸집공/유로폼","0-7M",106,"㎡"]
["      거푸집공/거친마감","0-7m",7,"㎡"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      철근가공조립","보통",4.1219999999999999,"Ton"]
["      상수맨홀 뚜껑 및 받침대 설치","보도용",2,"조"]
["      맨홀발디딤쇠","PE코팅ø22mm",14,"개소"]
["      강관동바리","암거용(3개월)",21,"공/㎥"]
["      강관비계","3개월이하",80,"m2"]
["      스페이셔","벽체용",89,"m2"]
["      스페이셔","슬라브 및 기초",32,"m2"]
["      모르터(1:2),(토목,조경)","1:2",4.0000000000000001E-3,"㎥"]
["      아스팔트코팅","2회",96,"m2"]
["     다) 제수변실","3.0 x 3.0",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",4,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",4,"㎥"]
["      철근콘크리트타설","다짐포함",180,"㎥"]
["      무근콘크리트타설","소형구조물",18,"㎥"]
["      거푸집공/유로폼","0-7M",642,"㎡"]
["      거푸집공/거친마감","0-7m",40,"㎡"]
["      강재거푸집(D=3m)","0-7m",33,"M2"]
["      철근가공조립","보통",25.75,"Ton"]
["      상수맨홀 뚜껑 및 받침대 설치","차도용",10,"조"]
["      맨홀발디딤쇠","PE코팅ø22mm",70,"개소"]
["      잡석부설","50mm이하",1,"m3"]
["      강관동바리","암거용(3개월)",153,"공/㎥"]
["      강관비계","3개월이하",440,"m2"]
["      스페이셔","벽체용",516,"m2"]
["      스페이셔","슬라브 및 기초",223,"m2"]
["      아스팔트코팅","2회",577,"m2"]
["     라) 제수변실","4.0 x 3.0",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",1,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",1,"㎥"]
["      철근콘크리트타설","다짐포함",23,"㎥"]
["      무근콘크리트타설","소형구조물",3,"㎥"]
["      거푸집공/유로폼","0-7M",79,"㎡"]
["      거푸집공/거친마감","0-7m",5,"㎡"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      철근가공조립","보통",4.1529999999999996,"Ton"]
["      상수맨홀 뚜껑 및 받침대 설치","차도용",1,"조"]
["      맨홀발디딤쇠","PE코팅ø22mm",7,"개소"]
["      잡석부설","50mm이하",1,"m3"]
["      강관동바리","암거용(3개월)",22,"공/㎥"]
["      강관비계","3개월이하",51,"m2"]
["      스페이셔","벽체용",61,"m2"]
["      스페이셔","슬라브 및 기초",29,"m2"]
["      아스팔트코팅","2회",70,"m2"]
["     마) 제수변실","5.0 x 3.0",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",1,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",1,"㎥"]
["      철근콘크리트타설","다짐포함",27,"㎥"]
["      무근콘크리트타설","소형구조물",3,"㎥"]
["      거푸집공/유로폼","0-7M",87,"㎡"]
["      거푸집공/거친마감","0-7m",6,"㎡"]
["      강재거푸집(D=3m)","0-7m",4,"M2"]
["      철근가공조립","보통",6.0919999999999996,"Ton"]
["      상수맨홀 뚜껑 및 받침대 설치","차도용",1,"조"]
["      맨홀발디딤쇠","PE코팅ø22mm",7,"개소"]
["      강관동바리","암거용(3개월)",27,"공/㎥"]
["      강관비계","3개월이하",56,"m2"]
["      스페이셔","벽체용",62,"m2"]
["      스페이셔","슬라브 및 기초",39,"m2"]
["      아스팔트코팅","2회",79,"m2"]
["     바) 제수변실","6.0 x 3.0",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",1,"㎥"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",2,"㎥"]
["      철근콘크리트타설","다짐포함",123,"㎥"]
["      무근콘크리트타설","소형구조물",13,"㎥"]
["      거푸집공/유로폼","0-7M",393,"㎡"]
["      거푸집공/거친마감","0-7m",19,"㎡"]
["      강재거푸집(D=3m)","0-7m",12,"M2"]
["      철근가공조립","보통",35.588000000000001,"Ton"]
["      상수맨홀 뚜껑 및 받침대 설치","차도용",4,"조"]
["      맨홀발디딤쇠","PE코팅ø22mm",28,"개소"]
["      강관동바리","암거용(3개월)",130,"공/㎥"]
["      강관비계","3개월이하",240,"m2"]
["      스페이셔","벽체용",276,"m2"]
["      스페이셔","슬라브 및 기초",182,"m2"]
["      아스팔트코팅","2회",356,"m2"]
["    3) 공기변실","",0,""]
["     가) 인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",1,"㎥"]
["     나) 인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",1,"㎥"]
["     다) 철근콘크리트타설","다짐포함",20,"㎥"]
["     라) 무근콘크리트타설","소형구조물",3,"㎥"]
["     마) 거푸집공/유로폼","0-7M",111,"㎡"]
["     바) 거푸집공/거친마감","0-7m",8,"㎡"]
["     사) 강재거푸집(D=3m)","0-7m",3,"M2"]
["     아) 철근가공조립","보통",2.105,"Ton"]
["     자) 상수맨홀 뚜껑 및 받침대 설치","보도용",5,"조"]
["     차) 맨홀발디딤쇠","PE코팅ø22mm",30,"개소"]
["     카) 잡석부설","50mm이하",1,"m3"]
["     타) 강관동바리","암거용(3개월)",11,"공/㎥"]
["     파) 스페이셔","벽체용",105,"m2"]
["     하) 스페이셔","슬라브 및 기초",27,"m2"]
["     거) 모르터(1:2),(토목,조경)","1:2",0.01,"㎥"]
["     너) 아스팔트코팅","2회",108,"m2"]
["     더) 환기구 방충망설치","",0.4,"㎡"]
["    4) 이토변실","",0,""]
["     가) 인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",1,"㎥"]
["     나) 인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",1,"㎥"]
["     다) 철근콘크리트타설","다짐포함",16,"㎥"]
["     라) 무근콘크리트타설","소형구조물",2,"㎥"]
["     마) 거푸집공/유로폼","0-7M",89,"㎡"]
["     바) 거푸집공/거친마감","0-7m",6,"㎡"]
["     사) 강재거푸집(D=3m)","0-7m",5,"M2"]
["     아) 철근가공조립","보통",1.6839999999999999,"Ton"]
["     자) 상수맨홀 뚜껑 및 받침대 설치","차도용",3,"조"]
["     차) 상수맨홀 뚜껑 및 받침대 설치","보도용",1,"조"]
["     카) 맨홀발디딤쇠","PE코팅ø22mm",24,"개소"]
["     타) 강관동바리","암거용(3개월)",9,"공/㎥"]
["     파) 스페이셔","벽체용",84,"㎡"]
["     하) 스페이셔","슬라브 및 기초",22,"m2"]
["     거) 모르터(1:2),(토목,조경)","1:2",2E-3,"㎥"]
["     너) 아스팔트코팅","2회",87,"m2"]
["    5) 소화전 기초","",0,""]
["     가) 승하강 소화전","",0,""]
["      잡석부설","50mm이하",7,"m3"]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 40mm",1,"㎥"]
["      거푸집공/거친마감","0-7m",2,"㎡"]
["    6) 가압펌프장 설치","",0,""]
["     가) 가압펌프장","6.0 x 3.0",0,""]
["      인력비빔타설(소형구조물)(토목,조경)","B 배합, 25mm",1,"㎥"]
["      철근콘크리트타설","다짐포함",62,"M3"]
["      무근콘크리트타설","소형구조물",4,"M3"]
["      거푸집공/유로폼","0-7M",137,"㎡"]
["      거푸집공/거친마감","0-7m",12,"㎡"]
["      철근가공조립","보통",11.285,"Ton"]
["      가압장 뚜껑 설치","1.450x1.450m,스테인레스",1,"nr"]
["      환기구 방충망설치","#22, 0.18mm",0.1,"㎡"]
["      맨홀발디딤쇠","PE코팅ø22mm",5,"개소"]
["      강관동바리","암거용(3개월)",34,"공/㎥"]
["      강관비계","3개월이하",107,"m2"]
["      스페이셔","벽체용",112,"m2"]
["      스페이셔","슬라브 및 기초",55,"m2"]
["      수팽창 고무지수재","2010,시공죠인트Box연결부",21,"M"]
["      우레탄도막방수","바닥, 노출(T=3MM)",18,"m2"]
["      아스팔트코팅","2회",101,"m2"]
["      시멘트 액체방수","1종(시멘트,모래 제외)",56,"㎡"]
["     나) 가압장 제어반 기초","",0,""]
["      무근콘크리트타설","소형구조물",1,"㎥"]
["      거푸집공/거친마감","0-7m",3,"㎡"]
["      파상형경질폴리에틸렌전선관","D30mm",1,"M"]
["      파상형경질폴리에틸렌전선관","D50mm",1,"M"]
["      파상형경질폴리에틸렌전선관","D80mm",1,"M"]
["     다) 가압펌프","",0,""]
["      가압펌프설치공사(TM포함)","7.5HPx200Ax380Vx3ph",1,"개소"]
["   마. 부대공","",0,""]
["    1) 상수관로 테이프 및 분기관 표식","",0,""]
["     가) 분기표식(표시못)","상,오수관용(D45×140)",344,"개소"]
["     나) 관로표식(표시못)","상,오수관용(D45×90)",108,"개소"]
["     다) 관로표식(표시못)","상,오수관용(D45×140)",248,"개소"]
["     라) 분기표식ELP관","Φ=80m/m, H=1.5m",36,"개소"]
["     마) 상수관테이프설치","청색, 200MM",3279,"M"]
["    2) 이형관 보호공","",0,""]
["     가) 콘크리트(인력비빔)","B 배합, 40mm",31,"㎥"]
["     나) 거푸집공/거친마감","0-7m",175,"㎡"]
["    3) 새들접합","",0,""]
["     가) 단수 천공 분기점 분기","본관100mm,연결관25~30mm",310,"개소"]
["     나) 단수 천공 분기점 분기","본관100mm,연결관40~50mm",6,"개소"]
["     다) 단수 천공 분기점 분기","본관200mm,연결관40~50mm",6,"개소"]
["    4) 플랜지접합","",0,""]
["     가) 주철관이음쇠/플랜지접합","D=100mm",83,"개소"]
["     나) 주철관이음쇠/플랜지접합","D=125mm",1,"개소"]
["     다) 주철관이음쇠/플랜지접합","D=150mm",32,"개소"]
["     라) 주철관이음쇠/플랜지접합","D=200mm",3,"개소"]
["     마) 주철관이음쇠/플랜지접합","D=250mm",2,"개소"]
["     바) 주철관이음쇠/플랜지접합","D=350mm",3,"개소"]
["     사) 주철관이음쇠/플랜지접합","D=400mm",18,"개소"]
["    5) 나사접합","",0,""]
["     가) 스테인리스관/나사접합","D=25mm",930,"개소"]
["     나) 스테인리스관/나사접합","D=50mm",36,"개소"]
["    6) 제수변실 배수공","PVC VG1관",0,""]
["     가) 제수변 배수파이프 설치","D100mm(TS접합)",442,"M"]
["     나) PVC 파이프 절단","D100mm",43,"개소"]
["    7) 수압시험","",0,""]
["     가) 수압시험","",0,""]
["      수압시험","D=250mm",1,"회"]
["      수압시험","D=350mm",3,"회"]
["     나) 수압시험 플랜지접합 및 부설","",0,""]
["      플랜지 접합","D=250mm",2,"개소"]
["      플랜지 접합","D=350MM",6,"개소"]
["    8) 상수도 관로 퇴수 시험","",0,""]
["     가) 상수관로 퇴수시험","상수관로 퇴수시험용",221,"㎥"]
["   바. 주요자재 구입","",0,""]
["    1) 고재","",0,""]
["     가) 고철","중량A",4.1280000000000001,"Ton"]
["    2) 시 멘 트","40kg/포",529,"포"]
["    3) 모래 및 석분","",0,""]
["     가) 석분(기초용)","구입",752,"㎥"]
["     나) 모래(콘크리트, 모르타르용)","강모래",32,"㎥"]
["    4) 골재","",0,""]
["     가) 자갈","Ø25mm",8,"㎥"]
["     나) 자갈","Ø40mm",30,"㎥"]
["     다) 잡석","Ø50mm이하",9,"㎥"]
["    5) 승하강 소화전 부속","",0,""]
["     가) S형 EF단관","45도×100×375",11,"EA"]
["     나) 벽돌","190×90×57",3429,"매"]
["    6) 덕타일주철관","",0,""]
["     가) 수도용닥타일주철관(시멘트라이닝)","2종관,D 80mmⅹ6m",24,"본"]
["     나) 수도용닥타일주철관(시멘트라이닝)","2종관,D100mmⅹ6m",805,"본"]
["     다) 수도용닥타일주철관(시멘트라이닝)","2종관,D150mmⅹ6m",20,"본"]
["     라) 수도용닥타일주철관(시멘트라이닝)","2종관,D200mmⅹ6m",158,"본"]
["     마) 수도용닥타일주철관(시멘트라이닝)","2종관,D250mmⅹ6m",15,"본"]
["     바) 수도용닥타일주철관(시멘트라이닝)","2종관,D300mmⅹ6m",32,"본"]
["     사) 수도용닥타일주철관(시멘트라이닝)","2종관,D350mmⅹ6m",82,"본"]
["     아) 수도용닥타일주철관(시멘트라이닝)","2종관,D400mmⅹ6m",109,"본"]
["     자) 수도용닥타일주철관(에폭시분체도장)","D80mm∼D400mm",12608,"㎏"]
["    7) 스테인리스관","",0,""]
["     가) 스테인리스 강관","D25mm(STS304,K-TYPE)",1293,"M"]
["     나) 스테인리스 강관","D50mm(STS304,K-TYPE)",161,"M"]
["     다) 주름마디스테인레스분수전연결관","소켓일체형, D25mmⅹ700mm",326,"EA"]
["     라) 주름마디스테인레스분수전연결관","소켓일체형, D50mmⅹ1000mm",13,"EA"]
["     마) 소켓(STS304)","D25mm",326,"EA"]
["     바) 소켓(STS304)","D50mm",13,"EA"]
["     사) 밸브소켓(STS304)","D25mm",326,"EA"]
["     아) 밸브소켓(STS304)","D50mm",13,"EA"]
["     자) 플러그(STS304)","D25mm",326,"EA"]
["     차) 플러그(STS304)","D50mm",13,"EA"]
["    8) 새들붙이 분수전","",0,""]
["     가) 스테인리스새들분수전","D100mmⅹ25mm,주철관용",310,"EA"]
["     나) 스테인리스새들분수전","D100mmⅹ50mm,주철관용",6,"EA"]
["     다) 스테인리스새들분수전","D200mmⅹ50mm,주철관용",6,"EA"]
["    9) PVC관","",0,""]
["     가) P．V．C 파이프","VG1,KSM-3404 D100m/m",464,"m"]
["     나) P．V．C 파이프","VG1,KSM-3404 D150m/m",60,"m"]
["     다) P．V．C 파이프(VG2)","KS M 3404, D100m/m×3.1t×4m",5,"M"]
["     라) PVC 파이프 소켓","D100mm",93,"개"]
["    10) 밸브","",0,""]
["     가) 급속공기밸브(보수일체형)","D100mm",5,"EA"]
["     나) 게이트 밸브(청동)","10K,D25mm",310,"EA"]
["     다) 게이트 밸브(청동)","10K,D50mm",12,"EA"]
["     라) 세척밸브","",0,""]
["      표준형세척밸브","기본형,Φ100mm,닥타일",39,"EA"]
["      표준형세척밸브","기본형,Φ150mm,닥타일",1,"EA"]
["      표준형세척밸브","기본형,Φ200mm,닥타일",2,"EA"]
["      표준형세척밸브","기본형,Φ350mm,닥타일",2,"EA"]
["      표준형세척밸브","기본형,Φ400mm,닥타일",6,"EA"]
["      T분기형세척밸브(기본형)","닥타일,100mmⅹ100mm",10,"EA"]
["      T분기형세척밸브(기본형)","닥타일,150mmⅹ150mm",1,"EA"]
["      T분기형세척밸브(기본형)","닥타일,200mmⅹ100mm",2,"EA"]
["    11) 가압펌프","",0,""]
["     가) 상수도 가압펌프(스텐인레스)","7.5HPx200Ax380Vx3ph",2,"대"]
["   사. 주요자재 운반","",0,""]
["    1) 철근운반","L=10.00km(하치장-현장)",141.33600000000001,"Ton"]
["    2) 시멘트운반","40kg/포,L=10km(하치장-현장)",529,"포"]
["    3) 닥타일 주철관 운반","L=360KM(직관,이형관,접합부속)",1,"식"]
[" ","",0,""]
[" Ⅲ. 특수구조물","",0,""]
["  1. 송방천6교","합성형라멘교",0,""]
["   가. 토공","",0,""]
["    1) 터파기","",0,""]
["     가) 터파기/육상토사","0-4m 기계",561,"m3"]
["     나) 터파기/용수토사","0-4m 기계",1061,"m3"]
["     다) 터파기/용수리핑암","0-4m 기계",228,"m3"]
["     라) 터파기/용수발파암","0-4m 기계",84,"m3"]
["     마) 터파기/용수발파암","4-6m 기계",85,"㎥"]
["    2) 되메우기및 다짐공","기계",1634,"m3"]
["    3) 뒷채움 및 다짐공","SB-1,자재별산",1362,"M3"]
["    4) 직접잔토처리","",0,""]
["     가) 직접잔토처리","리핑암,L=0.7km",228,"㎥"]
["     나) 직접잔토처리","발파암, L=0.7km",170,"㎥"]
["    5) 부족토운반","",0,""]
["     가) 순성토운반","토사,L=1.0km,D/T15ton",223,"㎥"]
["    6) 물푸기","",281,"hr"]
["   나. 구조물공","",0,""]
["    1) 콘크리트 타설","",0,""]
["     가) 철근콘크리트타설/펌프카","슬럼프15(100m3이상/일)",2874,"m3"]
["     나) 무근콘크리트타설","빈배합(leanmix)",318,"m3"]
["    2) 거푸집","",0,""]
["     가) 거푸집/매끈한마감","0-7m",3323,"m2"]
["     나) 거푸집/매끈한마감","7m초과-10m이하",254,"m2"]
["     다) 거푸집/매끈한마감","10m초과-13m이하",150,"m2"]
["     라) 거푸집/매끈한마감","13m초과-16m이하",158,"m2"]
["     마) 거푸집/매끈한마감","16m초과~19m이하",271,"m2"]
["     바) 거푸집/매끈한마감","19m초과~22m이하",124,"㎡"]
["     사) 거푸집/보통마감","0-7m",318,"m2"]
["     아) 거푸집/거친마감","0-7m",36,"m2"]
["     자) 거푸집공/무늬거푸집","0-7m",81,"M2"]
["    3) 동바리","",0,""]
["     가) 강관동바리","교량용(3개월)",6383,"공m3"]
["     나) 목재동바리","4회",1119,"공m3"]
["     다) 목재동바리","4회(데크피니셔용)",55,"공m3"]
["     라) 강관동바리","수평연결재(3개월)",2596,"m2"]
["    4) 다웰바","",0,""]
["     가) 조인트/다웰바","접속슬라브 (D25×L600)",52,"개"]
["     나) 다웰바/신축이음부용","D32×L1000",48,"EA"]
["    5) 강관비계","",0,""]
["     가) 강관비계","3개월이하",2862,"m2"]
["     나) 비계발판","",1686,"M"]
["     다) 강관비계다리","3개월이하",282,"m"]
["    6) 스페이셔 설치","",0,""]
["     가) 스페이셔","벽체용",2227,"m2"]
["     나) 스페이셔","기초및슬라브",2341,"㎡"]
["    7) 아스팔트코팅","2회",738,"m2"]
["    8) 철근가공조립","",0,""]
["     가) 철근가공및조립","보통",17.623999999999999,"ton"]
["     나) 철근가공및조립","복잡",368.55200000000002,"ton"]
["    9) 조인트/스티로폼","",0,""]
["     가) 조인트/스티로폼","T=5mm",9,"m2"]
["     나) 조인트/스티로폼","T=20mm",13,"m2"]
["    10) 교량표면처리/슬라브양생","피막양생",932,"m2"]
["    11) 교면복합방수","",753,"M2"]
["    12) 교량표면처리/슬라브면고르기","데크피니셔",753,"m2"]
["    13) 교면포장","",0,""]
["     가) 아스콘포장/표층/포설및다짐","T=8cm",753,"㎡"]
["     나) 칼라아스콘포장","T=5.0cm,재료비별산",648,"㎡"]
["     다) 아스콘포장/택코팅","",0,""]
["      택코팅 구입","일반구간,30L/a",1507,"m2"]
["      아스콘포장/택코팅","RSC-4",1507,"㎡"]
["    14) NOTCH 설치","폴리에틸렌",101,"M"]
["    15) 교명주","",2,"NR"]
["    16) TBM 설치","황동주물",1,"nr"]
["    17) 전선관","P.V.C. ø100mm",161,"m"]
["    18) 난간","",0,""]
["     가) 보도용 난간","W2000*H1400",198,"M"]
["     나) 차량용 난간","W2000*H1400",161,"M"]
["    19) 합성라멘 구조물","",0,""]
["     가) 합성형 라멘 제작","",8,"본"]
["     나) Preflex Beam 운반 및 가설","",8,"주형"]
["     다) H 형강","300*300*10*15M/M",4.6449999999999996,"TON"]
["    20) 교면내부침투시설","Ø10",161,"M"]
["    21) 신구-콘크리트접합","-",15,"m2"]
["    22) 와이어메쉬","",0,""]
["     가) 구입","",0,""]
["      와이어메쉬","#6 Φ4.8 100X100",251,"M2"]
["      와이어메쉬","#10 Φ3.2 100X100",292,"M2"]
["     나) 설치","",0,""]
["      와이어메쉬 설치","",543,"m2"]
["    23) 교량배수시설","",0,""]
["     가) 교량배수시설","양방향",1,"식"]
["    24) 콘크리트양생","피막양생",377,"m2"]
["    25) 옹벽배수시설","",0,""]
["     가) 배수파이프","P.V.C. ø100mm",3,"m"]
["     나) 드레인보드설치","",161,"㎡"]
["     다) 부직포설치","",323,"M2"]
["    26) 시공이음면정리/콘크리트치핑","",20,"m2"]
["     머) 실런트","",37,"M"]
["      수축줄눈설치","면목",28,"M"]
["      수팽창 고무지수재","",37,"m"]
["    27) 말뚝기초","",0,""]
["     가) 강관말뚝,자재비","D=508mm,T=12mm",2016,"M"]
["     나) SDA+T4","D508mm",1888,"M"]
["     다) 강관말뚝두부보강","D508,D22*12EA",160,"본"]
["     라) 동재하시험","",4,"회"]
["     마) 정재하시험","",2,"회"]
["   다. 가도및축도","",0,""]
["    1) 흙쌓기 및 헐기","",3790,"m3"]
["    2) 파형강관부설","D800mm",60,"m"]
["    3) 파형강관철거","D=800mm,부설비의 50%",60,"M"]
["    4) 파형강관구입","6개월,손료30%",63,"ｍ"]
["    5) P．P 마대 쌓기 및 헐기","45 × 70cm",421,"m2"]
["   라. 자재운반","",0,""]
["    1) 철근 운반","L=10.00km(하치장-현장)",433.29899999999998,"Ton"]
["    2) 시멘트 운반","",1754,"대"]
["    3) 뒷채움재","골재생산유용,SB-2",6686,"㎥"]
["   마. 주요자재구입","",0,""]
["    1) 시멘트","40kg/포",6686,"대"]
["    2) 고철","",19.114999999999998,"Ton"]
[" ","",0,""]
[" Ⅳ. 가로수 조경공사","",0,""]
["  1. 가로수 식재공사","",0,""]
["   가. 식재공사","",0,""]
["    1) 소나무(조형)","H3.5ⅹW1.5ⅹR18",7,"주"]
["    2) 이팝나무","H4.0ⅹR15",649,"주"]
["    3) 백철쭉","H0.4ⅹW0.4",21790,"주"]
["    4) 자산홍","H0.4ⅹW0.4",14910,"주"]
["    5) 흰말채나무","H1.0ⅹW0.4",6890,"주"]
["   나. 식재부대공사","",0,""]
["    1) 삼발이지주목(중형)","ø70ⅹL2700",656,"Set"]
["    2) 유기질비료","20kg",20492,"㎏"]
["  ","",0,""]
["  2. 가로수 유지관리공사","",0,""]
["   가. 교목전정","준공후2회",131.19999999999999,"주"]
["   나. 관목전정","준공후2회",8718,"주"]
["   다. 교목 병충해방제 (기계)","준공후4회",131.19999999999999,"주"]
["   라. 관목 병충해방제 (기계)","준공후4회",21795,"주"]
["   마. 교목시비(준공후2회)","녹지내, H4.0이상",656,"주"]
["   바. 지주목재결속","준공후2회",328,"주"]
["   사. 관수(교목)","준공후4회",656,"주"]
["   아. 관수(관목)","준공후4회",4843,"주"]
["","",0,""]
["","",0,""]
["","",0,""]
["","",0,""]
["::","",0,""]
["*. 관급자재","",0,"",0,7252630757,0,7213676914,0,0,0,38953843]
[" Ⅰ. 도급자 설치 관급자재","",0,"",0,7252630757,0,7213676914,0,0,0,38953843]
["  1. 레미콘","",0,"",0,794812662,0,790543726,0,0,0,4268936]
["   가. 택지조성공사","",0,"",0,580024645,0,580024645,0,0,0,0]
["    1) 공통공사","",0,"",0,13436555,0,13436555,0,0,0,0]
["     가) 레미콘","25-16-08",8,"㎥",48345,386760,48345,386760,0,0,0,0]
["     나) 레미콘","25-18-08",136,"㎥",53155,7229080,53155,7229080,0,0,0,0]
["     다) 레미콘","25-18-12",50,"㎥",54664,2733200,54664,2733200,0,0,0,0]
["     라) 레미콘","25-21-12",53,"㎥",58255,3087515,58255,3087515,0,0,0,0]
["    2) 도로 및 포장공사","",0,"",0,115824745,0,115824745,0,0,0,0]
["     가) 레미콘","25-18-08",2179,"㎥",53155,115824745,53155,115824745,0,0,0,0]
["    3) 우수공사","",0,"",0,382261104,0,382261104,0,0,0,0]
["     가) 레미콘","25-24-12",1652,"㎥",60682,100246664,60682,100246664,0,0,0,0]
["     나) 레미콘","25-21-08",4210,"㎥",56491,237827110,56491,237827110,0,0,0,0]
["     다) 레미콘","25-16-08",914,"㎥",48345,44187330,48345,44187330,0,0,0,0]
["    4) 오수공사","",0,"",0,19748277,0,19748277,0,0,0,0]
["     가) 레미콘","25-21-08",327,"㎥",56491,18472557,56491,18472557,0,0,0,0]
["     나) 레미콘","25-18-08",24,"㎥",53155,1275720,53155,1275720,0,0,0,0]
["    5) 상수공사","",0,"",0,48753964,0,48753964,0,0,0,0]
["     가) 레미콘","25-21-08",784,"㎥",56491,44288944,56491,44288944,0,0,0,0]
["     나) 레미콘","25-18-08",84,"㎥",53155,4465020,53155,4465020,0,0,0,0]
["   나. 특수구조물","",0,"",0,210519081,0,210519081,0,0,0,0]
["    1) 송방천6교","",0,"",0,210519081,0,210519081,0,0,0,0]
["     가) 레미콘","25-40-15",129,"㎥",79691,10280139,79691,10280139,0,0,0,0]
["     나) 레미콘","25-27-15",2646,"㎥",62727,165975642,62727,165975642,0,0,0,0]
["     다) 레미콘","25-24-15",256,"㎥",60227,15418112,60227,15418112,0,0,0,0]
["     마) 레미콘","25-21-15",238,"㎥",59245,14100310,59245,14100310,0,0,0,0]
["     라) 레미콘","25-18-15",86,"㎥",55173,4744878,55173,4744878,0,0,0,0]
["   다. 조달수수료","재료비의",0.54,"%",790543726,4268936,0,0,0,0,790543726,4268936]
["  2. 아스팔트콘크리트","",0,"",0,1614224955,0,1605554959,0,0,0,8669996]
["   가. 택지조성공사","",0,"",0,1585085859,0,1585085859,0,0,0,0]
["    1) 공통공사","",0,"",0,10645803,0,10645803,0,0,0,0]
["     가) 아 스 콘(재생)","#78",189,"Ton",56327,10645803,56327,10645803,0,0,0,0]
["    2) 도로 및 포장공사","",0,"",0,1574440056,0,1574440056,0,0,0,0]
["     가) 아스콘","#78, 표층용",7051,"Ton",75100,529530100,75100,529530100,0,0,0,0]
["     나) 아스콘(중온 재생)","#67, 중간층용",3813,"Ton",56510,215472630,56510,215472630,0,0,0,0]
["     다) 아스콘(중온 재생)","#467, 기층용",13626,"Ton",44145,601519770,44145,601519770,0,0,0,0]
["     라) 아 스 콘 - 칼라","밀입도(13), #78,암적색",644,"Ton",135000,86940000,135000,86940000,0,0,0,0]
["     마) 아 스 콘 - 저소음","저소음포장",257,"Ton",130000,33410000,130000,33410000,0,0,0,0]
["     바) 중간층 첨가재","",35642,"㎏",3018,107567556,3018,107567556,0,0,0,0]
["   나. 특수구조물","",0,"",0,20469100,0,20469100,0,0,0,0]
["    1) 송방천6교","",0,"",0,20469100,0,20469100,0,0,0,0]
["     가) 중온 아스콘","#78, 표층용",141,"Ton",75100,10589100,75100,10589100,0,0,0,0]
["     나) 칼라투수아스콘","",76,"Ton",130000,9880000,130000,9880000,0,0,0,0]
["   다. 조달수수료","재료비의",0.54,"%",1605554959,8669996,0,0,0,0,1605554959,8669996]
["  3. 경하중 포장","",0,"",0,497946570,0,495272101,0,0,0,2674469]
["   가. 택지조성공사","",0,"",0,495272101,0,495272101,0,0,0,0]
["    1) 도로 및 포장공사","",0,"",0,495272101,0,495272101,0,0,0,0]
["     가) 소형고압블럭,U형","중간 황토색 T=6cm",2356,"㎡",8218,19361608,8218,19361608,0,0,0,0]
["     나) 소형고압블럭,U형","옅은 황토색 T=6cm",2356,"㎡",8218,19361608,8218,19361608,0,0,0,0]
["     다) 시각장애인용 점자블럭","",0,"",0,7774185,0,7774185,0,0,0,0]
["      장애자블럭(KS고강도콘크리트블럭)","점자블럭, 300×300×60",1376,"개",3545,4877920,3545,4877920,0,0,0,0]
["      장애자블럭(KS고강도콘크리트블럭)","유도블럭,300×300×60",817,"개",3545,2896265,3545,2896265,0,0,0,0]
["     라) 투수블록","",0,"",0,343134000,0,343134000,0,0,0,0]
["      투수블록","짙은 황토색 T=6cm",5225,"㎡",22000,114950000,22000,114950000,0,0,0,0]
["      투수블록","중간 황토색 T=6cm",5225,"㎡",22000,114950000,22000,114950000,0,0,0,0]
["      투수블록","옅은 황토색 T=6cm",5147,"㎡",22000,113234000,22000,113234000,0,0,0,0]
["     마) 투수성콘크리트","(자전거도로,보도용)",701,"㎥",150700,105640700,150700,105640700,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",495272101,2674469,0,0,0,0,495272101,2674469]
["  4. 보차도경계석(화강석)","",0,"",0,126695363,0,126014883,0,0,0,680480]
["   가. 택지조성공사","",0,"",0,126014883,0,126014883,0,0,0,0]
["    1) 도로 및 포장공사","",0,"",0,126014883,0,126014883,0,0,0,0]
["     가) 보차도경계석(화강석,직선)","200×250×1000",3832,"nr",18209,69776888,18209,69776888,0,0,0,0]
["     나) 보차도경계석(화강석,곡선)","200×250×1000",431,"nr",32909,14183779,32909,14183779,0,0,0,0]
["     다) 보차도경계석(화강석,직선)","180×200×1000",981,"nr",14345,14072445,14345,14072445,0,0,0,0]
["     라) 보차도경계석(화강석,곡선)","180×200×1000",434,"nr",26364,11441976,26364,11441976,0,0,0,0]
["     마) 보차도경계석,화강석(경사)","180×200~100×1000,직선",222,"nr",16200,3596400,16200,3596400,0,0,0,0]
["     바) 보차도경계석,낮춤경계석,화강석","180×100×1000,직선",250,"nr",8900,2225000,8900,2225000,0,0,0,0]
["     사) 보차도경계석,화강석(경사)","200×250~100×1000,직선",330,"nr",20400,6732000,20400,6732000,0,0,0,0]
["     아) 보차도도경계용,낮춤경계석(직선)","200×100×1000",371,"nr",10745,3986395,10745,3986395,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",126014883,680480,0,0,0,0,126014883,680480]
["  5. 도로경계석(블럭)","",0,"",0,90504599,0,90018500,0,0,0,486099]
["   가. 택지조성공사","",0,"",0,90018500,0,90018500,0,0,0,0]
["    1) 도로 및 포장공사","",0,"",0,90018500,0,90018500,0,0,0,0]
["     가) 도로경계블럭(콘크리트)","120×120×1000,직선",14446,"nr",3200,46227200,3200,46227200,0,0,0,0]
["     나) 보차도경계석(콘크리트)","150×170×200",8937,"M",4900,43791300,4900,43791300,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",90018500,486099,0,0,0,0,90018500,486099]
["  6. 파형강관 및 커플링밴드","",0,"",0,519668395,0,516877258,0,0,0,2791137]
["   가. 택지조성공사","",0,"",0,516877258,0,516877258,0,0,0,0]
["    1) 우수공사","",0,"",0,516877258,0,516877258,0,0,0,0]
["     가) PL 파형강관","D250mm,1.6T",5009,"M",24700,123722300,24700,123722300,0,0,0,0]
["     나) 파형강관(HPL)(1RS)","D450mm,1.6T",4798,"M",55909,268251382,55909,268251382,0,0,0,0]
["     다) 파형강관(HPL)(1RS)","D500mm,1.6T",256,"M",64000,16384000,64000,16384000,0,0,0,0]
["     라) 파형강관(HPL)(1RS)","D600mm,1.6T",383,"M",75082,28756406,75082,28756406,0,0,0,0]
["     마) 파형강관(PL) 연결자재","D=250",1174,"개",10291,12081634,10291,12081634,0,0,0,0]
["     바) 파형강관(PL) 연결자재","D=450",1274,"개",18155,23129470,18155,23129470,0,0,0,0]
["     사) 파형강관(PL) 연결자재","D=500",53,"개",20727,1098531,20727,1098531,0,0,0,0]
["     아) 파형강관(PL) 연결자재","D=600",101,"개",24327,2457027,24327,2457027,0,0,0,0]
["     자) 파형강관(HPL)-T형관","D450mm×D250mm",351,"EA",102182,35865882,102182,35865882,0,0,0,0]
["     차) 파형강관(HPL)-T형관","D500mm×D250mm",11,"EA",156570,1722270,156570,1722270,0,0,0,0]
["     카) 파형강관(HPL)-T형관","D600mm×D250mm",28,"EA",121727,3408356,121727,3408356,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",516877258,2791137,0,0,0,0,516877258,2791137]
["  7. PE2중피복 파형강관 및 커플링밴드","",0,"",0,976560770,0,971315666,0,0,0,5245104]
["   가. 택지조성공사","",0,"",0,971315666,0,971315666,0,0,0,0]
["    1) 우수공사","",0,"",0,971315666,0,971315666,0,0,0,0]
["     가) PE2중피복 파형강관(1RS)","D700mm,2.0T",859,"M",131100,112614900,131100,112614900,0,0,0,0]
["     나) PE2중피복 파형강관(1RS)","D800mm,2.0T",669,"M",155482,104017458,155482,104017458,0,0,0,0]
["     다) PE2중피복 파형강관(3RS)","D900mm,2.0T",342,"M",220691,75476322,220691,75476322,0,0,0,0]
["     라) PE2중피복 파형강관(3RS)","D1000mm,2.0T",58,"M",250709,14541122,250709,14541122,0,0,0,0]
["     마) PE2중피복 파형강관(3RS)","D1100mm,2.7T",254,"M",368627,93631258,368627,93631258,0,0,0,0]
["     바) PE2중피복 파형강관(3RS)","D1200mm,2.7T",969,"M",416200,403297800,416200,403297800,0,0,0,0]
["     사) PE2중피복 파형강관(3RS)","D1350mm,2.7T",82,"M",430055,35264510,430055,35264510,0,0,0,0]
["     아) PE2중피복 커플링밴드","D700mm",169,"개",35609,6017921,35609,6017921,0,0,0,0]
["     자) PE2중피복 커플링밴드","D800mm",156,"개",40391,6300996,40391,6300996,0,0,0,0]
["     차) PE2중피복 커플링밴드","D900mm",85,"개",44500,3782500,44500,3782500,0,0,0,0]
["     카) PE2중피복 커플링밴드","D1000mm",7,"개",54609,382263,54609,382263,0,0,0,0]
["     타) PE2중피복 커플링밴드","D1100mm",82,"개",59518,4880476,59518,4880476,0,0,0,0]
["     파) PE2중피복 커플링밴드","D1200mm",233,"개",70355,16392715,70355,16392715,0,0,0,0]
["     하) PE2중피복 커플링밴드","D1350mm",28,"개",74509,2086252,74509,2086252,0,0,0,0]
["     거) PE 2중피복 파형강관-T형관","D700mm×D250mm",33,"EA",238009,7854297,238009,7854297,0,0,0,0]
["     너) PE 2중피복 파형강관-T형관","D800mm×D250mm",38,"EA",299045,11363710,299045,11363710,0,0,0,0]
["     더) PE 2중피복 파형강관-T형관","D900mm×D250mm",22,"EA",400836,8818392,400836,8818392,0,0,0,0]
["     러) PE 2중피복 파형강관-T형관","D1100mm×D250mm",26,"EA",557309,14490034,557309,14490034,0,0,0,0]
["     머) PE 2중피복 파형강관-T형관","D1200mm×D250mm",59,"EA",726455,42860845,726455,42860845,0,0,0,0]
["     버) PE 2중피복 파형강관-T형관","D1350mmxD250mm",9,"EA",804655,7241895,804655,7241895,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",971315666,5245104,0,0,0,0,971315666,5245104]
["  8. 파형강관(평활형)(3RS) 및 플랜지","",0,"",0,286492746,0,284953995,0,0,0,1538751]
["   가. 택지조성공사","",0,"",0,284953995,0,284953995,0,0,0,0]
["    1) 우수공사","",0,"",0,284953995,0,284953995,0,0,0,0]
["     가) 파형강관(평활형)(3RS)","D1500mm,2.7T",290,"M",787000,228230000,787000,228230000,0,0,0,0]
["     나) 플랜지 연결자재(스텐)","D1500mm",55,"조",343909,18914995,343909,18914995,0,0,0,0]
["     다) 파형강관(평활형)-T형관","D1500mm×D250mm",10,"EA",3780900,37809000,3780900,37809000,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",284953995,1538751,0,0,0,0,284953995,1538751]
["  9. 조립식 PC 암거","",0,"",0,112363780,0,111760275,0,0,0,603505]
["   가. 택지조성공사","",0,"",0,111760275,0,111760275,0,0,0,0]
["    1) 우수공사","",0,"",0,111760275,0,111760275,0,0,0,0]
["     가) 조립식 PC 암거","1.5×1.8(H=1.0~3.0m)",219,"M",450545,98669355,450545,98669355,0,0,0,0]
["     나) 조립식 PC 암거 - 낙차부","1.5×2.3(H=1.0~3.0m)",24,"M",545455,13090920,545455,13090920,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",111760275,603505,0,0,0,0,111760275,603505]
["  10. 스틸그레이팅","",0,"",0,373925133,0,371916783,0,0,0,2008350]
["   가. 택지조성공사","",0,"",0,371916783,0,371916783,0,0,0,0]
["    1) 우수공사","",0,"",0,371916783,0,371916783,0,0,0,0]
["     가) 우수받이","",0,"",0,16565699,0,16565699,0,0,0,0]
["      스틸그레이팅-우수받이 1호","500×400×50",667,"개",16000,10672000,16000,10672000,0,0,0,0]
["      스틸그레이팅 받침-우수받이 1호","500×400×50",667,"개",8091,5396697,8091,5396697,0,0,0,0]
["      스틸그레이팅-우수받이 2호","1000×400×50",11,"개",32182,354002,32182,354002,0,0,0,0]
["      스틸그레이팅 받침-우수받이 2호","1000×400×50",11,"개",13000,143000,13000,143000,0,0,0,0]
["     나) 집수정","",0,"",0,12437055,0,12437055,0,0,0,0]
["      스틸그레이팅-집수정","400×400×50",67,"개",15909,1065903,15909,1065903,0,0,0,0]
["      스틸그레이팅 받침-집수정","400×400×50",67,"개",8182,548194,8182,548194,0,0,0,0]
["      스틸그레이팅-집수정","700×700×50",1,"개",35455,35455,35455,35455,0,0,0,0]
["      스틸그레이팅 받침-집수정","700×700×50",1,"개",9909,9909,9909,9909,0,0,0,0]
["      스틸그레이팅-집수정","1,000×1,000×50",95,"개",75091,7133645,75091,7133645,0,0,0,0]
["      스틸그레이팅 받침-집수정","1,000×1,000×50",95,"개",17455,1658225,17455,1658225,0,0,0,0]
["      스틸그레이팅-뚜껑 및 받침-집수정","1,700×1,700×50",9,"개",220636,1985724,220636,1985724,0,0,0,0]
["     다) 측구","",0,"",0,342618720,0,342618720,0,0,0,0]
["      스틸그레이팅","50×995×400",623,"개",29273,18237079,29273,18237079,0,0,0,0]
["      스틸그레이팅 받침","50×995×400",623,"개",12000,7476000,12000,7476000,0,0,0,0]
["      스틸그레이팅","50×995×500",2799,"개",35455,99238545,35455,99238545,0,0,0,0]
["      스틸그레이팅 받침","50×995×500",2799,"개",12182,34097418,12182,34097418,0,0,0,0]
["      스틸그레이팅","50×995×600",1189,"개",42273,50262597,42273,50262597,0,0,0,0]
["      스틸그레이팅 받침","50×995×600",1189,"개",13273,15781597,13273,15781597,0,0,0,0]
["      스틸그레이팅","50×995×700",960,"개",48909,46952640,48909,46952640,0,0,0,0]
["      스틸그레이팅 받침","50×995×700",960,"개",14727,14137920,14727,14137920,0,0,0,0]
["      스틸그레이팅","50×995×800",707,"개",58000,41006000,58000,41006000,0,0,0,0]
["      스틸그레이팅 받침","50×995×800",707,"개",15364,10862348,15364,10862348,0,0,0,0]
["      스틸그레이팅","50×995×900",56,"개",65091,3645096,65091,3645096,0,0,0,0]
["      스틸그레이팅 받침","50×995×900",56,"개",16455,921480,16455,921480,0,0,0,0]
["     라) 측구외부유입수 처리시설","",0,"",0,295309,0,295309,0,0,0,0]
["      스틸그레이팅","695×1390×50",2,"개",73636,147272,73636,147272,0,0,0,0]
["      스틸그레이팅 받침","695×1390×50",2,"개",18182,36364,18182,36364,0,0,0,0]
["      스틸그레이팅","1670×1280×50",1,"개",70909,70909,70909,70909,0,0,0,0]
["      스틸그레이팅 받침","1670×1280×50",1,"개",40764,40764,40764,40764,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",371916783,2008350,0,0,0,0,371916783,2008350]
["  11. 맨홀뚜껑","",0,"",0,106011047,0,105441663,0,0,0,569384]
["   가. 택지조성공사","",0,"",0,105441663,0,105441663,0,0,0,0]
["    1) 우수공사","",0,"",0,39812256,0,39812256,0,0,0,0]
["     가) 맨홀뚜껑(회주철)","φ648, 우수",137,"조",181818,24909066,181818,24909066,0,0,0,0]
["     나) 디자인맨홀 뚜껑(보도용)","φ648x95",45,"조",331182,14903190,331182,14903190,0,0,0,0]
["    2) 오수공사","",0,"",0,35054842,0,35054842,0,0,0,0]
["     가) 맨홀뚜껑(안전잠금장치)","φ648, 오수및우수",85,"조",233182,19820470,233182,19820470,0,0,0,0]
["     나) 디자인맨홀 뚜껑(보도용)","φ648x95",46,"조",331182,15234372,331182,15234372,0,0,0,0]
["    3) 상수공사","",0,"",0,30574565,0,30574565,0,0,0,0]
["     가) 맨홀뚜껑(구상흑연주철)","KS, φ918X135상수",4,"조",624728,2498912,624728,2498912,0,0,0,0]
["     나) 맨홀뚜껑(구상흑연주철)","KS, φ648X250상수",43,"조",383091,16472913,383091,16472913,0,0,0,0]
["     다) 디자인맨홀 뚜껑(보도용)","φ648x95",10,"조",331182,3311820,331182,3311820,0,0,0,0]
["     라) 제수변보호철개(2단)","Ø265ⅹ200",120,"EA",69091,8290920,69091,8290920,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",105441663,569384,0,0,0,0,105441663,569384]
["  12. 부직포","",0,"",0,12807388,0,12738600,0,0,0,68788]
["   가. 택지조성공사","",0,"",0,12738600,0,12738600,0,0,0,0]
["    1) 도로 및 포장공","",0,"",0,12393000,0,12393000,0,0,0,0]
["     가) 부직포","맹암거용",20655,"㎡",600,12393000,600,12393000,0,0,0,0]
["    2) 우수공사","",0,"",0,345600,0,345600,0,0,0,0]
["     가) 부직포","맹암거용",576,"㎡",600,345600,600,345600,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",12738600,68788,0,0,0,0,12738600,68788]
["  13. 경질폴리염화비닐관","",0,"",0,108864637,0,108279926,0,0,0,584711]
["   가. 택지조성공사","",0,"",0,108279926,0,108279926,0,0,0,0]
["    1) 오수공사","",0,"",0,108279926,0,108279926,0,0,0,0]
["     가) 고강성 PVC이중벽관","D150MM",1906,"M",9609,18314754,9609,18314754,0,0,0,0]
["     나) 고강성 PVC이중벽관","D200MM",2909,"M",16015,46587635,16015,46587635,0,0,0,0]
["     다) 고강성 PVC이중벽관","D300MM",1034,"M",28973,29958082,28973,29958082,0,0,0,0]
["     라) 고강성 PVC이중벽관 이경티","D200X150MM",241,"EA",35591,8577431,35591,8577431,0,0,0,0]
["     마) 고강성 PVC이중벽관 이경티","D300X150MM",66,"EA",73364,4842024,73364,4842024,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",108279926,584711,0,0,0,0,108279926,584711]
["  14. 폴리에틸렌관 및 관이음","",0,"",0,69797652,0,69422770,0,0,0,374882]
["   가. 택지조성공사","",0,"",0,69422770,0,69422770,0,0,0,0]
["    1) 오수공사","",0,"",0,69422770,0,69422770,0,0,0,0]
["     가) 고강도 PE삼중벽관","D150MM",124,"M",11545,1431580,11545,1431580,0,0,0,0]
["     나) 고강도 PE삼중벽관","D300MM",2100,"M",26485,55618500,26485,55618500,0,0,0,0]
["     다) PE조임소켓","D150MM",25,"EA",16500,412500,16500,412500,0,0,0,0]
["     라) PE조임소켓","D300MM",363,"EA",32120,11659560,32120,11659560,0,0,0,0]
["     마) PE삼중벽관 이경티","D300X150MM",6,"EA",50105,300630,50105,300630,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",69422770,374882,0,0,0,0,69422770,374882]
["  15. 난간","",0,"",0,371359755,0,369365184,0,0,0,1994571]
["   가. 택지조성공사","",0,"",0,178926624,0,178926624,0,0,0,0]
["    1) 도로 및 포장공사","",0,"",0,178926624,0,178926624,0,0,0,0]
["     가) 어린이 보호휀스","W2.1,H1.2",864,"M",207091,178926624,207091,178926624,0,0,0,0]
["   나. 특수구조물","",0,"",0,190438560,0,190438560,0,0,0,0]
["    1) 송방천6교","",0,"",0,190438560,0,190438560,0,0,0,0]
["     가) 보도용 난간","W2000*H1400",198,"M",522720,103498560,522720,103498560,0,0,0,0]
["     나) 차량용 난간","W2000*H1400",161,"M",540000,86940000,540000,86940000,0,0,0,0]
["   다. 조달수수료","재료비의",0.54,"%",369365184,1994571,0,0,0,0,369365184,1994571]
["  16. 상수도용 밸브","",0,"",0,63952661,0,63609172,0,0,0,343489]
["   가. 택지조성공사","",0,"",0,63609172,0,63609172,0,0,0,0]
["    1) 상수공사","",0,"",0,63609172,0,63609172,0,0,0,0]
["     가) 소프트실 제수밸브(비동력)","",0,"",0,52867352,0,52867352,0,0,0,0]
["      소프트실제수밸브","수도용,캡상승식,D80mm,980.7kPa",11,"EA",238455,2623005,238455,2623005,0,0,0,0]
["      소프트실제수밸브","수도용,캡상승식,D100mm,980.7kPa",121,"EA",270546,32736066,270546,32736066,0,0,0,0]
["      소프트실제수밸브","수도용,캡상승식,D150mm,980.7kPa",4,"EA",474728,1898912,474728,1898912,0,0,0,0]
["      소프트실제수밸브","수도용,캡상승식,D200mm,980.7kPa",13,"EA",647364,8415732,647364,8415732,0,0,0,0]
["      소프트실제수밸브","수도용,캡상승식,D250mm,980.7kPa",6,"EA",950000,5700000,950000,5700000,0,0,0,0]
["      소프트실제수밸브","수도용,캡상승식,D350mm,980.7kPa",1,"EA",1493637,1493637,1493637,1493637,0,0,0,0]
["     나) 소프트실 버터플라이밸브(수동)","",0,"",0,10741820,0,10741820,0,0,0,0]
["      버터플라이밸브","메탈,980kPa,D400mm, 수동",4,"EA",2685455,10741820,2685455,10741820,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",63609172,343489,0,0,0,0,63609172,343489]
["  17. 철근","",0,"",0,492959810,0,490312125,0,0,0,2647685]
["   가. 택지조성공사","",0,"",0,246028125,0,246028125,0,0,0,0]
["    1) 공통공사","",0,"",0,983267,0,983267,0,0,0,0]
["     가) 이형철근(SD30A)","D13m/m",1.744,"Ton",563800,983267,563800,983267,0,0,0,0]
["    2) 도로 및 포장공사","",0,"",0,1276587,0,1276587,0,0,0,0]
["     가) 이형철근(SD30A)","D13m/m",0.10199999999999999,"Ton",563800,57507,563800,57507,0,0,0,0]
["     나) 이형철근(SD30A)","D22m/m",1.3640000000000001,"Ton",558955,762414,558955,762414,0,0,0,0]
["     다) 이형철근(SD30A)","D29m/m",0.81699999999999995,"Ton",558955,456666,558955,456666,0,0,0,0]
["    3) 우수공사","",0,"",0,162287285,0,162287285,0,0,0,0]
["     가) 이형철근(SD30A)","D32m/m",0,"Ton",558955,0,558955,0,0,0,0,0]
["     나) 이형철근(SD30A)","D13m/m",96.361999999999995,"Ton",563800,54328895,563800,54328895,0,0,0,0]
["     다) 이형철근(SD30A)","D16m/m",12.976000000000001,"Ton",558955,7253000,558955,7253000,0,0,0,0]
["     라) 이형철근(SD30A)","D19m/m",13.343999999999999,"Ton",558955,7458695,558955,7458695,0,0,0,0]
["     마) 이형철근(SD30A)","H13m/m",107.38,"Ton",568655,61062173,568655,61062173,0,0,0,0]
["     바) 이형철근(SD30A)","H16m/m",50.201999999999998,"Ton",563800,28303887,563800,28303887,0,0,0,0]
["     사) 이형철근(SD30A)","H19m/m",6.883,"Ton",563800,3880635,563800,3880635,0,0,0,0]
["    4) 오수공사","",0,"",0,2339706,0,2339706,0,0,0,0]
["     가) 이형철근,(SD30A)","D13mm",1.9450000000000001,"Ton",563800,1096591,563800,1096591,0,0,0,0]
["     나) 이형철근,(SD30A)","D16mm",2.08,"Ton",558955,1162626,558955,1162626,0,0,0,0]
["     다) 이형철근,(SD30A)","D19mm",0.14399999999999999,"Ton",558955,80489,558955,80489,0,0,0,0]
["    5) 상수공사","",0,"",0,79141280,0,79141280,0,0,0,0]
["     가) 이형철근(SD30A)","D13mm",29.065000000000001,"Ton",563800,16386847,563800,16386847,0,0,0,0]
["     나) 이형철근(SD30A)","D16mm",60.36,"Ton",558955,33738523,558955,33738523,0,0,0,0]
["     다) 이형철근(SD300)","D19mm",15.589,"Ton",558955,8713549,558955,8713549,0,0,0,0]
["     라) 이형철근(SD300)","D22mm",7.9939999999999998,"Ton",558955,4468286,558955,4468286,0,0,0,0]
["     마) 이형철근(SD300)","D25mm",12.54,"Ton",558955,7009295,558955,7009295,0,0,0,0]
["     바) 이형철근(SD300)","D29mm",13.143000000000001,"Ton",558955,7346345,558955,7346345,0,0,0,0]
["     사) 이형철근(SD300)","D32mm",2.645,"Ton",558955,1478435,558955,1478435,0,0,0,0]
["   나. 특수구조물","",0,"",0,244284000,0,244284000,0,0,0,0]
["    1) 송방천6교","",0,"",0,244284000,0,244284000,0,0,0,0]
["     가) 이형철근(SD30A)","D13m/m",1.59,"Ton",563800,896442,563800,896442,0,0,0,0]
["     나) 이형철근(SD30A)","D16-32m/m",17.193999999999999,"Ton",558955,9610672,558955,9610672,0,0,0,0]
["     다) 이형철근(SD40)","H13m/m",15.103999999999999,"Ton",568655,8588965,568655,8588965,0,0,0,0]
["     라) 이형철근(SD40)","H16-32m/m",399.411,"Ton",563800,225187921,563800,225187921,0,0,0,0]
["   다. 조달수수료","재료비의",0.54,"%",490312125,2647685,0,0,0,0,490312125,2647685]
["  18. 유공관","",0,"",0,75198637,0,74794746,0,0,0,403891]
["   가. 택지조성공사","",0,"",0,74794746,0,74794746,0,0,0,0]
["    1) 도로 및 포장공사","",0,"",0,74794746,0,74794746,0,0,0,0]
["     가) P．E 유공관","200mm",5794,"M",12909,74794746,12909,74794746,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",74794746,403891,0,0,0,0,74794746,403891]
["  19. 교통안전표지판","",0,"",0,21633378,0,21517186,0,0,0,116192]
["   가. 택지조성공사","",0,"",0,21517186,0,21517186,0,0,0,0]
["    1) 도로 및 포장공사","",0,"",0,21517186,0,21517186,0,0,0,0]
["     가) 교통안전표지(원형)","ø600",14,"nr",47727,668178,47727,668178,0,0,0,0]
["     나) 교통안전표지(사각형)","600 x 600mm",16,"nr",46364,741824,46364,741824,0,0,0,0]
["     다) 교통안전표지판(주의표지)","2.0Tx900mm(변삼각)",15,"nr",50455,756825,50455,756825,0,0,0,0]
["     라) 표지판지주(교통표지용)","ø60.5,L=3.0m",58,"nr",30000,1740000,30000,1740000,0,0,0,0]
["     마) 교통안전표지판(갈매기표지)","450x600mm",13,"nr",70727,919451,70727,919451,0,0,0,0]
["     바) 교통안전표지(어린이보호구역)","3000 x 2000mm",3,"nr",1603636,4810908,1603636,4810908,0,0,0,0]
["     사) 표지판지주(편지식)","ø355.6,편지식",3,"nr",3960000,11880000,3960000,11880000,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",21517186,116192,0,0,0,0,21517186,116192]
["  20. 자전거보관소","",0,"",0,63724083,0,63381822,0,0,0,342261]
["   가. 택지조성공사","",0,"",0,63381822,0,63381822,0,0,0,0]
["    1) 도로 및 포장공","",0,"",0,63381822,0,63381822,0,0,0,0]
["     가) 자전거보관대","L7,800×W1,900×H2,615",14,"조",4527273,63381822,4527273,63381822,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",63381822,342261,0,0,0,0,63381822,342261]
["  21. 강판자재비","열연후판",0,"",0,319401076,0,317685574,0,0,0,1715502]
["   가. 특수구조물","",0,"",0,317685574,0,317685574,0,0,0,0]
["    1) 송방천6교","",0,"",0,317685574,0,317685574,0,0,0,0]
["     가) 열연후판(SM520)","12.0＜T≤ 20.0",119.432,"M/T",1221000,145826472,1221000,145826472,0,0,0,0]
["     다) 열연후판(SM520)","20.0＜T≤ 25.0",140.608,"M/T",1220000,171541760,1220000,171541760,0,0,0,0]
["     다) 열연후판(SS400)","12.0＜T≤ 20.0",2.3119999999999998,"M/T",1110,2566,1110,2566,0,0,0,0]
["     라) 열연후판(SM400)","20.0＜T≤ 30.0",0.28000000000000003,"M/T",1124200,314776,1124200,314776,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",317685574,1715502,0,0,0,0,317685574,1715502]
["  22. 소화전","",0,"",0,37601960,0,37400000,0,0,0,201960]
["   가. 택지조성공사","",0,"",0,37400000,0,37400000,0,0,0,0]
["    1) 상수공사","",0,"",0,37400000,0,37400000,0,0,0,0]
["     가) 승하강 소화전","100mm",11,"EA",3400000,37400000,3400000,37400000,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",37400000,201960,0,0,0,0,37400000,201960]
["  23. 차선도색","",0,"",0,116123700,0,115500000,0,0,0,623700]
["   가. 택지조성공사","",0,"",0,115500000,0,115500000,0,0,0,0]
["    1) 도로 및 포장공","",0,"",0,115500000,0,115500000,0,0,0,0]
["     가) 험프횡단보도","",0,"",0,5171250,0,5171250,0,0,0,0]
["      융착성도료","KSM-6080 백색",985,"㎏",5250,5171250,5250,5171250,0,0,0,0]
["     나) 고원식교차로","",0,"",0,3974250,0,3974250,0,0,0,0]
["      융착성도료","KSM-6080 백색",757,"㎏",5250,3974250,5250,3974250,0,0,0,0]
["     다) 과속방지턱","",0,"",0,6468000,0,6468000,0,0,0,0]
["      융착성도료","KSM-6080 황색",616,"㎏",5250,3234000,5250,3234000,0,0,0,0]
["      융착성도료","KSM-6080 백색",616,"㎏",5250,3234000,5250,3234000,0,0,0,0]
["     라) 차선도색","",0,"",0,99886500,0,99886500,0,0,0,0]
["      융착성도료","KSM-6080 황색",3938,"㎏",5250,20674500,5250,20674500,0,0,0,0]
["      융착성도료","KSM-6080 백색",15088,"㎏",5250,79212000,5250,79212000,0,0,0,0]
["   나. 조달수수료","재료비의",0.54,"%",115500000,623700,0,0,0,0,115500000,623700]
["","",0,"",0,0,0,0,0,0,0,0]
["","",0,"",0,0,0,0,0,0,0,0]
["::","",0,""]
["*. 시공상세도 작성","",0,""]
[" Ⅰ. 시공상세도 작성","",0,""]
["  1. 시공상세도작성","단순",2639,"장"]
["  2. 시공상세도작성","보통",392,"장"]
["  3. 시공상세도작성","복잡",52,"장"]