{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["허용공종"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":49,"defined_names":5621,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"허용공종","index":0,"n_rows":84,"n_cols":15,"rows_kept":84,"cut":false,"hidden":false,"merged":[[1,6,1,7],[1,8,1,9],[1,10,1,11],[1,12,2,12],[1,13,2,13],[1,14,2,14],[0,0,0,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,1,5]],"flags":["formulas_cached_only"]}
["물량내역수정입찰 허용공종"]
["공    종","규  격","수 량","단위","합    계",null,"재 료 비",null,"노 무 비",null,"경    비",null,"비  고","코  드-1","코  드-2"]
[{"$nulls":4},"단  가","금  액","단  가","금  액","단  가","금  액","단  가","금  액"]
["  4. 우수공사","",0,"",0,390054587,0,37865705,0,319671651,0,32517231,""]
["   나. 관로","",0,"",0,390054587,0,37865705,0,319671651,0,32517231,""]
["    1) 파형강관","",0,"",0,88545805,0,6705843,0,74850296,0,6989666,""]
["     가) D250mm","",0,"",0,7602400,0,977600,0,5605600,0,1019200,""]
["      파형강관접합 및 부설","D250mm",5200,"M",1462,7602400,188,977600,1078,5605600,196,1019200,"제  84호표","BIL0000014","IL0000014"]
["     나) D450mm","",0,"",0,24720289,0,2097282,0,20436306,0,2186701,""]
["      PL파형강관접합 및 부설","D450mm",8129,"M",3041,24720289,258,2097282,2514,20436306,269,2186701,"제  85호표","BIL0000013","IL0000013"]
["     다) D500mm","",0,"",0,2554524,0,210168,0,2125116,0,219240,""]
["      플랜지파형강관접합 및 부설","D=500mm",756,"M",3379,2554524,278,210168,2811,2125116,290,219240,"제  86호표","BIL0000406","IL0000406"]
["     라) D600mm","",0,"",0,8267350,0,608300,0,7025075,0,633975,""]
["      플랜지파형강관접합 및 부설","D=600mm",1975,"M",4186,8267350,308,608300,3557,7025075,321,633975,"제  87호표","BIL0000405","IL0000405"]
["     마) D700mm","",0,"",0,4243192,0,297888,0,3635432,0,309872,""]
["      플랜지파형강관접합 및 부설","D=700mm",856,"M",4957,4243192,348,297888,4247,3635432,362,309872,"제  88호표","BIL0000404","IL0000404"]
["     바) D800mm","",0,"",0,7013409,0,467883,0,6057090,0,488436,""]
["      플랜지파형강관접합 및 부설","D=800mm",1209,"M",5801,7013409,387,467883,5010,6057090,404,488436,"제  89호표","BIL0000403","IL0000403"]
["     사) D900mm","",0,"",0,3436633,0,223321,0,2980577,0,232735,""]
["      PE2중피복 파형강관접합 및 부설","D=900mm",523,"M",6571,3436633,427,223321,5699,2980577,445,232735,"제  90호표","BIL0000005","IL0000005"]
["     아) D1000mm","",0,"",0,5430208,0,336352,0,4743520,0,350336,""]
["      PE2중피복 파형강관접합 및 부설","D=1000mm",736,"M",7378,5430208,457,336352,6445,4743520,476,350336,"제  91호표","BIL0000007","IL0000007"]
["     자) D1100mm","",0,"",0,6503700,0,396606,0,5693730,0,413364,""]
["      PE2중피복 파형강관접합 및 부설","D=1100mm",798,"M",8150,6503700,497,396606,7135,5693730,518,413364,"제  92호표","BIL0000009","IL0000009"]
["     차) D1200mm","",0,"",0,7330110,0,437655,0,6436870,0,455585,""]
["      PE2중피복 파형강관접합 및 부설","D=1200mm",815,"M",8994,7330110,537,437655,7898,6436870,559,455585,"제  93호표","BIL0000008","IL0000008"]
["     카) D1350mm","",0,"",0,3028968,0,173456,0,2674656,0,180856,""]
["      PE2중피복 파형강관접합 및 부설","D=1350mm",296,"M",10233,3028968,586,173456,9036,2674656,611,180856,"제  94호표","BIL0000368","IL0000368"]
["     타) D1500mm","",0,"",0,8415022,0,479332,0,7436324,0,499366,""]
["      파형강관(평활형)접합 및 부설","D=1500mm",742,"M",11341,8415022,646,479332,10022,7436324,673,499366,"제  95호표","BIL0000367","IL0000367"]
["    3) 관기초","",0,"",0,177138368,0,0,0,177138368,0,0,""]
["     가) 모래(석분)기초","",0,"",0,177138368,0,0,0,177138368,0,0,""]
["      모래(석분)부설및다짐","석분(생산+구입)",11968,"㎥",14801,177138368,0,0,14801,177138368,0,0,"제  96호표","BIL0000141","IL0000141"]
["    4) 관거 내부조사 및 경고용테이프","",0,"",0,124370414,0,31159862,0,67682987,0,25527565,""]
["     가) 우수관경고용테이프","회색,10cm",25253,"M",439,11086067,195,4924335,244,6161732,0,0,"제  97호표","BIL0000259","IL0000259"]
["     나) 우수관식별용테이프","회색,10cm",25253,"M",439,11086067,195,4924335,244,6161732,0,0,"제  97호표","BIL0000259","IL0000259"]
["     다) 하수관거 내부조사","신설",13448,"M",3740,50295520,259,3483032,2711,36457528,770,10354960,"제  98호표","BIL0000412","IL0000412"]
["     라) 하수도기계준설","흡입준설기(25Ton)",735,"㎥",70616,51902760,24256,17828160,25717,18901995,20643,15172605,"산근  67호표","SK0000069","K0000069"]
["  5. 오수공사","",0,"",0,176092890,0,9965051,0,163398434,0,2729405,""]
["   나. 관로접합 및 부설","",0,"",0,176092890,0,9965051,0,163398434,0,2729405,""]
["    1) 고강성 다층벽관","",0,"",0,11212832,0,0,0,11212832,0,0,""]
["     가) 고강성다층벽관 접합 및 부설","D150mm, 삼각MS밴드",112,"M",3378,378336,0,0,3378,378336,0,0,"제 114호표","BIL0000063","IL0000063"]
["     나) 고강성다층벽관 접합 및 부설","D300mm, 삼각MS밴드",2624,"M",4129,10834496,0,0,4129,10834496,0,0,"제 115호표","BIL0000064","IL0000064"]
["    2) 고강성 PE삼중벽관","",0,"",0,34557561,0,0,0,34557561,0,0,""]
["     가) 고강도PE삼중벽관 접합 및 부설","D150mm, PE조임소켓",1515,"M",2992,4532880,0,0,2992,4532880,0,0,"제 116호표","BIL0000053","IL0000053"]
["     나) 고강도PE삼중벽관 접합 및 부설","D200mm, PE조임소켓",615,"M",3180,1955700,0,0,3180,1955700,0,0,"제 117호표","BIL0000052","IL0000052"]
["     다) 고강도PE삼중벽관 접합 및 부설","D300mm, PE조임소켓",7019,"M",3999,28068981,0,0,3999,28068981,0,0,"제 118호표","BIL0000051","IL0000051"]
["    3) 레진콘크리트관","",0,"",0,31271647,0,6618896,0,21923346,0,2729405,""]
["     가) 레진콘크리트관 접합 및 부설","D=300mm,콘크리트기초",478,"m",11564,5527592,2665,1273870,7979,3813962,920,439760,"ECGR040003000","ECGR040003000","CGR040003000"]
["     나) 레진콘크리트관 접합 및 부설","D=400mm,콘크리트기초",318,"m",11803,3753354,2574,818532,8262,2627316,967,307506,"ECGR040004000","ECGR040004000","CGR040004000"]
["     다) 레진콘크리트관 접합 및 부설","D=500mm,콘크리트기초",747,"m",17597,13144959,3688,2754936,12318,9201546,1591,1188477,"ECGR040005000","ECGR040005000","CGR040005000"]
["     라) 레진콘크리트관 접합 및 부설","D=600mm,콘크리트기초",502,"m",17621,8845742,3529,1771558,12511,6280522,1581,793662,"ECGR040006000","ECGR040006000","CGR040006000"]
["    4) 관기초","",0,"",0,85922712,0,3346155,0,82576557,0,0,""]
["     가) 모래기초","",0,"",0,73930995,0,0,0,73930995,0,0,""]
["      모래기초부설","강모래, 인력",4995,"㎥",14801,73930995,0,0,14801,73930995,0,0,"제  96호표","BIL0000141","IL0000141"]
["     나) 콘크리트 관기초","",0,"",0,11991717,0,3346155,0,8645562,0,0,""]
["      무근콘크리트타설","빈배합(leanmix)",180,"M3",22356,4024080,0,0,22356,4024080,0,0,"ECEC110110020","ECEC110110020","CEC110110020"]
["      거푸집공/거친마감","0-7m",549,"㎡",14513,7967637,6095,3346155,8418,4621482,0,0,"ECED100010000","ECED100010000","CED100010000"]
["    6) 이형관(이경티)설치","",0,"",0,13128138,0,0,0,13128138,0,0,""]
["     나) 고강성 PE삼중벽관","",0,"",0,13128138,0,0,0,13128138,0,0,""]
["      PE삼중벽관 이경티 접합 및 부설","D300mm, PE조임소켓",554,"nr",23697,13128138,0,0,23697,13128138,0,0,"제 132호표","BIL0000012","IL0000012"]
["  7. 구조물공사","",0,"",0,321048545,0,221896971,0,86000420,0,13151154,""]
["   가. 보강토옹벽","",0,"",0,195360045,0,96208471,0,86000420,0,13151154,""]
["    1) 블럭식보강토옹벽","",0,"",0,27312961,0,1612280,0,24172901,0,1527780,""]
["     나) 보강토옹벽","",0,"",0,27312961,0,1612280,0,24172901,0,1527780,""]
["      보강토 부설 및 다짐","",1270,"m3",4498,5712460,1159,1471930,2519,3199130,820,1041400,"ECCG110401000","ECCG110401000","CCG110401000"]
["      보강토블럭쌓기","표준형",332,"㎡",50325,16707900,0,0,48860,16221520,1465,486380,"제 246호표","BIL0000171","IL0000171"]
["      강봉보강재설치","TYPE-1",2807,"M",1743,4892601,50,140350,1693,4752251,0,0,"산근  81호표","SK0000078","K0000078"]
["    2) 산석형보강토옹벽","",0,"",0,162010469,0,93703130,0,57238896,0,11068443,""]
["     나) 보강사면(배면체)","",0,"",0,99652005,0,75239310,0,21911695,0,2501000,""]
["      보강토부설 및 다짐","",3050,"㎥",4498,13718900,1159,3534950,2519,7682950,820,2501000,"ECCG110401000","ECCG110401000","CCG110401000"]
["      거푸집/보통마감","0-7m",555,"m2",17565,9748575,7026,3899430,10539,5849145,0,0,"ECED200010000","ECED200010000","CED200010000"]
["      지오그리드설치","6T",6983,"m2",10910,76184530,9710,67804930,1200,8379600,0,0,"ECCG110310000","ECCG110310000","CCG110310000"]
["     다) 산석(전면체)","",0,"",0,62358464,0,18463820,0,35327201,0,8567443,""]
["      산석(전면체)쌓기","H=3.0m미만",75,"㎡",96680,7251000,31332,2349900,51507,3863025,13841,1038075,"제 248호표","BIL0000438","IL0000438"]
["      산석(전면체)쌓기","H=3.0~5.0m미만",136,"㎡",105325,14324200,32252,4386272,58474,7952464,14599,1985464,"제 249호표","BIL0000439","IL0000439"]
["      산석(전면체)쌓기","H=5.0~7.0m미만",344,"㎡",118556,40783264,34092,11727648,68348,23511712,16116,5543904,"제 250호표","BIL0000440","IL0000440"]
["    3) 연약지반처리","",0,"",0,6036615,0,893061,0,4588623,0,554931,""]
["     가) 기초치환공","1호 옹벽구간",0,"",0,6036615,0,893061,0,4588623,0,554931,""]
["      되메우기/토사","",1989,"m3",3035,6036615,449,893061,2307,4588623,279,554931,"ECDH110000000","ECDH110000000","CDH110000000"]
["   나. 주요자재 구입","",0,"",0,125688500,0,125688500,0,0,0,0,""]
["    1) 강봉보강재","",0,"",0,24573500,0,24573500,0,0,0,0,""]
["     가) 강봉보강재","TYPE-1",2891,"M",8500,24573500,8500,24573500,0,0,0,0,"MJAJAE0153","MJAJAE0153","JAJAE0153"]
["    2) 산석(조경석)","16목이상",749,"Ton",135000,101115000,135000,101115000,0,0,0,0,"M000-0310","M000-0310","000-0310"]