{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["내역서","공사원가(공)"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"내역서","index":0,"n_rows":901,"n_cols":13,"rows_kept":901,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,12,1,12],[0,4,0,5],[0,6,0,7],[0,8,0,9],[0,10,0,11]],"flags":["formulas_cached_only"]}
["공    종","규  격","수 량","단위","합    계",null,"재 료 비",null,"노 무 비",null,"경    비",null,"비  고"]
[{"$nulls":4},"단  가","금  액","단  가","금  액","단  가","금  액","단  가","금  액"]
["*. 순 공 사 비","",0,""]
[" 1. 토    공","",0,""]
["  1) 벌개제근","",120040,"㎡"]
["  2) 흙 깎 기","",0,""]
["   가. 흙깎기","토사(도쟈 32Ton)",138170,"㎥"]
["   나. 흙깍기","토사(백호 1.0㎥)",680002,"㎥"]
["   다. 흙깍기","풍화암(리퍼도쟈 32Ton)",189405,"㎥"]
["  3) 발 파","",0,""]
["   가. 일반발파","121-200 m",30581,"㎥"]
["   나. 대규모발파","200 m 이상",80883,"㎥"]
["  4) 흙 운 반","",0,""]
["   가. 유용무대","",60249,"㎥"]
["   나. 도쟈운반","",0,""]
["    가) 도쟈운반","토  사(L=23m)",88865,"㎥"]
["    나) 도쟈운반","리핑암(L=27m)",1980,"㎥"]
["   다. 덤프운반","",0,""]
["    가) 덤프운반(지구내)","토  사(L=275m)",652102,"㎥"]
["    나) 덤프운반(지구내)","리핑암(L=282m)",169600,"㎥"]
["    다) 덤프운반(지구내)","연  암(L=233m)",54522,"㎥"]
["    라) 덤프운반(유용토운반)","보통암(L=278m)",56662,"㎥"]
["  5) 비옥토운반","",0,""]
["   가. 비옥토 운반","발생지-야적지(L=271m)",30990,"㎥"]
["   나. 비옥토 운반","야적지-사용지(L=154m)",30990,"㎥"]
["   다. 비옥토 적치장 설치","",1,"식"]
["  6) 골재운반","",0,""]
["   가. 동상방지층운반","리핑암(L=169m),적치장",17705,"㎥"]
["   나. 동상방지층운반","리핑암(L=151m),사용처",17705,"㎥"]
["   다. 보통암운반","깬  돌(L=181m)",313,"㎥"]
["   라. 보통암운반","깬  돌(L=168m)",313,"㎥"]
["  7) 부설및다짐","",0,""]
["   가. 노상","95%다짐",22423,"㎥"]
["   나. 노체","90%다짐",136583,"㎥"]
["   다. 단지정지","토사",535973,"㎥"]
["   라. 단지정지","리핑암",172007,"㎥"]
["   마. 단지정지","발파암",113453,"㎥"]
["  8) 법면보호공","",0,""]
["   가. 줄떼","성토부",7324,"㎡"]
["   나. 자연표토복원공법","절토부",5067,"㎡"]
["   다. 깬돌쌓기","",1054,"㎡"]
["   라. 절토면고르기","리핑암",1062,"㎡"]
["   마. 절토면고르기","발파암",558,"㎡"]
["  9) 기존구조물철거","",0,""]
["   가. 철근콘크리트 깨기","T=30cm이상",257,"㎥"]
["   나. 철근콘크리트 깨기","T=30cm미만",226,"㎥"]
["   다. 무근콘크리트 깨기","T=30cm미만",1385,"㎥"]
["   라. 콘크리트포장절단","",12,"M"]
[" 10) 터파기","",0,""]
["   가. 인력터파기","토사(깊이 0∼1m)",41,"㎥"]
["   나. 기계터파기","토사(백호우1.0㎥)",4668,"㎥"]
["   다. 기계터파기","육상리핑",6,"㎥"]
["   라. 기계터파기","육상발파",33,"㎥"]
["   마.되메우기 및 다짐","백호우+콤팩터",2917,"㎥"]
["   바.되메우기 및 다짐","백호우+램머",428,"㎥"]
["  11) 규준틀설치","비탈규준틀",107,"개소"]
["  12) 임목폐기물처리","",475,"㎥"]
[" 2. 우 수 공","",0,""]
["  1) 토    공","",0,""]
["   가. 터 파 기","",0,""]
["    가) 터파기,토  사","인  력",2333,"㎥"]
["    나) 터파기,토  사","백호우1.0㎥",36421,"㎥"]
["    다) 터파기,리핑암","육상리핑",557,"㎥"]
["    라) 터파기,발파암","육상발파",821,"㎥"]
["   나. 되메우기","",0,""]
["    가) 되메우기","인력",1635,"㎥"]
["    나) 되메우기 및 다짐","백호우+콤팩터",9235,"㎥"]
["    다) 되메우기 및 다짐","백호우+램머",2253,"㎥"]
["    라) 흙쌓기,다짐도90%","노  체",23332,"㎥"]
["  2) 피복파형강관접합및부설","",0,""]
["   가. 피복파형강관 ","ø250mm,토사기초",1307,"M"]
["   나. 피복파형강관 ","ø450mm,토사기초",650,"M"]
["   다. 피복파형강관 ","ø450mm,모래기초",91,"M"]
["   라. 피복파형강관 ","ø500mm,토사기초",382,"M"]
["   마. 피복파형강관 ","ø600mm,토사기초",221,"M"]
["   바. 피복파형강관 ","ø700mm,토사기초",494,"M"]
["   사. 피복파형강관 ","ø700mm,모래기초",66,"M"]
["   아. 피복파형강관 ","ø800mm,토사기초",167,"M"]
["   자. 피복파형강관 ","ø900mm,토사기초",105,"M"]
["   차. 피복파형강관 ","ø900mm,모래기초",106,"M"]
["   카. 피복파형강관 ","ø1000mm,토사기초",392,"M"]
["   타. 피복파형강관 ","ø1100mm,토사기초",396,"M"]
["   파. 피복파형강관 ","ø1200mm,토사기초",100,"M"]
["  3) 파형강관T자관","",0,""]
["   가. 파형강관T자관","D450X250",64,"EA"]
["   나. 파형강관T자관","D500X250",24,"EA"]
["   다. 파형강관T자관","D600X250",26,"EA"]
["   라. 파형강관T자관","D700X250",55,"EA"]
["   마. 파형강관T자관","D800X250",20,"EA"]
["   바. 파형강관T자관","D900X250",12,"EA"]
["   사. 파형강관T자관","D1000X250",21,"EA"]
["   아. 파형강관T자관","D1100X250",7,"EA"]
["   자. 파형강관T자관","D1200X250",9,"EA"]
["  4) 하수관거 내부조사","CCTV",3114,"M"]
["  5) 경고용테이프","녹색,10cm",4672,"M"]
["  6) 암    거","",0,""]
["   가. 암    거","",0,""]
["    가) 콘크리트 타설","",0,""]
["      ㄱ. 콘크리트타설(철근)","100㎥이상/일,슬럼프15cm",3142,"㎥"]
["      ㄴ. 콘크리트타설(무근)","레미콘 일반타설",314,"㎥"]
["    나) 거 푸 집","",0,""]
["     ㄱ.거푸집,보통마감","합판4회(수직)",11506,"㎡"]
["     ㄴ. 거푸집,거친마감","합판6회(수직)",271,"㎡"]
["    다) 동바리,비계","",0,""]
["     ㄱ. 동바리,강재","암거구조물,3개월",3283,"공㎥"]
["     ㄴ. 강관비계","3개월",4139,"㎡"]
["    라) 시공이음면정리","(CHIPPING)",1534,"㎡"]
["    마) 다웰바 설치","D32 L=1000",715,"EA"]
["    바) 스페이셔","",0,""]
["     ㄱ. 스페이셔","T=100mm(슬래브용)",8836,"EA"]
["     ㄴ. 스페이셔","T=100mm(벽체용)",14087,"EA"]
["    사) 신축이음","T=20MM(스치로폴)",132,"m2"]
["    아) 봉합제"," ",481,"M"]
["    자) 지수판","",426,"M"]
["    차) 철근 및 보강재","",0,""]
["     ㄱ. 이형철근(연강)","복잡",352.675,"Ton"]
["     ㄴ. 이형철근(연강)","보통",0.611,"Ton"]
["     ㄷ. 이형철근(연강)","간단",4.983,"Ton"]
["   나. 암거날개벽","",0,""]
["    가) 콘크리트타설(철근)","레미콘펌프카,슬럼프15cm",104,"㎥"]
["    나) 콘크리트타설(무근)","레미콘 일반타설",33,"㎥"]
["    다) 콘크리트타설(무근)","레미콘 일반타설",10,"㎥"]
["    라) 거 푸 집","",0,""]
["     ㄱ. 거푸집,매끈한마감","합판3회(수직)",263,"m2"]
["     ㄴ. 거푸집,보통마감","합판4회(수직)",90,"㎡"]
["     ㄷ. 거푸집,거친마감","합판6회(수직)",12,"㎡"]
["    마) 철근및보강재(연강)","공칭직경13mm,복잡",8.701,"Ton"]
["    바) 강관비계","3개월",152,"㎡"]
["    사) 스페이셔","",0,""]
["     ㄱ. 스페이셔 설치","슬래브용",438,"EA"]
["     ㄴ. 스페이셔 설치","벽체용",191,"EA"]
["    아) 시공이음","",0,""]
["     ㄱ. 수팽창고무지수재","시공이음",64,"M"]
["     ㄴ. 수축줄눈"," ",62,"M"]
["    자) 드레인보드 설치","10㎜x1200㎜",56,"㎡"]
["  7) 우수맨홀","",0,""]
["   가. 우수맨홀(차도)","원형1호(D=900m/m)",15,"nr"]
["   나. 우수맨홀(차도)","원형2호(D=1200m/m)",14,"nr"]
["   다. 우수맨홀(차도)","특2호(1200×1200m/m)",10,"nr"]
["   라. 우수맨홀(차도)","특3호(1200×1400m/m)",5,"nr"]
["   마. 우수맨홀(차도)","특4호(1500×1500m/m)",1,"nr"]
["   바. 우수맨홀(차도)","암거맨홀(900×900m/m)",4,"nr"]
["   사. 우수맨홀(보도)","원형1호(D=900m/m)",5,"nr"]
["   아. 우수맨홀(보도)","특2호(1200×1200m/m)",2,"nr"]
["   자. 우수맨홀(보도)","특3호(1200×1400m/m)",7,"nr"]
["   차. 우수맨홀(보도)","암거맨홀(900×900m/m)",7,"nr"]
["  8) 우수받이","1호",233,"nr"]
["  9) 집 수 정","",0,""]
["   가. 집수정","0.9×0.9m",9,"nr"]
["   나. 집수정","1.5×1.5m",1,"nr"]
[" 10) 측    구","",0,""]
["   가. 산마루측구","TYPE A",592,"M"]
["   나. 산마루측구","TYPE B",500,"M"]
["   다. 도 수 로","0.8*0.5",34,"M"]
["   라. 측구수로","기성제품",473,"M"]
["   마. 벤치플륨관","기성제품",270,"M"]
[" 11) 원형관날개벽","",0,""]
["   가. 콘크리트타설(소형)","레미콘 일반타설",8,"㎥"]
["   나. 거푸집,보통마감","합판4회(수직)",39,"㎡"]
[" 12) P.P마대쌓기및헐기","45x70㎝",11370,"매"]
[" 3. 오 수 공","",0,""]
["  1) 토    공","",0,""]
["   가. 터 파 기","",0,""]
["    가) 터파기,토  사","인  력",148,"㎥"]
["    나) 터파기,토  사","백호우1.0㎥",12840,"㎥"]
["    다) 터파기,리핑암","육상리핑",199,"㎥"]
["    라) 터파기,발파암","육상발파",291,"㎥"]
["   나. 되메우기","",0,""]
["    가) 되메우기","인력",146,"㎥"]
["    나) 되메우기 및 다짐","백호우+콤팩터",11798,"㎥"]
["    다) 되메우기 및 다짐","백호우+램머",1077,"㎥"]
["  2) 유리섬유복합관","",0,""]
["   가. 복합관 접합 및 부설","ø400mm,토사기초",3050,"M"]
["   나. 복합관 접합 및 부설","ø400mm,모래기초90˚",99,"M"]
["   다. 유리섬유연결관","D150",215,"M"]
["  3) 유리섬유복합관절단","",0,""]
["   가. 복합관절단","400m/m",163,"nr"]
["   나. 복합관절단","150m/m",48,"nr"]
["   다. 오수맨홀","",0,""]
["    가) 오수맨홀(차도)","원형1호(D=900m/m)",9,"nr"]
["    나) 오수맨홀(보도)","원형1호(D=900m/m)",58,"nr"]
["    다) 오수맨홀(차도)","원형2호(D=1200m/m)",1,"nr"]
["    라) 오수맨홀(보도)","원형2호(D=1200m/m)",3,"nr"]
["   라. 오수관분기표식","",48,"nr"]
["   마. 분기표식ELP관","ø80mm",72,"nr"]
["   바. 오수관경고용테이프","흑갈색,10cm",5048,"M"]
["   사. 하수관 수밀시험","400m/m",35,"개소"]
["   아. 하수관거 내부조사","CCTV",3149,"M"]
[" 4. 상 수 공","",0,""]
["  1) 토    공","",0,""]
["   가. 터 파 기","",0,""]
["    가) 터파기,토  사","인  력",234,"㎥"]
["    나) 터파기,토  사","백호우1.0㎥",7970,"㎥"]
["    다) 터파기,리핑암","육상리핑",496,"㎥"]
["    라) 터파기,발파암","육상발파",894,"㎥"]
["   나. 되메우기","",0,""]
["    가) 되메우기","인력",233,"㎥"]
["    나) 되메우기 및 다짐","백호우+콤팩터",7947,"㎥"]
["    다) 되메우기 및 다짐","백호우+램머",720,"㎥"]
["  2) 에폭시피복강관접합및부설","",0,""]
["   가. 폴리에틸렌피복강관","ø80mm,토사기초",738,"M"]
["   나. 폴리에틸렌피복강관","ø100mm,토사기초",1981,"M"]
["   다. 폴리에틸렌피복강관","ø100mm,모래기초",74,"M"]
["   라. 폴리에틸렌피복강관","ø150mm,토사기초",526,"M"]
["   마. 폴리에틸렌피복강관","ø200mm,토사기초",373,"M"]
["   바. 폴리에틸렌피복강관","ø200mm,모래기초",3,"M"]
["   사. 폴리에틸렌피복강관","ø250mm,토사기초",308,"M"]
["   아. 폴리에틸렌피복강관","ø250mm,모래기초",118,"M"]
["   자. 폴리에틸렌피복강관","ø300mm,토사기초",981,"M"]
["   차. 폴리에틸렌피복강관","ø300mm,모래기초",129,"M"]
["   카. 폴리에틸렌피복강관","ø350mm,토사기초",147,"M"]
["   타. 폴리에틸렌피복강관","ø350mm,모래기초",92,"M"]
["  3)  플랜지접합","",0,""]
["   가. 플랜지 접합","80m/m",4,"개소"]
["   나. 플랜지 접합","100m/m",28,"개소"]
["  4)  변실접합","",0,""]
["   가. 제수변접합및부설","80m/m",10,"개소"]
["   나. 제수변접합및부설","100m/m",19,"개소"]
["   다. 제수변접합및부설","150m/m",2,"개소"]
["   라. 제수변접합및부설","250m/m",2,"개소"]
["  5) 에폭시피복강관절단","",0,""]
["   가.에폭시피복강관절단","80m/m",9,"개소"]
["   나.에폭시피복강관절단","100m/m",21,"개소"]
["   다.에폭시피복강관절단","150m/m",12,"개소"]
["   라.에폭시피복강관절단","200m/m",6,"개소"]
["   마.에폭시피복강관절단","250m/m",4,"개소"]
["   바.에폭시피복강관절단","300m/m",35,"개소"]
["   사.에폭시피복강관절단","350m/m",20,"개소"]
["  6) 에폭시피복강관이형관","",0,""]
["     1] 에폭시피복단관","D80X0.9M",6,"EA"]
["     2] 에폭시피복단관","D80X1.0M",7,"EA"]
["     3] 에폭시피복단관","D80X1.1M",6,"EA"]
["     4] 에폭시피복단관","D80X2.4M",1,"EA"]
["     5] 에폭시피복단관","D80X4.2M",1,"EA"]
["     6] 에폭시피복단관","D100X0.6M",1,"EA"]
["     7] 에폭시피복단관","D100X0.9M",8,"EA"]
["     8] 에폭시피복단관","D100X1.0M",11,"EA"]
["     9] 에폭시피복단관","D100X1.6M",3,"EA"]
["    10] 에폭시피복단관","D150X0.95M",2,"EA"]
["    11] 에폭시피복단관","D150X1.0M",2,"EA"]
["    12] 에폭시피복단관","D150X2.0M",1,"EA"]
["    13] 에폭시피복단관","D200X2.0M",1,"EA"]
["    14] 에폭시피복단관","D200X5.0M",1,"EA"]
["    15] 에폭시피복단관","D250X0.8M",4,"EA"]
["    16] 에폭시피복단관","D250X1.0M",6,"EA"]
["    17] 피복링1F레듀샤(B)","D350X250",1,"EA"]
["    18] 에폭시피복링엘보","D300X22.5",13,"EA"]
["    19] 에폭시피복링엘보","D300X11.25",3,"EA"]
["    20] 에폭시피복링엘보","D350X22.5",16,"EA"]
["    21] 에폭시피복직관","D150X6.0M",1,"EA"]
["    22] 피복홈1F티이(B)","D80X80",1,"EA"]
["    23] 피복홈1F티이(B)","D100X100",10,"EA"]
["    24] 피복홈1F티이(B)","D150X100",1,"EA"]
["    25] 피복홈1F티이(B)","D250X100",2,"EA"]
["    26] 피복홈2F티이(B)","D100X100",1,"EA"]
["    27] 에폭시피복홈레듀샤","D100X80",3,"EA"]
["    28] 에폭시피복홈레듀샤","D150X80",1,"EA"]
["    29] 에폭시피복홈레듀샤","D150X100",2,"EA"]
["    30] 에폭시피복홈레듀샤","D200X150",1,"EA"]
["    31] 에폭시피복홈레듀샤","D250X100",1,"EA"]
["    32] 에폭시피복홈레듀샤","D250X200",1,"EA"]
["    33] 에폭시피복홈레듀샤","D300X200",1,"EA"]
["    34] 에폭시피복홈엘보","D80X45",6,"EA"]
["    35] 에폭시피복홈엘보","D100X45",4,"EA"]
["    36] 에폭시피복홈엘보","D150X11.25",2,"EA"]
["    37] 에폭시피복홈엘보","D150X22.5",4,"EA"]
["    38] 에폭시피복홈엘보","D150X45",6,"EA"]
["    39] 에폭시피복홈엘보","D200X11.25",2,"EA"]
["    40] 에폭시피복홈엘보","D200X45",4,"EA"]
["    41] 에폭시피복홈엘보","D300X45",9,"EA"]
["    42] 에폭시피복홈엘보","D300X11.25",8,"EA"]
["    43] 에폭시피복홈티이","D80X80",2,"EA"]
["    44] 에폭시피복홈티이","D100X100",1,"EA"]
["    45] 에폭시피복홈티이","D150X80",1,"EA"]
["    46] 에폭시피복홈티이","D150X100",1,"EA"]
["    47] 에폭시피복홈티이","D250X250",1,"EA"]
["    48] 에폭시피복홈티이","D300X150",1,"EA"]
["    49] 피복홈플랜지아답터","D80",12,"EA"]
["    50] 피복홈플랜지아답터","D100",15,"EA"]
["    51] 피복홈플랜지아답터","D150",4,"EA"]
["    52] 피복홈플랜지아답터","D250",2,"EA"]
["    53] 피복홈플랜지아답터","D300",2,"EA"]
["    54] 홈엘보","D65X90",1,"EA"]
["    55] 소화전용곡관","D80",2,"EA"]
["    56] 소화전용곡관","D100",14,"EA"]
["    57] 소화전용단관","D80",1,"EA"]
["    58] 소화전용단관","D100",8,"EA"]
["    59] 소화전중간플랜지","D80",1,"EA"]
["    60] 소화전중간플랜지","D100",7,"EA"]
["  7) 내충격수도관 접합및부설","",0,""]
["   가. 내충격수도관부설접합","ø40mm",225,"M"]
["   나. 내충격수도관부설접합","ø65mm",38,"M"]
["   다. 내충격수도관부설접합","ø75mm",6,"M"]
["  8) 내충격수도관이형관","",0,""]
["      1] 내충격관새들접합","100×40m/m,내충격관용",45,"nr"]
["      2] 연결유니온","40m/m",45,"EA"]
["      3] 청동밸브","40m/m",45,"EA"]
["      4] HI-TS(90 엘보)","40m/m",90,"EA"]
["      5] HI-TS(벨브소켓)","40m/m",90,"EA"]
["      6] HI-3P(마감캡)","40m/m",45,"EA"]
["      7] HI-3P(단관)","40x0.2m/m",45,"EA"]
["      8] 홈1F티이(B)","D200X75",1,"EA"]
["      9] 홈1F티이(B)","D150X75",2,"EA"]
["     10] HI-3P(DF플랜지소켓)","75m/m",6,"EA"]
["     11] HI-3P(마감캡)","75m/m",3,"EA"]
["  9) 내충격수도관절단","",0,""]
["   가. 내충격수도관절단","40m/m",45,"개소"]
["   나. 충격격수도관절단","65m/m",2,"개소"]
["   다. 내충격수도관절단","75m/m",3,"개소"]
["  10) 밸    브","",0,""]
["   가. 소프트실제수밸브","수동식",0,""]
["    가) 소프트실제수밸브","80m/m,10k",7,"nr"]
["    나) 소프트실제수밸브","100m/m,10k",19,"nr"]
["    다) 소프트실제수밸브","150m/m,10k",2,"nr"]
["    라) 소프트실제수밸브","250m/m,10k",2,"nr"]
["   나. 공기밸브(쌍구형)","100m/m",1,"nr"]
["  11) 각종변실","",0,""]
["   가. 제수변실","3.0×3.0m",10,"nr"]
["   나. 공기변실","1.2×1.2m",1,"nr"]
["   다. 이토변실","1.2×1.2m",2,"nr"]
["   라. 제수변키보호통","1호",9,"nr"]
["  12) 상수부대시설","",0,""]
["   가. 지상식 소화전","",0,""]
["    가) 지상식 소화전","D80m/m",1,"개소"]
["    나) 지상식 소화전","D100m/m",7,"개소"]
["   나. 표  식","",0,""]
["    가) 상수관분기표식","",48,"EA"]
["    나) 분기표식ELP관","ø80mm",72,"nr"]
["   라. 이형관보호공","",0,""]
["    가) 곡관보호공","체적0.1㎥이하",16,"nr"]
["    나) 곡관보호공","체적0.1∼0.2㎥",13,"nr"]
["    다) 곡관보호공","체적0.2∼0.5㎥",39,"nr"]
["  13) 수압시험비","",0,""]
["    가.수압시험비","80m/m",4,"회"]
["    나.수압시험비","100m/m",10,"회"]
["    다.수압시험비","150m/m",3,"회"]
["    라.수압시험비","200m/m",2,"회"]
["    마.수압시험비","250m/m",2,"회"]
["    바.수압시험비","300m/m",6,"회"]
["    사.수압시험비","350m/m",1,"회"]
["  14) 강관퇴수시험","",164,"㎥"]
["  15) 상수관경고테이프","",0,""]
["    가. 흑갈색테이프","흑갈색,10cm",58,"M"]
["    나. 청색테이프","청색,10cm",8586,"M"]
["  16) 가 압 장","",0,""]
["   가. 토    공","",0,""]
["    가) 흙깎기,토  사","백호우 1.0㎥",1023,"㎥"]
["    나) 흙깎기,리핑암","리퍼도쟈 32Ton",114,"㎥"]
["    다) 되메우기 및 다짐","백호우+콤팩터",695,"㎥"]
["    라) 되메우기 및 다짐","백호우+램머",5,"㎥"]
["    마) 절토면고르기,리핑암","",126,"㎡"]
["   나. 구조물공","",0,""]
["    가) 콘크리트타설","",0,""]
["     ㄱ. 콘크리트타설(무근)","인력",1,"㎥"]
["     ㄴ. 콘크리트타설(철근)","슬럼프15cm",147,"㎥"]
["     ㄷ. 콘크리트타설(무근)","슬럼프8∼12cm",13,"㎥"]
["    나) 거 푸 집","",0,""]
["     ㄱ. 거푸집,매끈한마감","합판3회,0-7M(수직)",156,"m2"]
["     ㄴ. 거푸집,매끈한마감","합판3회,0-7M(경사)",32,"m2"]
["     ㄷ. 거푸집,매끈한마감","합판3회,0-7M(수평)",16,"m2"]
["     ㄹ. 거푸집,보통마감","합판4회(수직)",201,"m2"]
["     ㅁ. 거푸집,거친마감","합판6회(수직)",44,"m2"]
["    다) 철근및보강,이형철근","연강,직경22∼29mm,복잡",29.289,"Ton"]
["    라) 스페이셔설치","",0,""]
["     ㄱ.스페이서","슬래브및기초용",181,"m2"]
["     ㄴ.스페이서","벽체용",357,"m2"]
["    마) 강관비계","3개월",182,"㎡"]
["    바) 동 바 리","",0,""]
["     ㄱ. 동바리,강재","암거구조물,3개월",263,"공m3"]
["     ㄴ. 강관동바리(3개월)","수평연결재",116,"m2"]
["    사) 시공이음","수팽창성지수판",72,"m"]
["    아) 방   수","",0,""]
["     ㄱ. 폴리우레탄쉬트방수","수직면",201,"㎡"]
["     ㄴ. 에폭시방수","",270,"㎡"]
["    자) 수팽창고무지수재","5x20",4,"M"]
["    차) 난    간","",17,"M"]
["   다. 관    로","",0,""]
["    가) 폴리에틸렌피복강관","ø300mm,토사기초",15,"M"]
["    나) 내충격수도관","ø65mm",38,"M"]
["   라. 부 대 공","",0,""]
["    가) 아스콘포장","",0,""]
["     ㄱ. 표층,#78","5cm",76,"㎡"]
["     ㄴ. 기층,#467","10cm",76,"㎡"]
["     ㄷ. 택코팅","RS(C)-4",76,"㎡"]
["     ㄹ. 프라임코팅","RS(C)-3",76,"㎡"]
["    나) 보조기층","T=20cm",19,"㎥"]
["    다) 동상방지층","T=40cm",34,"㎥"]
["    라) 휀스 및 출입문","",0,""]
["     ㄱ. 터파기,토  사","인  력",24,"㎥"]
["     ㄴ. 되메우기","인  력",21,"㎥"]
["     ㄷ. 잔토처리","인  력",3,"㎥"]
["     ㄹ. 콘크리트타설","레미콘",3,"m3"]
["     ㅁ. 거푸집,거친마감","합판6회(수직)",34,"㎡"]
["     ㅂ. 경계용휀스","H1.8xW2.0",45,"M"]
["     ㅅ. 정   문","H1.8xW4.0",1,"nr"]
["    마) 이형관보호공","",0,""]
["     ㄱ. 곡관보호공","D300 45˚곡관",2,"nr"]
["     ㄴ. 곡관보호공","D300 45˚x2곡관",1,"nr"]
[" 5. 포 장 공","",0,""]
["  1) 아스콘 포장","",0,""]
["   가. 아스콘포장,표층,#78","5cm",36368,"㎡"]
["   나. 아스콘포장,중간층,#67","6cm",8816,"㎡"]
["   다. 아스콘포장,기층,#467","10cm",36368,"㎡"]
["  2) 아스팔트살포","",0,""]
["   가. 택코팅","RS(C)-4",36368,"㎡"]
["   나. 프라임코팅","RS(C)-3",36368,"㎡"]
["  3) 보조기층","T=20cm",9231,"㎥"]
["  4) 동상방지층","T=44~45cm",16842,"㎥"]
["  5) 보도블록포장","",0,""]
["   가. 소형고압블록","T=6cm,회색",4158,"㎡"]
["   나. 소형고압블록","T=6cm,적색",3119,"㎡"]
["   다. 소형고압블록","T=6cm,녹색",3119,"㎡"]
["  6) 자전거도로포장(투수성)","",0,""]
["   가. 투수성평판블럭(회색)","T=6CM",430,"㎡"]
["   나. 투수성평판블럭(녹색)","T=6CM",430,"㎡"]
["  7) 투수콘크리트포장","T=7cm,적갈색",924,"㎡"]
["  8) 장애자용블록","",0,""]
["    가) 맹인용점자블록","",240,"㎡"]
["    나) 보도,자전거(쇄석)","7~10cm",1207,"㎡"]
["  9) 보차도경계석(화강석)","",0,""]
["   가. 경계석설치(직선)","대로(200ⅹ300)",791,"m"]
["   나. 경계석설치(곡선)","대로(200ⅹ300)",58,"m"]
["   다. 경계석설치(경사)","대로(200ⅹ300)",32,"m"]
["   라. 경계석설치(낮춤,직선)","대로(200ⅹ300)",53,"m"]
["   마. 경계석설치(낮춤,곡선)","대로(200ⅹ300)",121,"m"]
["   바. 경계석설치(직선)","중로(200ⅹ250)",4180,"m"]
["   사. 경계석설치(곡선)","중로(200ⅹ250)",203,"m"]
["   아. 경계석설치(경사)","중로(200ⅹ250)",52,"m"]
["   자. 경계석설치(낮춤,직선)","중로(200ⅹ250)",80,"m"]
["   차. 경계석설치(낮춤,곡선)","중로(200ⅹ250)",188,"m"]
["   카. 경계석설치(직선)","소로(180ⅹ200)",164,"m"]
["  10) 도로경계석(화강석)","",0,""]
["   가. 경계석,직선부","150×150×1000mm",2230,"m"]
["   나. 경계석,대지경계블록","150×120×1000mm",4697,"m"]
["  11) 차선도색","",0,""]
["   가.차선도색","가열형(백색)",1042,"㎡"]
["   나.차선도색","가열형(황색)",625,"㎡"]
["   다. 차선도색,문자 및 형상","융착식(수동식),백색",950,"㎡"]
["   라. 차선도색,문자 및 형상","융착식(수동식),황색",34,"㎡"]
["  12) 안전시설","",0,""]
["   가. 화강석,볼라드","H=700,R=400",136,"개"]
["   나. 미끄럼방지","",456,"㎡"]
["  13) 가로수분","",276,"nr"]
["  14) 표 지 판","",0,""]
["   가. 표지판","단주식,삼각1변900",7,"nr"]
["   나. 표지판","단주식,삼각2변900",10,"nr"]
[" 6. 구조물공","",0,""]
["  1) 반중력식옹벽","",0,""]
["   가. 콘크리트 타설","",0,""]
["    가) 콘크리트타설(철근)","100㎥이상/일,슬럼프15cm",95,"㎥"]
["    나) 콘크리트타설(무근)","레미콘 일반타설",9,"㎥"]
["   나. 거 푸 집","",0,""]
["    가) 거푸집,매끈한마감","합판3회(수직)",227,"m2"]
["    나) 거푸집,보통마감","합판4회(수직)",59,"㎡"]
["    다) 거푸집,거친마감","합판6회(수직)",14,"㎡"]
["   다.이형철근(연강)","보통",2.862,"Ton"]
["   라. 옹벽신축이음","",0,""]
["    가) 스치로폴설치","T=20MM",4,"㎡"]
["    나) DOWEL BAR","φ32mm",18,"EA"]
["    다) 수축줄눈"," ",15,"M"]
["   마. 스페이셔","",0,""]
["    가) 스페이셔 설치","슬래브용",112,"㎡"]
["    나) 스페이셔 설치","벽체용",224,"㎡"]
["   바. 매입부속물,선형매입","PVC 100mm",7,"M"]
["   사. 시공이음","",0,""]
["    가) 수팽창고무지수재","시공이음",70,"M"]
["    나) 수축줄눈"," ",16,"M"]
["  2) 보강토옹벽","",0,""]
["   가.터파기,토  사","백호우1.0㎥",263,"㎥"]
["   나. 되메우기 및 다짐","백호우+콤팩터",129,"㎥"]
["   다. 잔토처리,인  력","",133,"㎥"]
["   라. 성토부설 및 다짐","(보강토옹벽)",1893,"㎥"]
["   마. 기초잡석부설","(보강토옹벽)",96,"㎥"]
["   바. 속채움잡석부설","(보강토옹벽)",207,"㎥"]
["   사. 보강토 블록설치","마감형",14,"㎡"]
["   아. 보강토 블록설치","일반형",456,"㎡"]
["   자. 보강재 설치","65R",2541,"㎡"]
["   차. 보강재 설치","90R",94,"㎡"]
[" 7. 저류지공","",0,""]
["  1) 토   공","",0,""]
["   가. 터파기,토  사","백호우1.0㎥",1896,"㎥"]
["   나. 되메우기및다짐","백호우+램머",744,"㎥"]
["  2) 콘크리트 타설","",0,""]
["   가. 콘크리트타설(철근)","레미콘 일반타설",286,"㎥"]
["   나. 콘크리트타설(무근)","레미콘 일반타설",36,"㎥"]
["  3) 거푸집","",0,""]
["   가. 거푸집,보통마감","합판4회(수직)",1398,"㎡"]
["   나. 거푸집,거친마감","합판6회(수직)",409,"㎡"]
["  4) 이형철근(연강)","공칭직경13mm,보통",10.264,"Ton"]
["  5) 잡석부설","",36,"㎥"]
["  6) 피복파형강관 접합,부설","ø1350mm,토사기초",57,"M"]
["  7) 수문(저류지용)","ø1350mm용",1,"nr"]
["  8) 생태블럭","1240x1074x250",2009,"EA"]
["  9) 관로경고용테이프","녹색,10cm",86,"M"]
["  10) 부직포 부설","",2009,"㎡"]
["  11) 식    재","",2009,"㎡"]
[" 8. 배수지","",0,""]
["  1) 토   공","",0,""]
["   가. 절    취","",0,""]
["    가) 흙깎기,토  사","백호우 1.0㎥",3274,"㎥"]
["    나) 흙깎기,리핑암","리퍼도쟈 32Ton",904,"㎥"]
["    다) 흙깍기,일반발파","121-200 m",120,"㎥"]
["   나. 터 파 기","",0,""]
["    가) 터파기,토  사","백호우1.0㎥",536,"㎥"]
["    다) 터파기,리핑암","육상리핑",252,"㎥"]
["    라) 터파기,발파암","육상발파",144,"㎥"]
["   다. 성    토","노  체",981,"㎥"]
["   라. 되메우기","",0,""]
["    가) 되메우기 및 다짐","백호우+콤팩터",874,"㎥"]
["    나) 되메우기 및 다짐","백호우+램머",21,"㎥"]
["   마. 절토면고르기","보통암",630,"㎡"]
["  2) 구조물공","",0,""]
["   가. 배 수 지","",0,""]
["    가) 콘크리트타설","",0,""]
["     ㄱ. 콘크리트타설(철근)","슬럼프15cm",786,"㎥"]
["     ㄴ. 콘크리트타설(무근)","슬럼프8∼12cm",650,"㎥"]
["    나) 거 푸 집","",0,""]
["     ㄱ. 거푸집,매끈한마감","합판3회(수직)",75,"m2"]
["     ㄴ. 거푸집,매끈한마감","합판3회,0-7M(경사)",177,"m2"]
["     ㄷ. 거푸집,매끈한마감","합판3회,0-7M(수평)",397,"m2"]
["     ㄹ. 거푸집,보통마감","합판4회(수직)",716,"㎡"]
["     ㅁ. 거푸집,거친마감","합판6회(수직)",35,"㎡"]
["    다) 이형철근(연강)","직경13mm,복잡",102.873,"Ton"]
["    라) 강관비계","3개월",302,"㎡"]
["    마) 동 바 리","",0,""]
["     ㄱ. 동바리,강재","암거구조물,3개월",1442,"공㎥"]
["     ㄴ. 강관동바리(3개월)","수평연결재",448,"m2"]
["    바) 이    음","",0,""]
["     ㄱ. 조인트","",258,"M"]
["     ㄴ. 지수철판","",4.71,"Ton"]
["    사) 스페이서설치","",0,""]
["     ㄱ. 스페이셔 설치","벽체용",802,"㎡"]
["     ㄴ. 스페이셔 설치","슬래브용",927,"㎡"]
["    아) 방    수","",0,""]
["     ㄱ. 폴리우레탄쉬트방수","수직면",716,"㎡"]
["     ㄴ. 폴리우레탄쉬트방수","수평면",490,"㎡"]
["     ㄷ. 에폭시방수","",1078,"㎡"]
["    자) 난    간","",21,"M"]
["    차) 도 류 벽","(PDF판넬.T=65MM)",291,"M2"]
["    카) 수팽창고무지수재","",18,"M"]
["  3) 관    로","",0,""]
["   가. 폴리에틸렌피복강관","ø250mm,토사기초",40,"M"]
["   나. 폴리에틸렌피복강관","ø250mm,모래기초",54,"M"]
["   다. 폴리에틸렌피복강관","ø300mm,모래기초",14,"M"]
["   라. 폴리에틸렌피복강관","ø350mm,모래기초",15,"M"]
["  4)  플랜지접합","",0,""]
["   가. 플랜지 접합","250m/m",11,"개소"]
["   나. 플랜지 접합","300m/m",6,"개소"]
["   다. 플랜지 접합","350m/m",6,"개소"]
["  5) 에폭시피복강관절단","",0,""]
["   가.에폭시피복강관절단","250m/m",9,"개소"]
["   나.에폭시피복강관절단","300m/m",1,"개소"]
["   다.에폭시피복강관절단","350m/m",3,"개소"]
["  6) 에폭시피복강관이형관","",0,""]
["     1] 나팔관","D250",11,"EA"]
["     2] 나팔관","D300",2,"EA"]
["     3] 나팔관","D350",2,"EA"]
["     4] 에폭시피복단관","D250X2.27M",1,"EA"]
["     5] 에폭시피복단관","D250X3.06M",2,"EA"]
["     6] 에폭시피복단관","D250X1.81M",2,"EA"]
["     7] 에폭시피복단관","D250X0.35M",2,"EA"]
["     8] 에폭시피복단관","D250X0.44M",1,"EA"]
["     9] 에폭시피복단관","D250X1.33M",1,"EA"]
["    10] 에폭시피복단관","D250X1.2M",1,"EA"]
["    11] 에폭시피복단관","D350X0.86M",1,"EA"]
["    12] 에폭시피복단관","D350X1.1M",2,"EA"]
["    13] 에폭시피복단관","D350X3.96M",1,"EA"]
["    14] 에폭시피복단관","D350X1.2M",1,"EA"]
["    15] 에폭시피복단관","D350X0.95M",1,"EA"]
["    16] 에폭시피복단관","D300X1.97M",1,"EA"]
["    17] 에폭시피복단관","D300X2.60M",4,"EA"]
["    18] 에폭시피복단관","D300X3.27M",1,"EA"]
["    19] 에폭시피복단관","D300X4.3M",1,"EA"]
["    20] 에폭시피복단관","D300X4.05M",1,"EA"]
["    21] 에폭시링엘보","D350X45",2,"EA"]
["    22] 에폭시링엘보","D350X90",1,"EA"]
["    23] 에폭시링엘보","D350X11.25",2,"EA"]
["    24] 에폭시링엘보","D250X90",5,"EA"]
["    25] 에폭시링엘보","D300X45",2,"EA"]
["    26] 에폭시링엘보","D300X90",2,"EA"]
["    27] 에폭시링엘보","D250X22.5",8,"EA"]
["    28] 에폭시홈티이","D350X350",1,"EA"]
["    29] 에폭시홈티이","D250X250",3,"EA"]
["    30] 에폭시홈티이","D300X300",1,"EA"]
["    31] 링플랜지아답터","D350",6,"EA"]
["    32] 링플랜지아답터","D250",10,"EA"]
["    33] 링플랜지아답터","D300",6,"EA"]
["  7) 밸    브","",0,""]
["   가. 소프트실제수밸브:수동식","",0,""]
["    가) 소프트실제수밸브","250m/m,10k",4,"nr"]
["    나) 소프트실제수밸브","300m/m,10k",2,"nr"]
["    다) 소프트실제수밸브","350m/m,10k",2,"nr"]
["  8) 상수관경고테이프","",0,""]
["    가. 흑갈색테이프","흑갈색,10cm",142,"M"]
["    나. 청색테이프","청색,10cm",44,"M"]
["  9) 부 대 공","",0,""]
["   가. 아스콘포장","",0,""]
["    가) 표층,#78","5cm",318,"㎡"]
["    나) 기층,#467","10cm",318,"㎡"]
["    다) 택코팅","RS(C)-4",318,"㎡"]
["    라) 프라임코팅","RS(C)-3",318,"㎡"]
["   나. 보조기층부설다짐","",0,""]
["    가) 보조기층,혼합골재","T=20cm",79,"㎥"]
["    나) 동상방지층,리핑암유용","T=44~45cm",143,"㎥"]
["    다) 자연표토복원공법","절토부",716,"㎡"]
["   다. 휀스 및 출입문","",0,""]
["    가) 토    공","",0,""]
["     ㄱ. 터파기,토  사","인  력",68,"㎥"]
["     ㄴ. 되메우기","인  력",60,"㎥"]
["     ㄷ. 잔토처리","인  력",8,"㎥"]
["    나) 휀스 및 출입문","",0,""]
["     ㄱ. 콘크리트타설","레미콘타설",8,"m3"]
["     ㄴ. 거푸집,거친마감,수직면","합판6회",97,"㎡"]
["     ㄷ. 경계용휀스","H1.8xW2.0",135,"M"]
["     ㄹ. 정    문","H1.8xW4.0",1,"nr"]
["   라. U형측구(현장타설)","토사구간,400x400",128,"M"]
["   마. 집수정(배수지)","800x800x1000",2,"nr"]
["   바. 곡관보호공","D350X11.25˚곡관",1,"nr"]
[" 9. 부 대 공","",0,""]
["  1) 가드레일","",172,"M"]
["  2) 엔드레일","경간",8,"EA"]
["  3) 낙석방지책","경간",79,"nr"]
["  4) 가설사무소","",0,""]
["   가. 발주자용 가설건물","150㎡, 24개월",1,"sum"]
["   나. 도급자용 가설건물","200㎡, 24개월",1,"sum"]
["   다. 도급자용 창고","100㎡, 24개월",1,"sum"]
["   라. 시험실"," 50㎡, 24개월",1,"sum"]
["   마. 복리후생시설","120㎡, 24개월",1,"sum"]
["  5) 안내판 및 조감도,상황판","",1,"sum"]
["  6) 현장관리비","",0,""]
["   가. 세륜 세차 시설","자동세륜기",1,"nr"]
["   나. 방음방진막","H=4m(방음2.5m,방진1.5m)",457,"경간"]
["   다. 폐기물처리비","폐유저장소",1,"식"]
["   라. 대기오염방지","공사현장살수",1,"sum"]
["   마. 침사지","각종,3개소",1,"sum"]
["  7) 하천우회시설","B1.5*H0.7",485,"M"]
["  8) 현장관리비","",0,""]
["   가. 품질시험비","",1,"식"]
["   다. 시공상세도작성","",1,"식"]
["   다. 기타 품질관리비","",1,"식"]
["  9) 장비운반","",1,"식"]
["  10) 자재운반비","",0,""]
["   가.시멘트운반","12 Ton",701,"대"]
["   나.철근운반","12 Ton",570.786,"Ton"]
["   다.모래운반","덤프 15Ton",803,"㎥"]
["   라.아스팔트 운반","RS(C)-3,4",204,"DM"]
["   마.투수콘크리트","7cm,적갈색",942,"㎡"]
["   바.폴리에틸렌피복강관운반","",0,""]
["    가)에폭시피복강관 운반","D 80m/m",760,"M"]
["    나)에폭시피복강관 운반","D 100m/m",2116,"M"]
["    다)에폭시피복강관 운반","D 150m/m",541,"M"]
["    라)에폭시피복강관 운반","D 200m/m",388,"M"]
["    마)에폭시피복강관 운반","D 250m/m",536,"M"]
["    바)에폭시피복강관 운반","D 300m/m",1174,"M"]
["    사)에폭시피복강관 운반","D 350m/m",261,"M"]
["   사.내충격수도관운반","",0,""]
["    가)수도용 경질염화비닐관 운반","D 40m/m",231,"M"]
["    나)수도용 경질염화비닐관 운반","D 65m/m",39,"M"]
["    다)수도용 경질염화비닐관 운반","D 75m/m",6,"M"]
["  11) 고재대","중량A",18.609,"Ton"]
[" 10. 건    축","",0,""]
["   1) 가설공사","",0,""]
["    가. 규준틀설치","귀",4,"개소"]
["    나. 규준틀설치","평",2,"개소"]
["    다. 이동식강관말비계","3개월 H=4M",1,"대"]
["    라. 강관동바리","3개월,5.0M이하",86,"㎡"]
["    마. 강관쌍줄비계","30M 이하.6개월",255,"㎡"]
["    바. 먹메김","학교,공장",82,"㎡"]
["    사. 콘크리트보양","보온덮게",82,"㎡"]
["    아. 현장정리","RC조",82,"㎡"]
["   2) 철근콘크리트공사","",0,""]
["    가. PE필림깔기","바닥",82,"㎡"]
["    나. 펌프카붐타설(철근)","50~100M3미만",65,"㎥"]
["    다. 펌프카붐타설(무근)","50~100M3미만",9,"㎥"]
["    라. 거푸집,매끈한마감","합판3회(수직)",246,"m2"]
["    마. 거푸집,보통마감","합판4회(수직)",7,"㎡"]
["    바. 유로폼벽","",291,"㎡"]
["    사. 철근및보강재(연강)","직경13mm,보통",8.064,"Ton"]
["   3) 조적공사","",0,""]
["    가. 시멘트벽돌쌓기","0.5B",1,"천매"]
["    나. 토석벽돌치장쌓기","0.5B,한면",3,"천매"]
["    다. 벽돌소운반","1층",3,"천매"]
["    라. 벽돌소운반","2층",1,"천매"]
["    마. 스치로폴설치","벽공간70/0.03",42,"㎡"]
["   4) 방수공사","",0,""]
["    가. 쉬트방수A","바닥,3MM",82,"㎡"]
["    나. 쉬트방수A","벽,3MM",16,"㎡"]
["    다. 치장줄눈","SAW CUT ",95,"M"]
["   5) 미장공사","",0,""]
["    가. 시멘트몰탈","바닥",73,"㎡"]
["    나. 시멘트몰탈","내벽",80,"㎡"]
["    다. 시멘트몰탈","외벽",30,"㎡"]
["    라. 쇠흙손마감","",165,"㎡"]
["    마. 콘크리트면처리","외벽",12,"㎡"]
["    바. 콘크리트면처리","내벽",141,"㎡"]
["    사. 콘크리트면처리","",82,"㎡"]
["   6) 창호공사","",0,""]
["    가. 도아체크","K-1630 일반용",2,"EA"]
["    나. 도아로크","9000 PB 현관용",2,"EA"]
["    다. 샷타개폐기","400KG",1,"EA"]
["    라. 스틸고정창","100*50*1.0",1,"㎡"]
["    마. 스틸힌지도아","1.2T 정진분체도장",3,"㎡"]
["    바. 알미늄샷타(이중샷다)","T=1.2MM:내풍압",8,"㎡"]
["    사. 알미늄창틀(미서기고정창)","100MM 볼소수지코팅",25,"㎡"]
["    아. 알미늄창틀(고정창)","100MM 볼소수지코팅",5,"㎡"]
["    자. 알미늄창틀(안젖힘창)","100MM 볼소수지코팅",1,"㎡"]
["    차. 알미늄방충망","볼소코팅",4,"㎡"]
["    카. 후로아힌지달기","",2,"EA"]
["    타. 도아체크달기","",2,"EA"]
["    파. 도아록달기","",2,"EA"]
["    하. 코킹/창호주위","10*10",75,"M"]
["    가. 창틀주위충진몰탈","",77,"M"]
["   7) 유리공사","",0,""]
["    가. 복층유리","칼라16MM(5CO+A6+5CL)",32,"㎡"]
["    나. 유리끼우고딱기 ","복층유리",32,"㎡"]
["    다. 유리코킹","유리용 SL-801",198,"M"]
["   8) 도장공사","",0,""]
["    가. 에폭시바닥제","T=3MM",42,"㎡"]
["    나. 수성페인트","내벽3회",221,"㎡"]
["    다. 수성페인트","천정3회",82,"㎡"]
["    라. 수성페인트","외벽3회",43,"㎡"]
["    마. 세라민페인트","2회",5,"㎡"]
["   9) 수장공사","",0,""]
["    가. 외벽단열마감","스치로폴T50+메쉬+마감재",153,"㎡"]
["    나. 와이아메쉬깔기","#8-150*150",82,"㎡"]
["    다. 메탈라스설치 벽#800","#800",4,"㎡"]
["    라. 재료분리대설치(바닥)","2.0MM,HL",1,"㎏"]
["    마. 디럭스타일붙이기","3*300*3T",33,"㎡"]
["    바. 스치로폴바닥깔기","50MM",82,"㎡"]
["   10) 잡 공 사","",0,""]
["    가. 빗물받이블럭","",2,"EA"]
["    나. 루프드레인설치 주철","ø100",2,"EA"]
["    다. SST선홈통","ø100",10,"M"]
["    라. 스텐레스사다리","",6,"M"]
[" 11. 기    계","",0,""]
["   1) 기자재비","",0,""]
["    가. M-101 흡입밸브","소프트실제수밸브(200A)",4,"개"]
["    나. M-102 가압펌프","편흡입단단1.96M3/minX37m",3,"대"]
["    다. M-103 역지변","주철제스윙체크밸브(150A)",3,"개"]
["    라. M-104 토출밸브","진동버터플라이밸브(150A)",3,"개"]
["    마. M-105 유지관리밸브","소프트실제수밸브(150A)",3,"개"]
["    바. M-106 SUREGE RELIEF 밸브","WIDE Y-PATTERN (150A)",1,"개"]
["    사. M-107 바닥배수펌프","수중펌프,0.1M3 X 10mH",1,"대"]
["    아. M-108 기기반출","진동모노레일1tonX8mHX9mL",1,"대"]
["   2) 기자재설치비","",0,""]
["    가. 흡입밸브","200A",4,"개"]
["    나. 가압펌프","",3,"대"]
["    다. 역 지 변","150A",3,"개"]
["    라. 토출밸브","150A",3,"개"]
["    마. 유지관리밸브","150A",3,"개"]
["    바. SUREGE RELIEF 밸브","150A",1,"개"]
["    사. 바닥배수펌프","",1,"대"]
["    아. 모노레일설치","",1,"대"]
["   3) 배관자재비","",0,""]
["       1] STS강관","25Ax3.0T",1,"M"]
["       2] STS강관","65Ax3.0T",4,"M"]
["       3] STS강관","150Ax3.4T",5,"M"]
["       4] STS강관","200Ax4.0T",3,"M"]
["       5] STS강관","300Ax4.5T",9,"M"]
["       6] SPS강관","200A",6,"M"]
["       7] 90엘보(STS)","65A",1,"EA"]
["       8] 90엘보(STS)","150A",2,"EA"]
["       9] R．TEE(STS)","300x200A",4,"EA"]
["       10] R．TEE(STS)","300x150A",4,"EA"]
["       11] RED．(STS)","65x40A",1,"EA"]
["       12] RED．(STS)","150x125A",3,"EA"]
["       13] RED．(STS)","200x150A",3,"EA"]
["       14] 플랜지 (STS)","40A",1,"EA"]
["       15] 플랜지 (STS)","65A",3,"EA"]
["       16] 플랜지 (STS)","125A",3,"EA"]
["       17] 플랜지 (STS)","150A",27,"EA"]
["       18] 플랜지 (STS)","200A",7,"EA"]
["       19] 플랜지 (STS)","300A",4,"EA"]
["       20] 맹플랜지 (STS)","200A",1,"EA"]
["       21] 맹플랜지 (STS)","300A",2,"EA"]
["       22] 게이트밸브(주철제)","65A",1,"EA"]
["       23] 게이트밸브(주철제)","150A",2,"EA"]
["       24] CHECK V/V","65A",1,"EA"]
["       25] 볼밸브","25A",1,"EA"]
["       26] AIRVENT","25A",1,"EA"]
["       27] 플렉시블조인트","65A",1,"EA"]
["       28] 플렉시블조인트","150A",3,"EA"]
["       29] 플렉시블조인트","200A",3,"EA"]
["       30] ㄱ- 형강","50x50x6T",0.007,"Ton"]
["       31] ㄷ- 형강 (CHANNEL)","(SS400)50x50x6T",0.031,"Ton"]
["       32] ㄷ- 형강 (CHANNEL)","(SS400)150x75x6.5T",0.021,"Ton"]
["       33] 강판 (SS400)","9T",0.009,"Ton"]
["       34] 앙카볼트","M12x200L",32,"조"]
["       35] U볼트,너트,와셔","(65A)M12x75L",4,"조"]
["       36] U볼트,너트,와셔","(150A)M16x130L",3,"조"]
["       37] U볼트,너트,와셔","(200A)M20x65L",5,"조"]
["       38] U볼트,너트,와셔","(300A)M24x240L",7,"조"]
["   4) 배관설치비","",0,""]
["       1] STS 배관 설치공사","25A",1,"M"]
["       2] STS 배관 설치공사","65A",0.02,"Ton"]
["       3] STS 배관 설치공사","150A",0.072,"Ton"]
["       4] STS 배관 설치공사","200A",0.059,"Ton"]
["       5] STS 배관 설치공사","300A",0.316,"Ton"]
["       6] STS 플랜지접합","40A",1,"개소"]
["       7] STS 플랜지접합","65A",4,"개소"]
["       8] STS 플랜지접합","125A",3,"개소"]
["       9] STS 플랜지접합","200A",30,"개소"]
["       10] STS 플랜지접합","300A",11,"개소"]
["       11] STS 밸브설치","φ15~50",4,"개소"]
["       12] 밸브설치(플랜지식)","65A",3,"개"]
["       13] 밸브설치(플랜지식)","150A",5,"개"]
["       14] 밸브설치(플랜지식)","200A",3,"개"]
["       15] STS 관접합","25A",2,"개소"]
["       16] STS 관접합","200A",6,"개소"]
["       17] STS 관접합","150A",30,"개소"]
["       18] STS 관접합","200A",14,"개소"]
["       19] STS 관접합","300A",18,"개소"]
["       20] 잡철물제작설치","간단(스텐)",0.06,"Ton"]
["       21] 녹막이페인트칠","2회",2,"㎡"]
["       22] 조합페인트칠","2회",2,"㎡"]
[" 12.주요자재비","",0,""]
["  1)골재","",0,""]
["   가. 쇄석자갈","25㎜이하",217,"㎥"]
["   나. 쇄석자갈","40mm이하",11138,"㎥"]
["   다. 혼합골재","80mm이하",17702,"㎥"]
["   라. 쇄석자갈","150mm이하",54,"㎥"]
["   마. 모래","하천모래",803,"㎥"]
["  2)시멘트","40kg/포",701,"포"]
["  3)레미콘","",0,""]
["   가.레미콘","25-160-08",338,"㎥"]
["   나.레미콘","25-180-08",37,"㎥"]
["   다.레미콘","25-180-15",8,"㎥"]
["   라.레미콘","25-210- 8",569,"㎥"]
["   마.레미콘","25-240-08",24,"㎥"]
["   바.레미콘","25-240-15",4427,"㎥"]
["   사.레미콘","40-160-08",235,"㎥"]
["   아.레미콘","40-180-08",1484,"㎥"]
["   자.레미콘","40-210-08",771,"㎥"]
["  4)철근","",0,""]
["   가.이형철근(SD30A)","D10m/m",3.219,"Ton"]
["   나.이형철근(SD30A)","D13m/m",341.011,"Ton"]
["   다.이형철근(SD30A)","D22m/m",52.469,"Ton"]
["   라.이형철근(SD30A)","D16-D32m/m",172.944,"Ton"]
["  5)포장아스팔트","",0,""]
["   가.아스콘"," #67",1186,"Ton"]
["   나.아스콘"," #78",4029,"Ton"]
["   다.아스콘","#467",8007,"Ton"]
["   라.유화아스팔트","RSC-3,4, 200ℓ",204,"D/M"]
["  6)도로용경계석(화강암)","",0,""]
["   가.경계석(화강암)직선","200ⅹ300ⅹ1000",814,"개"]
["   나.경계석(화강암)곡선","200ⅹ300ⅹ1000",59,"개"]
["   다.경계석(화강암)경사","200ⅹ300-70ⅹ1000",32,"개"]
["   라.경계석(화강암)낮춤","200ⅹ300ⅹ1000",54,"개"]
["   마.경계석(화강암)낮춤","200ⅹ300ⅹ1000",124,"개"]
["   바.경계석(화강암)직선","200ⅹ250ⅹ1000",4305,"개"]
["   사.경계석(화강암)곡선","200ⅹ250ⅹ1000",209,"개"]
["   아.경계석(화강암)경사","200ⅹ250ⅹ1000",53,"개"]
["   자.경계석(화강암)낮춤","200ⅹ250ⅹ1000",82,"개"]
["   차.경계석(화강암)낮춤","200ⅹ250ⅹ1000",193,"개"]
["   카.경계석(화강암)직선","180ⅹ200ⅹ1000",168,"개"]
["   타.보차도경계블록","150x150x200x1000mm",2296,"개"]
["   파.도로경계블록","150x120x1000mm",4837,"개"]
["  7)투수콘크리트","10∼180㎏/㎠",942,"㎡"]
["  8)가로수분받침틀","말굽형,1200x950x15T",276,"nr"]
["  9)피복파형강관","",0,""]
["   가.피폭파형강관","D250m/m",1346,"M"]
["   나.피폭파형강관","D450m/m",764,"M"]
["   다.피폭파형강관","D500m/m",393,"M"]
["   라.피폭파형강관","D600m/m",227,"M"]
["   마.피폭파형강관","D700m/m",576,"M"]
["   바.피폭파형강관","D800m/m",172,"M"]
["   사.피폭파형강관","D900m/m",217,"M"]
["   아.피폭파형강관","D1,000m/m",515,"M"]
["   자.피폭파형강관","D1,100m/m",407,"M"]
["   차.피폭파형강관","D1,200m/m",103,"M"]
["   카.피폭파형강관","D1,350m/m",58,"M"]
["  10)유리섬유복합관","",0,""]
["    가.유리섬유복합관","D400m/m",3243,"M"]
["    나.유리섬유복합관","D150m/m",221,"M"]
["    다.유리섬유이음관","D400m/m",621,"EA"]
["    라. 유리섬유이음관","D150m/m",66,"EA"]
["  11)에폭시피복강관","",0,""]
["   가.에폭시피복강관"," D80mm, 6m",760,"M"]
["   나.에폭시피복강관"," D100mm, 6m",2116,"M"]
["   다.에폭시피복강관"," D150mm, 6m",541,"M"]
["   라.에폭시피복강관"," D200mm, 6m",388,"M"]
["   마.에폭시피복강관"," D250mm, 6m",536,"M"]
["   바.에폭시피복강관"," D300mm, 6m",1174,"M"]
["   사.에폭시피복강관"," D350mm, 6m",261,"M"]
[" 12)내충격수도관","",0,""]
["   가. 내충격수도관","40m/m(4m/본)",231,"M"]
["   나. 내충격수도관","65m/m(6m/본)",39,"M"]
["   다. 내충격수도관","D75㎜(6m/본)",6,"M"]
[" 13)수도용밸브","",0,""]
["   가.제수밸브(공기변부착)","80m/m",10,"nr"]
["   나.제수밸브(공기변부착)","100m/m",19,"nr"]
["   다.제수밸브(공기변부착)","150m/m",2,"nr"]
["   라.제수밸브(수동수직)","10K, D250m/m, GCD450",6,"nr"]
["   마.제수밸브(수동수직)","10K, D300m/m, GCD450",2,"nr"]
["   바.제수밸브(수동수직)","10K, D350m/m, GCD450",2,"nr"]
[" 14)맨홀뚜껑","",0,""]
["   가.맨홀뚜껑 ","φ648,상하수,회주철",72,"조"]
["   나.칼라보도맨홀뚜껑","120kg,φ648,800x800x60",82,"조"]
[" 15)측구용배수관","",0,""]
["   가.벤치플륨관(소켓식)","1200*1000",270,"M"]
["   나.측구수로관","400*400*2000",473,"M"]

{"sheet":"공사원가(공)","index":1,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[[28,0,28,2],[25,0,25,2],[26,0,26,2],[21,0,21,2],[22,0,22,2],[23,0,23,2],[24,0,24,2],[2,0,2,2],[18,0,18,2],[19,0,19,2],[20,0,20,2],[3,1,4,1],[5,1,7,1],[8,1,17,1],[3,0,17,0]],"flags":["formulas_cached_only"]}
[null,null,null,"공 사 원 가 계 산 서"]
[]
["구        분",null,null,"금     액(원)","비        고"]
["순\n\n공\n\n사\n\n비","재\n료\n비","직접재료비"]
[null,null,"1. 소 계"]
[null,"노\n무\n비","직접노무비"]
[null,null,"간접노무비",null,"직접노무비 *     %"]
[null,null,"2. 소 계"]
[null,"경\n\n비","직접경비"]
[null,null,"산재보험료",null,"[직노+간노] *     %"]
[null,null,"산업안전보건관리비",null,"[재료비+직노] *     %"]
[null,null,"건강보험료",null,"직접노무비 *     %"]
[null,null,"연금보험료",null,"직접노무비 *     %"]
[null,null,"기타경비",null,"[재료비+직노+간노] *     %"]
[null,null,"퇴직공제부금비",null,"직접노무비 *     %"]
[null,null,"고용보험료",null,"[직노+간노] *     %"]
[null,null,"건설하도급대금지급          보증서발급수수료",null,"[재료비+직노+산출경비] *      %"]
[null,null,"3. 소 계"]
["계(1)"]
["일반관리비",null,null,null,"계(1) *     %"]
["계(2)",null,null,null,"[계(1)+일반관리비]"]
["이     윤",null,null,null,"[계(2)-재료비] *     %"]
["합    계"]
["현지사무원 급료"]
["공  사  비"]
["부가가치세"]
["총공사비"]